Back

##### APX 8000XE

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Software and Services
- HazLoc Approved Accessories (Div 2)
- Ship Card
- Product Specifications

Back

##### APX 8000XE

### Model

APX™ 8000XE P25 All-Band Portable Radio

700/800 MHz
VHF
UHF R1 & UHF R2

### Updates

NEW 2022: Please note H02 option STUN/KILL does not require encryption. We do "Recommend ordering encryption (other than ADP only selection), otherwise radios will be susceptible to remote STUN/KILL from an adversary"

Effective October 5th, 2020: All U.S. orders will require an encryption selection. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. G193/Q667 ADP only is also available at $0. Please see encryption section for AES and other encryption options that come with ADP. Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.

### Ordering Information

#### Standard Features

All ASTRO Digital APX 8000XE models include the following features:

- All-Band Capability (UHF, VHF, 7/800)

- Adaptive Audio Engine

- GPS Software & Hardware (QA00782)

- Mission Critical Wireless Bluetooth® 4.0 (LE) (QA00583)

- Radio Packet Data (Q947)

- Software Key (QA01749)

- Extreme 1-Sided Noise Reduction (QA01833)

- One Touch/Status Message (H46)

- Radio Trace/Remote Monitor (H43)

- Enhanced Zone Bank (QA01768)

- 3 Programmable Side Buttons
- Orange Programmable Button
- 16 Position Mode Rotary Select Switch
- Angled On/Off Volume Knob
- 1 Top Mounted Programmable 3 Position Toggle Switch

- Top Display: 1 line of text, 1 line of icons, 0 menu lines
- Dual Microphone

- 3 Watt Rated Audio

- Detachable Belt Clip (Model 1.5) / Carry Holder (Models 2.5 & 3.5)

- IMPRES 2 Battery with UL Certification for ISA 12.12.01-2015 and CAN /CSA C22.2 No. 213-15 (PMNN4504)

- MIL-STD Delta-T, IP68 (2 m, 4 hr)

- XE All-Band Antenna (AN000342A01)

- Models 2.5 & 3.5:
  - Unified Call List
  - Front Color Display: 4 Lines of Text, 2 Lines of Icons
  - Radio Profiles
  - 3 Programmable Buttons
  - 4-Way Navigation
  - Home & Data Buttons

- Model 3.5: 4 X 3 Alpha-Numeric Keypad

#### Additional Ordering Information for Service Options

SmartConnect End to End Ordering Guide

ViQi Virtual Partner End to End Ordering Guide

### Configuration

####

#### Models

1A: Main Model (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
APX 8000 ALL BAND PORTABLE MODEL 1.5 | - | H91TGD9PW5 N | 579 | $7,943.00
APX 8000 ALL BAND PORTABLE MODEL 2.5 | - | H91TGD9PW6 N | 579 | $8,226.00
APX 8000 ALL BAND PORTABLE MODEL 3.5 | - | H91TGD9PW7 N | 579 | $8,651.00

1B: XE Housing (Must Select for APX 8000XE)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: APX8000XE RUGGED RADIO | - | QA02006 | 581 | $880.00

#### Operation Mode (Must Select One)

2A: Digital Trunking (SN/SZ P25 Phase I Interop)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SMARTZONE OPERATION | A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | H38 | 655 | $1,766.00
ADD: P25 9600 BAUD TRUNKING | MUST also order H38 & Q806. INCLUDED at 'NO Charge' Q173-OminLink. APX digital radios require Advanced System Keys (ASK- DVN4046A) to be configured to operate on a trunking system. | Q361 | 655 | $353.00
ADD: ASTRO DIGITAL CAI OPERATION | - | Q806 | 579 | $607.00

2B: Digital Trunking (SN/SZ)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SMARTZONE OPERATION | A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | H38 | 655 | $1,766.00

2C: Digital Conventional (P25)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ASTRO DIGITAL CAI OPERATION | - | Q806 | 579 | $607.00
ADD: CONVENTIONAL OPERATION | - | H35 | 655 | $942.00

2D: Analog Trunking

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SMARTZONE OPERATION | A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | H38 | 655 | $1,766.00

2E: Analog Conventional

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: CONVENTIONAL OPERATION | - | H35 | 655 | $942.00
ADD: ANALOG OPERATION | - | Q241 | 579 | $0.00

#### Options

3: Housing (Optional-Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ALT:APX 8000 HOUSING YELLOW | - | H64 | 579 | $30.00
ALT:APX 8000 HOUSING GREEN | - | QA01427 | 579 | $30.00

4: Delete Frequency Bands (Optional. Can select a MAXIMUM of TWO)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
DEL: DELETE UHF BAND | Deletes both UHF R1 and UHF R2 frequency bands | QA05509AA | 0579 | ($800.00)
DEL: DELETE 7/800 MHZ BAND | DEL: DELETE 7/800 MHZ BAND | QA05507AA | 0579 | ($800.00)
DEL: DELETE VHF BAND | DEL: DELETE VHF BAND | QA05508AA | 0579 | ($800.00)

5: RFID Enabled Volume Knob (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: RFID KNOB | Compatible with APX6000, APX7000 & APX8000. Portable radio volume knob with embedded RFID tag making it easier to track assets. When option is ordered, RFID Volume knob will come in the box with the portable radio and other ordered accessories but RFID knob will not be assembled to the radio. AFTERMARKET purchase through Parts department for fielded radios NNTN8646 (APX6000/APX7000/APX8000) and NNTN8647 (APX6000XE/APX7000XE/APX8000XE). See RFID Solution Partner link for information on partners that can provide customers with scanner hardware and back end asset management solutions. | QA04526 | 655 | $30.00

6: System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 Trunking (Q361) | QA01767 | 655 | $118.00
ADD: TDMA OPERATION | Requires Q806, H38, Q361. A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | QA00580 | 655 | $530.00
ADD: PROGRAMMING OVER P25 (OTAP) | Requires Digital and IV&D. Compatible with P25 Trunking and Conventional Operation. POP25 requires AES encryption for ASTRO Conventional operation. To do in field POP25 programming must use Advanced System Key (DVN4046A). | G996 | 655 | $118.00
ADD: MULTICAST VOTING SCAN | Requires Q806 (ASTRO DIGITAL CAI OPERATION) | Q387 | 655 | $235.00
ADD: ENHANCED DATA APX | Digital (Q806/G806), Smartzone (H38/G51), IV&D (Q947) and P25 Trunking (Q361/G361) are required when ordering QA03399 (Enhanced Data) | QA03399 | 656 | $177.00
ADD: DVRS PSU ACTIVATION | Enables DVRS Enhanced PSU functionality on APX Mobile Radios. Requires Digital Operation. QA00631 is to be ordered for radios that are not connected directly to a DVR. If you are connecting your radio directly to a DVR then order GA00631. | QA00631 | 655 | $118.00
ADD: FRONT PANEL PROGRAMMING & CLONING | The APX radio can do FPP on a Trunking equipped radio only on conventional channels. Requires FPP HW dongle (NNTN7526A)to be purchased. | Q53 | 655 | $165.00
ADD: MISSION CRITICAL GEOFENCING | Requires GPS (QA00782). | QA09012 | 426 | $177.00
ADD: GROUP SERVICES | Group Services offers Conventional Alias updates, Trunking Alias updates and Trunking Group Messaging. This option requires G/Q806 for Conventional only capabilities and G/Q361 for any Trunking only capabilities. You can now also do Over the Air Firmware Updates with this feature. (requires digital) | QA09008 | 655 | $177.00
ADD: APX Personnel Accountability | This feature now also allows the user to use a side button of the radio as a method to transmit the acknowledgement of an Evacuation instead of using PTT button. | Q445 | 481 | $177.00
ENH: TACTICAL RADIO STW-STUN/KILL | Tactical Stun Kill is not compatible with DVRs QA00631. Please note H02 option STUN/KILL does not require encryption. We do "Recommend ordering encryption (other than ADP only selection), otherwise radios will be susceptible to remote STUN/KILL from an adversary" | H02 | 481 | $89.00
ADD: WIFI CAPABILITY | Enables Wi-Fi capability in the radio. Supports codeplug updates, firmware refreshes, and FLASHport upgrades over pre-provisioned wireless networks. Requires Radio Management SW (ordered separately). Must order Out of the Box Wi-Fi Provisioning option (QA09007) if provisioning the radios out of the box using Wi-Fi is desired. | QA09001 | 579 | $353.00
ADD: OUT OF THE BOX WIFI PROVISIONING | Requires Wi-Fi (QA09001). Must be added if provisioning the radios out of the box using Wi-Fi is desired. Refer to the 'Out of the Box Wi-Fi Provisioning' section above for details. | QA09007 | 579 | $0.00
ADD: DATA MODEM TETHERING | Requires QA09001 (WiFi) | GA09011 | 681 | $110.00
ADD: SMARTCONNECT | Requires P25 9600 Trunking Q361, WIFI QA09001 and Service offering SSV01S01663A | QA07682AA | 0579 | $0.00

7: Advanced System Key (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: HW KEY SUPPLEMENTAL DATA | The SOFTWARE KEY is the default Advance System Key option that ships standard on all APX products. You cannot order software key QA01749. The HARDWARE KEY QA01648 can be ordered instead. Be sure to enter the CORRECT SYSTEM OWNER ID in the supplemental data. If an INCORRECT ID is entered, a FLASHport order is required to fix the error. Order HARDWARE KEY (QA01648) if required to operate/program on a trunking system. Not compatible with conventional. | QA01648AA | 0655 | $6.42

8: Algorithm Types (Required)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: DVP-XL ENCRYPTION AND ADP | Multikey is required for use of more than one key. Includes ADP. Non-P25 CAP Compliant option. | H797 | 655 | $574.00
CHIFFRAGE DES, DES-XL, DES-OFB | Multikey is required for use of more than one key. Non-P25 CAP Compliant option. Includes ADP | Q625 | 655 | $659.00
CHIFFRAGE AES | Requires digital operation. P25 CAP Compliant option. Includes ADP. | Q629 | 655 | $523.00
ADD: AES/DES-XL/DES-OFB ENCRYPTION AND ADP | Multikey is required for use of more than one key. AES and DES-OFB Operation require digital operation. P25 CAP Compliant option. Includes ADP. | Q15AJ | 0655 | $941.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | Q667BB | 0430 | $0.00
ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below. QA05751 is CAP a COM compliant option. | QA05751AA | 0655 | $0.00

9: Multikey Types (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
MULTICLE OTAR ASTRO P25 | Includes Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. | Q498 | 655 | $814.00
ADD: MULTI SYSTEM OTAR | Requires Q498 ASTRO 25 OTAR W/ MULTIKEY | QA07680AA | 0655 | $177.00

10: Antenna (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
DEL: DELETE STANDARD ANTENNA | Deletes the standard all-band (7/8/V/U) antenna (AN000342A01) | H112LT | 0579 | ($10.00)
ADD: ALT ANTENNA | AN000342A01 Antenna, Whip, V U 7/800 GPS Antenna | QA08425 | 579 | $0.00

#### 11: Battery (Optional)

Division 2 Approved

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ALT: BATT IMPRES 2 LIION DIV2 4850 | This option will delete the standard battery and replace it with UL2054 DIV2 IMPRESS 2 LIION 4850 MAH (PMNN4505). | QA05595 | 579 | $180.00

Not Compatible if Division 2 Certification is Required

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
DEL: DELETE BATTERY | The option will delete the standard battery (UL2054 DIV2 IMPRESS 2 LIION 3400 MAH PMNN4504). | H207EY | 0655 | ($47.00)

12: Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX DATA CABLE | PMKN4012B- Used to program the radio with Customer Programming Software and Tuner Software. PMKN4013C - Used to program and service the radio with Customer Programming Software and Tuner Software. Compatible on ALL APX Portable Radios | Q157 | 655 | $89.00

13: Belt Clips/Carry Holders (Optional-Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
DEL: DELETE BELT CLIP/BASIC CARRY HOLDER | This option deletes the standard belt clip that ships with the Top Display model, deletes the standard univeral carry holder that ships with the Dual Display model. | H301 | 655 | ($10.00)

14: Packaging (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SINGLE UNIT PACKING | - | H842 | 481 | $0.00

15: Service Options (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 3Y ESSENTIAL SERVICE | - | Q58 | 185 | $184.00
ADD: 3Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 3 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00022AC | 185 | $347.00
ADD: 5Y ESSENTIAL SERVICE | Provides 5 years of hardware coverage beginning at time of shipment. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | Q887 | 185 | $306.00
ADD: 5Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 5 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00025AH | 185 | $578.00
ADD: 7Y ESSENTIAL SERVICE HTP | - | HA00690 | 185 | $386.00
ADD: 7Y ESSENTIAL W ACC DMG HTP | - | HA00691 | 185 | $729.00

16: Documentation (Optional)

Online copies of User Guides can be found in the Resources Tab

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799BB | 0579 | $12.00
ADD: USER GUIDE APX 4KXE/6KXE/7KXE CD-ROM | - | H88 | 591 | $30.00

####

### Software and Services

#### General Information

Special Note for United States - State & Local Markets Only
In accordance with FCC mandate, the APX 8000XE all band radio is restricted to12.5 KHz operation only and does NOT support 25 KHz in the VHF and UHF Bands (excluding T-Band). This applies to customers under Rule Part 90. Customers with FCC waivers can contact their Business Development Representative.

DHS Project 25 Compliance Assessment Program (CAP) has defined a "CAP Encryption Requirements compliant radio" as a radio that can be ordered without encryption or one that can be ordered with AES256. << Click to learn more>>

The Master Key Start-Up Kit (DVN4046) is required to use the Hardware Key (QA01648) or to operate on a third-party trunking system if the customer does not already possess one, or if theirs has expired. Please CLICK HERE for further details regarding the DVN4046 Kit.

WI-FI

APX 8000XE supports Wi-Fi 802.11 b/g/n with WPA2/WPA (PSK), and WEP security protocols. Wi-Fi can be used with the Radio Management SW in order to do codeplug updates, firmware refreshes, and FLASHport upgrades over a Wireless Network (WLAN). The radio will only connect to available Wi-Fi networks which have been pre-provisioned in the radio codeplug via CPS. The radio can be pre-provisioned with up to 20 SSIDs.

The Wi-Fi feature requires ordering option QA09001. The Wi-Fi feature is also available aftermarket as a FLASHport upgrade if not ordered out of the factory.

Radio Management (RM) is required in order to take advantage of the Wi-Fi capabilities on APX 8000XE.

OUT OF THE BOX WI-FI PROVISIONING

If a radio is ordered the Wi-Fi option (QA09001) and the customer wishes to provision the radios out of the box using Wi-Fi, the radio must also be ordered with the Out of the Box Wi-Fi Provisioning option (QA09007).
A radio ordered with the Wi-Fi option and the Out of the Box Provisioning over Wi-Fi option will come with the following default codeplug configuration relative to Wi-Fi:

- Wi-Fi will be enabled.
- There will be one pre-configured network with the Network SSID set to “MyNetwork” and security type will be set to “None”.
- The default state of Wi-Fi will be “on”.

A Wi-Fi router is required for connecting the Wi-Fi capable radio to the Device Programmer. The Wi-Fi router is to be procured by the agency programming the radios and must be provisioned with the Network SSID set to “MyNetwork” (case sensitive) with no password enabled.

For more details regarding the Out of the Box Wi-Fi Provisioning process, please refer to the Out of the Box Wi-Fi Provisioning Leaflet.

BLUETOOTH 4.0 & EMERGENCY FIND ME

With Bluetooth 4.0 wireless technology and our APX™ Mission Critical Wireless portfolio, users can now connect a variety of Bluetooth audio accessories and data devices with their APX™ radio.

Bluetooth 4.0 also enables Emergency Find Me, a feature providing personnel with an added level of security by improving response time in emergencies. Once an emergency is activated on the APX 8000XE, a Bluetooth beacon signals other Bluetooth-enabled APX radios within range. Based on bluetooth signal strength, nearby APX radios will receive an emergency alert via intelligent lighting and a text message with users Radio ID along with signal strength status (excellent, poor, fair) to determine proximity, and will guide the nearest personnel to the user in distress.

FLASHPORT AFTERMARKET UPGRADES

The APX 8000XE P25 Portable Radios are part of the FLASHport Program. This means that APX 8000XE hardware models can be loaded with different software packages that provide the features and functionalities that our customers require.

System Enhancement Options can be loaded at the time of radio purchase or at a later date through the use of software field upgrades. The APX 8000 portable can be upgraded electronically in the field with new features in the current system or to new systems operation by ordering upgrade kits.

FLASHport upgrades are supported via Wi-Fi using Radio Management (RM) on APX 8000XE.

Fleet Management software was previously distributed on DVDs shipped out of Elgin. It is now downloadable from motsolutions.com at the link below. Look at the right edge of the page under Resources Spotlight. The first link is the Order Guide which tells you what you need. The second link is a free 90 day trial version that they can download and evaluate free for 90 days. The third link is the actual program, you need to purchase a license to use it (explained in the order guide).

#### Self-Quieting Spurs

7/800 Frequencies | VHF Frequencies | UHF Frequencies
--- | --- | ---
768 | 136.8 | 384
775.2 | 153.6 | 403.2
866.4 | 172.8 | 410.4

### HazLoc Approved Accessories (Div 2)

#### This information is subject to change. For the latest information on accessories approved for HazLoc environments, please refer to the UL manuals and addendums that ship with every HazLoc approved APX 8000XE.

Description | Model
--- | ---
Remote Speaker Microphone with Jack | HMN4101B
Display Remote Speaker Microphone with Jack | HMN4103B
Display Remote Speaker Microphone with Jack and Channel Selector | HMN4104B
Secondary Audio Accessory for Display Remote Speaker Microphone | RLN6424B
XE RSM with High Temperature Cable | NNTN8575A
XE RSM Black with High Temperature Cable | NNTN8575ABLK
IMPRES 2-Wire Surveillance Kit with translucent tube, programmable button, Black | PMLN6129A
Receive-Only Earpiece with Translucent Tube, 3.5 mm Jack, Short Coiled Cable | RLN4941A
Remote Speaker Microphone, IMPRES Wind porting IP55 3.5 mm Jack | PMMN4099A
1 Wire Receive-only Surveillance Kit with Translucent Tube, Black, Requires BDN6783 | RLN5313B
Temple transducer | RMN5116A
Remote Speaker Microphone | PMMN4106A
Remote Speaker Microphone | PMMN4106ABLK
Remote Speaker Microphone | PMMN4106B
Remote Speaker Microphone | PMMN4106ABBLK
Remote Speaker Microphone | PMMN4107A
Remote Speaker Microphone | PMMN4107ABLK
IMPRESS 2 Wire with Translucent Tube Black | PMLN7565A
IMPRES ANC RSM UL/Long CBL/NEX/3.5 | PMMN4102B
IMPRES ANC RSM UL/Long CBL/NEX/3.5/Green | PMMN4102BGRN
IMPRES OMNI RSM Long CBL/NEX/3.5 | PMMN4113A
Earpiece, ENH ATEX 3.5mm Earpiece with Translucent Tube | PMLN7188B
Remote Speaker Microphone, IP68 | PMMN4099B
Remote Speaker Microphone, High Impact Green | PMMN4106C
Next Gen Fire, Remote Speaker Microphone, Model 1.5 | PMMN4107B

### Ship Card

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
APX_PORTABLE | US1 | H112LT | DEL: DELETE STANDARD ANTENNA | 0579 |
APX_PORTABLE | US1 | H207EY | DEL: DELETE BATTERY | 0655 |
APX_PORTABLE | US1 | H799BB | ADD: TEST RESULTS / RATED AUDIO PRINTOUT | 0579 |
PORTABLES | FSC | H91TGD9PW5 N | APX 8000 ALL BAND PORTABLE MODEL 1.5 | 579 | 81
PORTABLES | FSC | H91TGD9PW6 N | APX 8000 ALL BAND PORTABLE MODEL 2.5 | 579 | 1
PORTABLES | FSC | H91TGD9PW7 N | APX 8000 ALL BAND PORTABLE MODEL 3.5 | 579 | 46
APX_PORTABLE | US1 | Q15AJ | ADD: AES/DES-XL/DES-OFB ENCRYPTION AND ADP | 0655 |
ASTRO_SUBS_SOFTWARE | US1 | Q667BB | ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | 0430 |
APX_PORTABLE | US1 | QA01648AA | ADD: HW KEY SUPPLEMENTAL DATA | 0655 |
APX_PORTABLE | US1 | QA05507AA | DEL: DELETE 7/800 MHZ BAND | 0579 |
APX_PORTABLE | US1 | QA05508AA | DEL: DELETE VHF BAND | 0579 |
APX_PORTABLE | US1 | QA05509AA | DEL: DELETE UHF BAND | 0579 |
APX_PORTABLE | US1 | QA05751AA | ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | 0655 |
APX_PORTABLE | US1 | QA07680AA | ADD: MULTI SYSTEM OTAR | 0655 |
APX_PORTABLE | US1 | QA07682AA | ADD: SMARTCONNECT | 0579 |

### Product Specifications

Firefighters said they wanted equivalent extreme features as the APX XE Series including a larger display, exaggerated control knobs and the capability to communicate with surrounding municipalities within an all-band radio solution. The APX 8000XE brings together not only these requirements, but also the integration of WiFi for programming flexibility.
The APX 8000XE is redefining mission critical communications by delivering an ultra-durable radio that combines unlimited interoperability, loud audio and secure WiFi connectivity. With a dedicated channel knob and ability to withstand 500˚F (260˚C) heat exposure, the APX XE500 Remote Speaker Microphone is the perfect companion to the APX 8000XE. When combined, the APX 8000XE All-Band Portable Radio and XE500 Remote Speaker Microphone create the ultimate mission critical solution designed for safety personnel in extreme environments.