Back

##### APX 8000HXE

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Software and Services
- Ship Card

Back

##### APX 8000HXE

### Model

·

·

·

·

·

·

APX™ 8000HXE P25 All-Band Portable Radio

700/800 MHz

VHF

UHF R1 & UHF R2

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

NEW: Beginning September 2023 APX radios can be ordered with the New Feature/Latest release or the Baseline release firmware. The Baseline release is defined as a single major software release (i.e. 202X.1) to ship from the factory for a 1 year duration. The first major release each year will be the Baseline Release. A New Feature Release is defined as the second and third major releases each year (202X.2 and 202X.3) and is required for customers to access new feature content and/or products. New Feature releases contain the current year’s Baseline content as well as content from the previous New Feature release.

IMPORTANT! Radios that are ordered via COF must add the Baseline Release option (QA09113) if the Baseline firmware is desired. If the Baseline option (QA09113) is not added to COF orders, radios will ship with the Latest Release and cannot be rolled back to the Baseline Release. Most quotes and orders should keep the default Baseline Firmware (QA09113) unless a customer desires new functionality only provided in a New Feature release. More information about the Baseline and New Feature Release strategy can be found in MTN-0111-23-NA.

NEW 2022: Please note H02 option STUN/KILL does not require encryption. We do "Recommend ordering encryption (other than ADP only selection), otherwise radios will be susceptible to remote STUN/KILL from an adversary."

Effective October 5th, 2020: All U.S. orders will require an encryption selection. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. G193/Q667 ADP only is also available at $0. Please see encryption section for AES and other encryption options that come with ADP. Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.

HAZARDOUS LOCATION

The APX 8000HXE will ship standard with PMNN4547. The APX 8000HXE is certified by Underwriters' Laboratory when properly equipped with the standard battery, PMNN4547. There is no option to delete this battery on this model.

When equipped with Motorola Battery PMNN4547, the APX 8000HXE models are certified as intrinsically safe for use in ANSI/TIA 4950-A ; Classification Rating Class I, Division 1, Groups C, D; Class II, Division 1, Group E, F, G; Class III, Hazardous (Classified) Locations. ANSI/ISA 12.12.01-2015 and CAN/CSA C22.2 No.213-15; Class I, Division 2, Groups A, B, C, D; T3C. Tamb = -25° C to +60° T3C.

Canada Customers: When equipped with Motorola Battery PMNN4547, the APX 8000HXE models are certified as intrinsically safe for use in CAN/CSA C22.2 NO. 157-92; Classification Rating Class I, Division 1, Group D; Class II, Division 1, Group E, F, G; Class III, Hazardous (Classified) Locations. ANSI/ISA 12.12.01-2015 and CAN/CSA C22.2 No.213-15; Class I, Division 2, Groups A, B, C, D; T3C. Tamb = -25° C to +60° T3C.

Special Note for United States - State & Local Markets Only
In accordance with FCC mandate, the APX 8000HXE all band radio is restricted to 12.5 KHz operation only and does NOT support 25 KHz in the VHF and UHF Bands (excluding T-Band). This applies to customers under Rule Part 90. Customers with FCC waivers can contact their Business Development Representative.

DHS Project 25 Compliance Assessment Program (CAP) has defined a "CAP Encryption Requirements compliant radio" as a radio that can be ordered without encryption or one that can be ordered with AES256. << Click to learn more>>

### Ordering Information

Ordering Guide

Standard Features

All ASTRO Digital APX 8000HXE models include the following features:

- All-Band Capability (UHF, VHF, 7/800)

- Adaptive Audio Engine

- GPS Software & Hardware (QA00782)

- Mission Critical Wireless Bluetooth® 4.0 (LE) (QA00583)

- Radio Packet Data (Q947)

- Software Key (QA01749)

- Extreme 1-Sided Noise Reduction (QA01833)

- One Touch/Status Message (H46)

- Radio Trace/Remote Monitor (H43)

- Enhanced Zone Bank (QA01768)

- 3 Programmable Side Buttons
- Orange Programmable Button
- 16 Position Mode Rotary Select Switch
- Angled On/Off Volume Knob
- 1 Top Mounted Programmable 3 Position Toggle Switch

- Top Display: 1 line of text, 1 line of icons, 0 menu lines
- Dual Microphone

- 3 Watt Rated Audio

- Carry Holder (PMLN7954)

- IMPRES 2 Battery (PMNN4547)

- All-Band Antenna (AN000342A01)

- Models 2.5 & 3.5:

- Unified Call List
- Front Color Display: 4 Lines of Text, 2 Lines of Icons
- Radio Profiles
- 3 Programmable Buttons
- 4-Way Navigation
- Home & Data Buttons

- Model 3.5: 4 X 3 Alpha-Numeric Keypad

- MIL-STD Delta-T, IP68 submersion (2m, 4hr)

#### APX 8000HXE must be ordered with the following options: QA02006 & QA01427

#### Additional Ordering Information for Service Options

SmartConnect End to End Ordering Guide

### Configuration

#### Models

1: Base Radio $14,375.42 List $7,906.48 Disc $6,656.48 w/Trade

Description | Full Description | Nomenclature | APC | Price
APX 8000H ALL BAND PORTABLE MODEL 3.5 | - | H91TGD9PW9 N | 673 | inc.
ADD: SMARTZONE OPERATION |  | H38 | 655 | inc.
ADD: P25 9600 BAUD TRUNKING |  | Q361 | 655 | inc.
ADD: ASTRO DIGITAL CAI OPERATION |  | Q806 | 579 | inc.
ADD: TDMA OPERATION |  | QA00580 | 655 | inc.
ADD: PROGRAMMING OVER P25 (OTAP) |  | G996 | 655 | inc.
ADD: DVRS PSU ACTIVATION |  | QA00631 | 655 | inc.
ADD: GROUP SERVICES |  | QA09008 | 655 | inc.
ADD: ENHANCED DATA APX |  | QA03399 | 656 | inc.
ADD: SMARTCONNECT |  | QA07682AA | 0579 | inc.
ADD: HW KEY SUPPLEMENTAL DATA |  | QA01648AA | 0655 | inc.
ENH: APX8000XE RUGGED RADIO | - | QA02006 | 673 | inc.
ALT:APX 8000 HOUSING GREEN | - | QA01427 | 579 | inc.

4: Delete Frequency Bands (Optional. Can select a MAXIMUM of TWO)

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE UHF BAND | Deletes both UHF R1 and UHF R2 frequency bands | QA05509AA | 0579 | ($800.00)
DEL: DELETE VHF BAND | DEL: DELETE VHF BAND | QA05508AA | 0579 | ($800.00)

5: RFID Enabled Volume Knob (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: RFID KNOB | Compatible with APX6000, APX7000 & APX8000. Portable radio volume knob with embedded RFID tag making it easier to track assets. When option is ordered, RFID Volume knob will come in the box with the portable radio and other ordered accessories but RFID knob will not be assembled to the radio. AFTERMARKET purchase through Parts department for fielded radios NNTN8646 (APX6000/APX7000/APX8000) and NNTN8647 (APX6000XE/APX7000XE/APX8000XE). See RFID Solution Partner link for information on partners that can provide customers with scanner hardware and back end asset management solutions. | QA04526 | 655 | $30.00

6: System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 Trunking (Q361) | QA01767 | 655 | $118.00
ADD: WIFI CAPABILITY | Enables Wi-Fi capability in the radio. Supports codeplug updates, firmware refreshes, and FLASHport upgrades over pre-provisioned wireless networks. Requires Radio Management SW (ordered separately). Must order Out of the Box Wi-Fi Provisioning option (QA09007) if provisioning the radios out of the box using Wi-Fi is desired. | QA09001 | 579 | $353.00
ADD: OUT OF THE BOX WIFI PROVISIONING | Requires Wi-Fi (QA09001). Must be added if provisioning the radios out of the box using Wi-Fi is desired. Refer to the 'Out of the Box Wi-Fi Provisioning' section above for details. | QA09007 | 579 | $0.00

8: Algorithm Types (Required)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

Description | Full Description | Nomenclature | APC | Price
CHIFFRAGE AES | Requires digital operation. P25 CAP Compliant option. Includes ADP. | Q629 | 655 | $523.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | Q667BB | 0430 | $0.00

9: Multikey Types (Optional)

Description | Full Description | Nomenclature | APC | Price
ENH: MULTIKEY | Required when purchasing more than one encryption algorithm or encryption key? "Requires MultiKey". | H869 | 655 | $363.00
MULTICLE OTAR ASTRO P25 | Includes Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. | Q498 | 655 | $814.00
ADD: MULTI SYSTEM OTAR | Requires Q498 ASTRO 25 OTAR W/ MULTIKEY | QA07680AA | 0655 | $177.00

#### Battery (Optional- Can Only Select One)

HAZLOC Approved

Description | Full Description | Nomenclature | APC | Price
ADD: BATT IMPRES 2 LIION TIA4950 IP68 | This option will delete the standard battery and replace it with TIA4950 BATT IMPRES 2 LIION 4600MAH (PMNN4573A) | QA07576 | 673 | $204.00

Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: APX DATA CABLE | PMKN4012B- Used to program the radio with Customer Programming Software and Tuner Software. PMKN4013C - Used to program and service the radio with Customer Programming Software and Tuner Software. Compatible on ALL APX Portable Radios | Q157 | 655 | $89.00

Belt Clips (Optional-Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE BELT CLIP/BASIC CARRY HOLDER | This option deletes the XE carry holder, PMLN7954. | H301 | 655 | ($10.00)

Packaging (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: SINGLE UNIT PACKING | - | H842 | 481 | $0.00

Service Options (Must Select One)

Description | Full Description | Nomenclature | APC | Price
EHN: STD 1 YR WARRANTY APPLIES | Provides no extended repair coverage after the standard warranty period expires. | QA05100AA | 0185 | $0.00
ADD: 3Y ESSENTIAL SERVICE | Provides 3 years of hardware coverage beginning at time of purchase. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | Q58 | 185 | $184.00
ADD: 3Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 3 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00022AC | 185 | $347.00
ADD: 5Y ESSENTIAL SERVICE | Provides 5 years of hardware coverage beginning at time of shipment. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | Q887 | 185 | $306.00
ADD: 5Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 5 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00025AH | 185 | $578.00
ADD: 7Y ESSENTIAL SERVICE HTP | Provides 7 years of hardware coverage beginning at time of shipment. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00690 | 185 | $386.00
ADD: 7Y ESSENTIAL W ACC DMG HTP | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 7 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00691 | 185 | $729.00

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
RadioManagement (On-Prem) | See “How to Order” section in the Ordering Guide below. | N/A | N/A | N/A

Documentation (Optional)

Online copies of User Guides can be found in the Resources Tab

Description | Full Description | Nomenclature | APC | Price
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799BB | 0579 | $12.00
ADD: APX8000H USER GUIDE | - | H88 | 673 | $30.00

#### Audio Accessories

Description | Full Description | Nomenclature | APC | Price
CARRY ACCESSORY-CASE,APX8000HXE LEATHER CARRY CASE | - | PMLN7955A | 271 | $75.00
XVE500 DIV 1 REMOTE SPEAKER MIC, HIGH IMPACT GREEN WITHOUT KNOB, UL | - | PMMN4152A | 372 | $707.00
XVE500 DIV 1 REMOTE SPEAKER MIC, BLACK WITHOUT KNOB, UL | - | PMMN4152ABLK | 372 | $756.00
XVE500 DIV 1 REMOTE SPEAKER MIC, HIGH IMPACT GREEN WITH KNOB, UL | - | PMMN4154A | 372 | $748.00
XVE500 DIV 1 REMOTE SPEAKER MIC, BLACK WITH KNOB, UL | - | PMMN4154ABLK | 372 | $800.00

### Software and Services

WI-FI

APX 8000HXE supports Wi-Fi 802.11 b/g/n with WPA2/WPA (PSK), and WEP security protocols. Wi-Fi can be used with the Radio Management SW in order to do codeplug updates, firmware refreshes, and FLASHport upgrades over a Wireless Network (WLAN). The radio will only connect to available Wi-Fi networks which have been pre-provisioned in the radio codeplug via CPS. The radio can be pre-provisioned with up to 20 SSIDs.
The Wi-Fi feature requires ordering option QA09001. The Wi-Fi feature is also available aftermarket as a FLASHport upgrade if not ordered out of the factory.
Radio Management (RM) is required in order to take advantage of the Wi-Fi capabilities on APX 8000HXE.

OUT OF THE BOX WI-FI PROVISIONING

If a radio is ordered the Wi-Fi option (QA09001) and the customer wishes to provision the radios out of the box using Wi-Fi, the radio must also be ordered with the Out of the Box Wi-Fi Provisioning option (QA09007).
A radio ordered with the Wi-Fi option and the Out of the Box Provisioning over Wi-Fi option will come with the following default codeplug configuration relative to Wi-Fi:
a. Wi-Fi will be enabled.
b. There will be one pre-configured network with the Network SSID set to “MyNetwork” and security type will be set to
“None”.
c. The default state of Wi-Fi will be “on”.
A Wi-Fi router is required for connecting the Wi-Fi capable radio to the Device Programmer. The Wi-Fi router is to be procured by the agency programming the radios and must be provisioned with the Network SSID set to “MyNetwork” (case sensitive) with no password enabled.

For more details regarding the Out of the Box Wi-Fi Provisioning process, please refer to the Out of the Box Wi-Fi Provisioning Leaflet.

Bluetooth 4.0 & Emergency Find Me

With Bluetooth 4.0 wireless technology and our APX™ Mission Critical Wireless portfolio, users can now connect a variety of Bluetooth audio accessories and data devices with their APX™ radio.

Bluetooth 4.0 also enables Emergency Find Me, a feature providing personnel with an added level of security by improving response time in emergencies. Once an emergency is activated on the APX 8000HXe, a Bluetooth beacon signals other Bluetooth-enabled APX radios within range. Based on bluetooth signal strength, nearby APX radios will receive an emergency alert via intelligent lighting and a text message with users Radio ID along with signal strength status (excellent, poor, fair) to determine proximity, and will guide the nearest personnel to the user in distress.

FLASHPORT AFTERMARKET UPGRADES

The APX 8000HXE P25 Portable Radios are part of the FLASHport Program. This means that APX 8000HXE hardware models can be loaded with different software packages that provide the features and functionalities that our customers require.

System Enhancement Options can be loaded at the time of radio purchase or at a later date through the use of software field upgrades. The APX 8000H portable can be upgraded electronically in the field with new features in the current system or to new systems operation by ordering upgrade kits.

FLASHport upgrades are supported via Wi-Fi using Radio Management (RM) on APX 8000HXE.

#### Self-Quieting Spurs

7/800 Frequencies | VHF Frequencies | UHF Frequencies
768 | 136.8 | 384
775.2 | 153.6 | 403.2
866.4 | 172.8 | 410.4

### HazLoc Approved Accessories

#### This information is subject to change. For the latest information on accessories approved for HazLoc environments, please refer to the UL manuals and addendums that ship with every HazLoc approved APX 8000HXE.

Description | Model
Remote Speaker Microphone | PMMN4106A
Remote Speaker Microphone | PMMN4106ABLK
OTH headset | PMLN7467A
Remote Speaker Microphone | PMMN4107A
Remote Speaker Microphone | PMMN4107ABLK
1-Wire Surveillance Kit-BLK | PMLN7561A
1-Wire Surveillance Kit-BGE | PMLN7562A
IMPRES 2-Wire Surveillance-BLK | PMLN7563A
IMPRES 2-Wire Surveillance-BGE | PMLN7564A
IMPRES 2-Wire with Transparent Tube BLK | PMLN7565A
IMPRES 2-Wire with Transparent Tube BGE | PMLN7566A
IMPRES 3-Wire with Transparent Tube BLK | PMLN7567A
IMPRES 3-Wire with Transparent Tube BGE | PMLN7568A
IMPRES ANC Remote Speaker Microphone UL/Long Cable/ NEX/3.5 mm | PMMN4102B
IMPRES ANC Remote Speaker Microphone UL/Long Cable/ NEX/3.5/Green | PMMN4102BGRN
IMPRES OMNI Remote Speaker Microphone Long Cable/NEX/ 3.5 mm | PMMN4113A
Earpiece, ENH ATEX 3.5 mm Earpiece with Transparent Tube | PMLN7188B
Remote Speaker Microphone | PMMN4099A
Remote Speaker Microphone, High Impact Green | PMMN4106B
Remote Speaker Microphone | PMMN4106BBLK
Surveillance Kit | PMLN6123A
Surveillance Kit | PMLN6124A
Earpiece | PMLN6125A
Earpiece | PMLN6126A
Surveillance Kit | PMLN6127A
Surveillance Kit | PMLN6128A
Surveillance Kit | PMLN6129A
Surveillance Kit | PMLN6130A
Earpiece | BDN6666A
Earpiece | BDN6668A
Earpiece | BDN6726A
Earpiece | BDN6727A
Earpiece | BDN6728A
Earpiece | BDN6729A
Earpiece | BDN6730A
Earpiece | BDN6731A
Earpiece | BDN6732A
Remote Speaker Microphone | NNTN8235A
Remote Speaker Microphone | NNTN8236A
Remote Speaker Microphone | PMMN4040A
Remote Speaker Microphone | PMMN4062A
Remote Speaker Microphone | PMMN4065A
Remote Speaker Microphone | PMMN4069A
Earpiece | PMLN4620B
Earset | PMLN5096B
Headset | PMLN5275C
Headset | PMLN6853A
Earpiece | RLN4941A
Public Safety Microphone | PMMN4059B
Public Safety Microphone | PMMN4060B
Public Safety Microphone | PMMN4061B
Surveillance Kit | RLN5313B
Earbud | RLN4885B
Audio Accessory Adaptor, 3.5 mm, with PTT | BDN6783B
Remote Speaker Microphone | PMMN4099B
Remote Speaker Microphone, High Impact Green | PMMN4106C
Remote Speaker Microphone | PMMN4024A
Remote Speaker Microphone | PMMN4025A
Next Gen Fire, Remote Speaker Microphone, Model 1.5 | PMMN4107B
Headset, Headband | RMN5137B
Headset, Neckband | RMN5138B
Headset, Hard Hat Attach Mounted | RMN5139B
Remote Speaker Microphone | PMMN4106D
Remote Speaker Microphone | PMMN4107C
Remote Speaker Microphone | PMMN4106CBLK
Remote Speaker Microphone | PMMN4107BBLK

####