Back

##### APX N50

###### Product Catalog

##### Jump to ...

- APX N50™
- Configuration
- Software and Services
- HazLoc Approved Accessories (UL Div 1)
- Ship Card

Back

##### APX N50

### APX N50™

·

·

·

·

·

Introducing APX N50, a next generation single band portable

Staying connected and being able to collaborate, whenever, wherever, is a prerequisite for mobile workers. Our APX N50 is a slim yet tough pick-up-and-go radio that’s designed to give first responders, public-safety support and administrative staff secure communications they can rely on in the field.

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

- New!! Intelligence Noise Reduction (QA10089) is now available on APX N50 models with the latest release SR2025.2

- NOTE: Do not use PMMN4815A battery with the APX N50 and N30 UHF models H25XDF9PW6AN and H15XDF9PW6AN

- The Essential Core Bundle includes ADP encryption (Q667). If a clear radio is required, QA05751 "Clear Radio No ADP" must be selected, OR, select the Essential Security Bundle which includes AES (Q629). When selecting Custom Configuration be aware that all U.S. orders will require an encryption selection. Q667 ADP Only is available at $0. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. Please see the encryption section for AES and other encryption options that include ADP.

- WARNING: Radios shipped with QA05751 Clear Radio No ADP are NOT field-upgradable for encryption and any changes will require the units to be sent to a Motorola depot.

Standard Features

All ASTRO Digital APX N50™ models include the following features:

- Supported bands (700/800MHz, VHF, & UHF only)

- ADP Privacy - Single Key (Q667)

- Radio Packet Data (Q947)

- Software Key (QA01749)

- GPS Software & Hardware (QA00782)

- Wireless Bluetooth® 4.2 (LE) (QA00583)

- Intelligent Noise Reduction (QA010089) with 2025.2 Release

- Front Display: 2.4” TFT Transflective, 24-bit Full Color

- 16 Position Mode Rotary Select Switch
- On/Off Volume Knob

- 3 Programmable Side Buttons

- 3 Programmable Front Buttons

- Limited Keypad: Backlight keypad with 3 soft keys, 4 direction keys, home and notification button

- Orange Programmable Button

- 2 High Dynamic Range Microphones

- IP68 (2 m, 2 hr)

Standard Radio configuration includes the following:

- IMPRES 2 Battery 2850 mAh IP68 (PMNN4813)

- Single Band Antenna (Band dependent)

- Plastic 2.0" Belt Clip (PMLN8369)

- Side Connector Dust Cover (PMHN4429A)

#### Models

1: Base Radio $6,666.42 List $3,666.53 Disc $2,666.53 w/Trade

Description | Full Description | Nomenclature | APC | Price
PORTABLE RADIO APX N50 7/800 MODEL 2 |  | H25UCF9PW6AN | 0287 |
SOFTWARE LICENSE ENH: 3600 OR 9600 TRUNKING BAUD SINGLE SYSTEM |  | QA02756AB | 0426 |
ADD:BASIC VOICE CONTROL |  | QA08715AA | 0681 |
ADD: DVRS PSU ACTIVATION |  | QA00631 | 655 |
ADD: ENHANCED DATA APX |  | QA03399 | 656 |
ADD: GROUP SERVICES |  | QA09008 | 655 |
SOFTWARE LICENSE ENH: TRUNKED RADIO TRACE/ REMOTE MO |  | H43BJ | 0426 |
ADD: PROGRAMMING OVER P25 (OTAP) |  | G996 | 426 |
ADD: TDMA OPERATION |  | QA00580 | 426 |
ADD: SMARTCONNECT N30/N50 |  | QA07682AC | 0579 |
ADD: HW KEY SUPPLEMENTAL DATA |  | QA01648AA | 0655 |

### Configuration

#### System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: ADAPTIVE NOISE SUPPRESSION | - | QA09006AA | 0579 | $177.00
ADD: ADAPTIVE SPEAKER VOLUME | Includes Rx Volume Leveling & Noise Sensing Volume Control (NSVC) | QA08676AA | 0411 | $177.00
EXTREME NOISE REDUCTION | - | QA01833 | 426 | $30.00
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 trunking operation | QA01767 | 426 | $118.00
ADD: WIFI CAPABILITY | Enables Wi-Fi capability in the radio. Supports codeplug updates, firmware refreshes, and FLASHport upgrades over pre-provisioned wireless networks. Requires Radio Management SW (ordered separately). Must order Out of the Box Wi-Fi Provisioning option (QA09007) if provisioning the radios out of the box using Wi-Fi is desired. | QA09001AM | 0437 | $353.00
ADD: OUT OF THE BOX WIFI PROVISIONING | Requires Wi-Fi (QA09001). Must be added if provisioning the radios out of the box using Wi-Fi is desired. Refer to the 'Out of the Box Wi-Fi Provisioning' section above for details. | QA09007AD | 0837 | $0.00
ENHANCEMENT LEVEL 1 | This option increases the limits of some codeplug parameters (ZONES, CHANNELS, SYSTEMS PERSONALITIES, UCL ENTRIES, VOICE ANNOUNCEMENT, ENCRYPTION KEYS). Please refer to the Software Catalog for more details. | QA01770 | 426 | $220.00
ADD: INTELLIGENT NOISE REDUCTION | Enhanced audio processing improves speech clarity by reducing ambient noise. Available with SR2025.2 | QA10089AA | 0437 | $177.00

#### Encryption Type (Required)

Description | Full Description | Nomenclature | APC | Price
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | Q667BB | 0430 | $0.00
SOFTWARE LICENSE ENH: AES ENCRYPTION AND ADP | Requires digital operation. P25 CAP Compliant option. Includes ADP. | Q629BD | 0437 | $560.00

#### Multikey Type (Required)

CPQ will require a multikey selection. "No Multikey" is a zero cost option available, but it may not be available with every encryption type selection.

Description | Full Description | Nomenclature | APC | Price
SOFTWARE LICENSE ENH: MULTIKEY | Required when using more than one encryption algorithm or encryption key | H869DB | 0437 | $388.00
SOFTWARE LICENSE ENH: ASTRO 25 OTAR W/ MULTIKEY | Not compatible with ADP-Only. Includes multikey, trunking OTAR, and Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. | Q498BN | 0437 | $871.00
ADD: MULTI SYSTEM OTAR | Requires Q498 ASTRO 25 OTAR W/ MULTIKEY | QA07680AA | 0655 | $177.00

#### Antenna (Optional)

The APX N50 ships with a standard antenna dependent on frequency (7/800 MHz: AN000411A01, VHF: AN000421A01, UHF: AN000452A01). You may select an alternate antenna from the list below.

Description | Full Description | Nomenclature | APC | Price
ALT: 7800 STUBBY 762-870MHZ | 7/800 Model Only. Replaces 7/800 whip antenna (AN000411A01) with 7/800 stubby antenna (AN000418A01) 10 cm. Will be available October, 2023. | QA08681AA | 0287 | $30.60

#### Battery Selection (Optional)

APX N50 ships standard with the LI-ION IMPRES 2 IP68 2850T mAh battery (PMNN4813). You may select an alternate battery from the list below.

NOTE: APX N50 batteries are only compatible with PMPN4819 Single Unit Charger and PMPN4593 6-Slot Multi Unit Charger.

Description | Full Description | Nomenclature | APC | Price
ALT: BATT LIION IMPRES 2 DIV 1 IP68 3200T | PMNN4815 IMPRES 2, LiIon, IP68, TIA4950, 3200mAh Battery Note: PMNN4815B is compatible with the UHF model. PMNN4815A is not compatible with UHF | QA08679AA | 0287 | $207.29
DEL: DELETE BATTERY | This option lets you delete the battery on N50 7/800, VHF, and UHF. | QA08686AA | 0287 | $0.00
ALT: BATT LIION IMPRES 2 DIV 1 IP68 3200T | Note: PMNN4815B is compatible with the UHF model. PMNN4815A is not compatible with UHF | QA08772AB | 0657 | $207.29

#### Belt Clip (Optional)

APX N50 ships standard with the 2.0" BELT CLIP (PMLN8369) You may select an alternate carry solution from the list below.

Description | Full Description | Nomenclature | APC | Price
ALT:2.5" BELT CLIP | Consists of: PMLN8370A APX N50 2.5" BELT CLIP | QA08684AA | 0287 | $13.77
DEL: BELT CLIP | - | QA08685AA | 0287 | ($10.00)

#### Packaging Selection (Optional)

APX N50 ships standard in Bulk (10 radios per box). Select QA08688 if you wish to have radios packaged in Individual boxes.

Description | Full Description | Nomenclature | APC | Price
ADD:SINGLE UNIT PACKAGING | - | QA08688AA | 0287 | $0.00

#### Factory Configuration (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799BH | 0437 | $12.00

#### SMA Antenna Adaptor (sold separately aftermarket)

Description | Nomenclature
SERVICE TOOL,RF ADAPTOR | AY000811A01

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programminging solutions including features like batch programming and programming over WiFi, you will need to order one of the below tools. You may select between 1-5 years of access. RadioManagement (MSI Hosted) is ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
RadioManagement (On-Prem) | See “How to Order” section in the below Ordering Guide. | N/A | N/A | N/A

#### Device Management Services (DMS)

Includes hardware repair, tech support, firmware updates and MyView access, with the option to add Accidental Damage. Can select 3, 5 or 7 years of coverage. Ordered per device.

Description | Full Description | Nomenclature | APC | Price
APX N50/30 DMS Essential | Provides HW repair, tech support, firmware updates and MyView | LSV01S03084A | 723 | $52.75
APX N50/30 DMS Essential with Accidental Damage | Provides accidental damage and HW repair, tech support, firmware updates and MyView | LSV01S03085A | 723 | $102.46

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

### Application Services

Available applications for the APX N50 and APX N30 include SmartConnect and can be ordered for up to 5 years.

If this is the first time you are quoting APX N-Series (including APX NEXT and N-Series) to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX N-Series radios and enable the customer system to support the required application services.

Refer to the End-to-End ordering guide below for more details.

Description | Nomenclature | Duration | Single App Service | APC
APX SmartConnect | SSV01S01663A | 1-5 Years | $96.00 | 712

#### Please refer to the End-to-End ordering guides below to see all components required to enable Application Services.

- SmartConnect

#### If this is the first time SmartConnect is being deployed on the customer's system, please engage your Pre-Sales team to ensure that all system components required to enable the services are ordered.

### Software and Services

Wi-Fi

APX N50 supports Wi-Fi 802.11 b/g/n with WPA2/WPA (PSK), and WEP security protocols. Wi-Fi can be used with the Radio Management SW in order to do codeplug updates, firmware refreshes, and FLASHport upgrades over a Wireless Network (WLAN). The radio will only connect to available Wi-Fi networks which have been pre-provisioned in the radio codeplug via CPS. The radio can be pre-provisioned with up to 20 SSIDs.
The Wi-Fi feature requires ordering option QA09001. The Wi-Fi feature is also available aftermarket as a FLASHport upgrade if not ordered out of the factory.

Radio Management (RM) is required in order to take advantage of the Wi-Fi capabilities on APX N50.

Out of the Box WiFi Provisioning

If a radio is ordered the Wi-Fi option (QA09001) and the customer wishes to provision the radios out of the box using Wi-Fi, the radio must also be ordered with the Out of the Box Wi-Fi Provisioning option (QA09007).
A radio ordered with the Wi-Fi option and the Out of the Box Provisioning over Wi-Fi option will come with the following default codeplug configuration relative to Wi-Fi:
a. Wi-Fi will be enabled.
b. There will be one pre-configured network with the Network SSID set to “MyNetwork” and security type will be set to “None”.
c. The default state of Wi-Fi will be “on”.
A Wi-Fi router is required for connecting the Wi-Fi capable radio to the Device Programmer. The Wi-Fi router is to be procured by the agency programming the radios and must be provisioned with the Network SSID set to “MyNetwork” (case sensitive) with no password enabled.

For more details regarding the Out of the Box Wi-Fi Provisioning process, please refer to the Out of the Box Wi-Fi Provisioning Leaflet

Bluetooth 4.0 & Emergency Find Me

With Bluetooth 4.0 wireless technology and our APX™ Mission Critical Wireless portfolio, users can now connect a variety of Bluetooth audio accessories and data devices with their APX™ radio.

Bluetooth 4.0 also enables Emergency Find Me, a feature providing personnel with an added level of security by improving response time in emergencies. Once an emergency is activated on the APX 6000, a Bluetooth beacon signals other Bluetooth-enabled APX radios within range. Based on bluetooth signal strength, nearby APX radios will receive an emergency alert via intelligent lighting and a text message with users Radio ID along with signal strength status (excellent, poor, fair) to determine proximity, and will guide the nearest personnel to the user in distress.

### Billing Options

#### Service Activation Delay

To accommodate the lead time sometimes required for new system deployments and radio configuration, customers may elect to delay the start of the Application Services and Device Managed Services contracts.

Service Activation Delay is available for 30 days after the shipment of radios.

#### Billing Options

Device purchases are invoiced at the time of shipment.

Service billing options are: Immediate, Annually, Monthly in Arrears (Federal only)

### Self-Quieting Spurs

7/800MHz | VHF
768 | 136.8
775.2 | 144
864 | 148.8
866.4 | 148.962

### HazLoc Approved Accessories (UL Div 1)

This information is subject to change. For the latest information on accessories approved for HazLoc environments, please refer to the UL manuals and addendums that ship with every HazLoc approved APX N50 radio.

Audio Accessories | Model
RM780 IMPRES WINDPORTING REMOTE SPEAKER MICROPHONE, LARGE (IP68) | PMMN4128
RM760 IMPRES WINDPORTING REMOTE SPEAKER MICROPHONE, LARGE (IP68) | PMMN4140
2-WIRE SWIVEL LOUD AUDIO EARPIECE WITH EARTIP | PMLN8295
BEHIND-THE-HEAD HEADSET | PMLN8085
OVER-THE-HEAD HEADSET | PMLN8086
REPLACEMENT CABLE FOR RSM | PMKN4232
RX ONLY XL CLEAR TUBE EARPIECE, 3.5MM JACK | PMLN8120

Antenna | Model
ANTENNA, WHIP, ANTENNA, WHIP, 136-174 MHz, 15CM, FERRULE | AN000411A01
ANTENNA, WHIP, ANTENNA, WHIP, 762-870 MHz, 18CM, FERRULE | AN000421A01
ANTENNA, STUBBY, ANTENNA, STUBBY, 762-870 MHz, 10 CM FERRULE | AN000418A01
ANTENNA, WHIP,ANTENNA, WHIP,ANTENNA, WHIP, 380-520MHZ, 12CM, FERRULE | AN000452A01

Batteries | Model
BATT LIION IMPRES 2 DIV 1 IP68 3200T | PMNN4815_