Back

##### APX 6000Li FLASHport

###### Product Catalog

##### Jump to ...

- Model
- Ordering Information
- Configuration
- Ship Card

Back

##### APX 6000Li FLASHport

### Model

ASTRO® Digital APX 6000Li
FLASHport® Aftermarket Upgrades
Secure and Trunked Radio Systems

### Ordering Information

#### General Information

FLASHport® Aftermarket Software is used to upgrade to the latest version of your System Enhancement Software Package to upgrade to a different System Enhancement Software Package or to order enhancements for existing for existing ASTRO® Digital APX 6000Li radios in the field. FLASHport® upgrade kits contain upgrade software, FLASHkey, and upgrade documentation.

There is a new way to upgrade radios in the field. The current method, which makes use of the FLASHport USB dongle, will be supported, but for those looking for a more convenient way, the new online method supported in Radio Management (RM) offers the following advantages:

- Reduce wait time by retrieving the order electronically, rather than via the FLASHport USB dongle
- Work more efficiently by using RM to automatically filter for those radios to which the upgrade order can be applied
- Work in parallel because you are no longer limited by the number of physical FLASHort USB dongles you have

NOTE: Radio Management must be deployed to manage your fleet of APX radios before you can use the online FLASHport method in Radio Management to upgrade radios. For more information on Radio Management please refer to the ASTRO Radio Management page.

#### Ordering Requirements

1. Specify the current System Enhancement Software Package that represents the software in the radio as the main line item ( T7813A, T815A, T816A, T817A, T818A)

2. If you choose to use Radio Management to perform the upgrade, enter the online delivery method (UA00083AA) as a sub-item, quanitity of 1 only. No selection is needed if using the traditional USB dongle.

3. Select the desired Operational Mode, System Enhancement Software Package, and/or System Enhancement Options and enter as sub-items.

4. IMPORTANT: If you are remaining at the same System Enhancement Software Package, use the column of the current System Enhancement Software Package to determine price and availability of System Enhancement Options.

5. ALL sub-items must have the same quantity listed (which equals the number of radios being upgraded) even though the main line is ALWAYS 1.

6. Radio Model number and EXISTING FLASHcode must be entered into designated COF fields. A separate line item must be entered for each different combination of Radio model and EXISTING FLASHcode.

7. "FLASH upgrades are not discountable"

NOTE: The FLASHcode can be read by using a USB cable.

OPERATION MODES (List as sub items) |  |  |  |  |
ENH: ASTRO® Digital CAI Operation Q808 NOTE 1 | X | X | N/A | N/A | N/A
SYSTEM ENHANCEMENT SOFTWARE (List as sub items) |  |  |  |  |
ENH: Upgrade Conventional to SMARTZONE® Q327BH | X | N/A | X | N/A | N/A
ENH: TDMA Operation QA00580 (Requires Digital, Smartzone, P25) | X | X | X | X | N/A
ENH: Conventional Vote Scan Q387 | X | X | X | X | X
SYSTEM ENHANCEMENT OPTIONS (List as sub items) |  |  |  |  |
ENH: Radio Packet Data Q947 | Requires Digital | Requires Digital | X | X | X
ENH: Programming Over P25 (OTAP) G996 | Requires Digital | Requires AES | X | X | X
ENH: SMARTZONE® Omnilink (Non-P25) Q173 | N/A | X | N/A | X | X
ENH: P25 9600 Baud Trunking Q361 | N/A | N/A | X | X | N/A
ENH: Enable Internal GPS Operation QA00782 | Requires Digital | Requires Digital | X | X | X
ENCRYPTION ENHANCEMENT OPTIONS (List as sub items) |  |  |  |  |
ADD: Multikey Operation H869 | X | X | X | X | X

Note 1: For feature details, see System Enhancement Software Packages Section under the General Information on the APX 6000Li price page.

A Universal Serial Bus (USB) cable is required to "FLASH" FLASHport® software into the ASTRO®: Digital APX 6000Li radios.

Software Prices BELOW DO NOT include field programming.

### Configuration

####

#### Models

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
TDMA | - | T7813 | 430 | $0.00
9600 OR 3600 SINGLE SYSTEM DIGITAL TRUNKING | - | T7815 | 430 | $0.00
ANALOG CONVENTIONAL | - | T7816 | 430 | $0.00
ANALOG 3600 TRUNKING | - | T7817 | 430 | $0.00
DIGITAL CONVENTIONAL | - | T7818 | 430 | $0.00

#### Options

Operation Mode

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: ANALOG CONVENTIONAL TO ANALOG 3600 TRUNKING | - | QA03214AA | 430 | $1,083.00
ENH: ANALOG CONVENTIONAL TO DIGITAL CONVENTIONAL | - | QA03215AA | 430 | $474.00
ENH: ANALOG CONVENTIONAL TO 9600 OR 3600 DIGITAL TRUNKING | - | QA03216AA | 430 | $1,719.00
ENH: ANALOG 3600 TRUNKING TO 9600 OR 3600 DIGITAL TRUNKING | - | QA03216AB | 430 | $771.00
ENH: DIGITAL CONVENTIONAL TO 9600 OR 3600 DIGITAL TRUNKING | - | QA03216AC | 430 | $1,380.00

System Enhancement Software

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: TDMA OPERATION | Requires Q808/Q806 (Digital), Q327/H38 (Smartzone), and Q361 (P25) to be ordered. A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | QA00580AE | 430 | $609.00
ADD: SITE SELECTABLE ALERT FLP PORTABLE | - | QA00982AC | 430 | $203.00
ADD: DIGITAL TONE SIGNALING | - | QA09000AB | 0430 | $203.00
ADD: GROUP SERVICES FLP | Group Services offers Conventional Alias updates, Trunking Alias updates and Trunking Group Messaging. This option requires G/Q806 for Conventional only capabilities and G/Q361 for any Trunking only capabilities. You can now also do Over the Air Firmware Updates with this feature. (Requires Digital. | QA09008 | 430 | $203.00
ADD: MISSION CRITICAL GEOFENCING FLP | Requires GPS (FL/QA00782). | QA09012AB | 430 | $203.00

Systems Enhancement Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: PROGRAMMING OVER P25 (OTAP) | Requires Digital and IV&D. Compatible with P25 Trunking and Conventional Operation. POP25 requires AES encryption for ASTRO Conventional operation. To do in field POP25 programming must use Advanced System Key (DVN4046A). | G996AX | 430 | $136.00
ENH:TRUNK RADIO TRACE/REM MONI | - | H43BH | 430 | $102.00
ENH: ONE TOUCH BUTTON | - | H46BD | 430 | $102.00
ADD: APX PERSONNEL ACCOUNTABILITY FLP | This feature now also allows the user to use a side button of the radio as a method to transmit the acknowledgement of an Evacuation instead of using PTT button. | Q445AF | 0430 | $203.00
ADD: ASTRO 25 INTEGRATED VOICE & DATA | - | Q947BE | 430 | $338.00
ADD: MISSION CRITICAL WIRELESS BLUETOOTH | - | QA00583AE | 430 | $203.00
ADD: DVRS PSU ACTIVATION APX PORTABLE FLASHPORT | - | QA00631AC | 0430 | $136.00
ENH: APX GPS ACTIVATION | Requires IV&D (Q947) | QA00782AE | 430 | $203.00
ADD: ASK SUPPLEMENTAL DATA FLP | The SOFTWARE KEY is the default Advance System Key option that ships standard on all APX products. You can nolonger order software key QA01749. The HARDWARE KEY QA01648 can be ordered instead. Be sure to enter the CORRECT SYSTEM OWNER ID in the supplemental data. If an INCORRECT ID is entered, a FLASHport order is required to fix the error. | QA01648AC | 430 | $6.00
ADD: SW KEY SUPPLEMENTAL DATA FLP | A SOFTWARE or ADVANCED SYSTEM KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. | QA01749AE | 430 | $0.00
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 Trunking (Q361). | QA01767AV | 430 | $136.00
ENH: ENHANCED ZONE BANK | This option will increase the channel/talkgroup capacity on a Model 1.5 Radio | QA01768AD | 430 | $102.00
ADD: EXTREME NOISE REDUCTION | - | QA01833AF | 430 | $34.00
ADD: MANDOWN OPERATION | APX6000 customers ONLY- with radios using tanapas with revision A or B will also need to order the APX6000 MAN DOWN UPGRADE HW KIT in addition to the Man Down SW flashport option QA01843AB. Please contact your sales representative for further details. | QA01843AB | 430 | $203.00
ADD: ENHANCED DATA | Digital (Q806/G806), Smartzone (H38/G51), IV&D (Q947) and P25 Trunking (Q361/G361) are required when ordering QA03399 (Enhanced Data). | QA03399AB | 430 | $203.00

Algorithm Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: TACTICAL REKEY | Requires IV&D (Q947). includes MULTIKEY. Tactical OTAR is not compatible with DVRs QA00631. | H04AW | 430 | $474.00
ENH: MULTIKEY | - | H869CC | 430 | $446.00

Programming

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: FRONT PANEL PROGRAMMING & CLONING | - | Q53AK | 430 | $203.00

UNDEFINED

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SOFTWARE LICENSE ONLINE DELIVERY | - | UA00083AA | 0430 | $0.00

### Ship Card

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
ASTRO_SUBS_SOFTWARE | US1 | Q445AF | ADD: APX PERSONNEL ACCOUNTABILITY FLP | 0430 |
ASTRO_SUBS_SOFTWARE | US1 | QA00631AC | ADD: DVRS PSU ACTIVATION APX PORTABLE FLASHPORT | 0430 |
ASTRO_SUBS_SOFTWARE | US1 | QA09000AB | ADD: DIGITAL TONE SIGNALING | 0430 |
PORTABLES | SCB | T7813 | TDMA | 430 | 97
PORTABLES | SCB | T7815 | 9600 OR 3600 SINGLE SYSTEM DIGITAL TRUNKING | 430 | 60
PORTABLES | SCB | T7816 | ANALOG CONVENTIONAL | 430 | 7
PORTABLES | SCB | T7817 | ANALOG 3600 TRUNKING | 430 | 8
PORTABLES | SCB | T7818 | DIGITAL CONVENTIONAL | 430 | 3
ASTRO_SUBS_SOFTWARE | US1 | UA00083AA | ADD: SOFTWARE LICENSE ONLINE DELIVERY | 0430 |