Back

##### APX NEXT XN All Band

###### Product Catalog

##### Jump to ...

- APX NEXT™ XN All Band
- Configuration
- Application Services
- Billing Options
- Software and Provisioning
- HazLoc Approved Accessories (UL Div 2) - Not for use in Hazard Zone Mode
- Ship Card

Back

##### APX NEXT XN All Band

### APX NEXT™ XN All Band

·

·

·

·

·

APX NEXT XN Smart Radio is designed with unprecedented durability, ready to operate from day-to-day situations to the most extreme environments. It mobilizes intelligence to bring vital information to your hands for improved collaboration — so you can outperform whatever the unexpected throws at you.

MISSION-CRITICAL DEVICE

You’ve seen tough, but not like this. APX NEXT XN takes toughness to a new level, designed to the latest standards in the fire service. Newly added software features enhance fireground safety and post incident review. Ruggedness and safety is bolstered with our leading APX audio in both the radio and XVN500 RSM, for the most intelligible audio in any environment. And when you need to go beyond voice, you are ultra connected with LTE, GPS, Wi-Fi and Bluetooth.

MOBILE CONNECTION TO INTELLIGENCE

SmartConnect automatically switches between LMR and LTE to extend radio communication beyond the boundaries of the radio system, so users can concentrate on their mission and not worry about coverage.

SmartLocate let’s dispatchers see where everyone under their care is, so they can stay focused on critical situations.

SmartMapping enhances situational awareness by enabling radio users to see their own location on the radio front display, find an address, drop waypoints, and view the locations other colleagues at a glance, then tap the screen to instantly communicate with them.

SmartIncident is a CAD client that gives frontline responders a clear, consolidated view of assignments, unit status updates, map views and multimedia – right on their radio.

SmartMessaging is a secure and convenient way to share texts, images, videos and voice notes across an extended team.

SmartVideo is designed for SVX users to offload critical video to CommandCentral DEMS via the APX NEXT’s LTE. It also allows for users to livestream into CommandCentral Aware via the LTE in APX NEXT.

STREAMLINED OWNERSHIP EXPERIENCE

Radio Central, the cloud based provisioning system, lets you prepare radios before they even arrive and SmartProgramming allows for radio updates to be delivered over broadband regardless of geographic location.

CustomerHub provides direct access to subscriptions, entitlements, warranties and licenses to administer your fleet, and a range of services help you to manage your operations.

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

- New Application service!! SMARTVIDEO is now available on APX NEXT family with the release SR2025.3 .

- ViQi Virtual Partner is no longer orderable for new customers. For existing customer add-on orders, contact Order Management. The ViQi Voice Control (QA09028) option will now be included at $0 when ordering separately.

A new plastic carry holster (PMLN8601) with a 2.5” belt clip (PMLN8602) and a 3.0” (PMLN8603A) belt clip are now available for the APX NEXT XN radio. The Standard Radio configuration will include the plastic carry holster (PMLN8601) with a 2.5” belt clip (PMLN8602).

- Core Bundle includes AES + ADP encryption (Q629), however when selecting Custom Configuration, all U.S. orders will require an encryption selection. Q667 ADP only is now available at $0. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. Please see the encryption section for AES and other encryption options that include ADP.
- WARNING: Radios shipped with QA05751 are not field-upgradable for encryption and any changes will require the units to be sent to a Motorola depot.

- Trunking System Key clarification: Software System Key (QA01749) is the default selection for all APX radios. APX NEXT radios ordered with Software Keys (QA01749), can be programmed with either Software keys, Hardware keys or a combination of Software and Hardware keys. APX NEXT radios ordered with Hardware System Key (QA01648), can only be programmed when all Hardware keys are loaded into RadioCentral. Be certain that you are making the correct selection, based on the type of System Keys that your customer is using, as it CANNOT be changed in the field after the radios ship.

Recommended APX NEXT training classes for new customers:

- APX NEXT Overview ($0) Direct Link to class: AST4002
- APX NEXT Radio Central Overview ($0) Direct Link to class: AST0137
- APX NEXT Features & Service ($0) Direct Link to class: AST4012

Standard Features

All ASTRO Digital APX NEXT™ XN models include the following features:

- All-Band Capability (UHF, VHF, 7/800)

- Front Display: 3.6” TFT Transflective, 24-bit Full Color

- User Interface: Capacitive Touch, immune to false actuation from water, snow, dirt, or grease

- Top Color Display: 1 line of icons, 2 lines of text, 14 characters per line

- 16 Position Mode Rotary Select Switch
- Angled On/Off Volume Knob

- 4 Programmable Side Buttons

- Orange Programmable Button

- Top Mounted Programmable 3 Position Toggle Switch

- 3-Watt Rated Audio

- Wireless Bluetooth® 5.0 (LE) (QA00583)

- LTE (AT&T FirstNet, Verizon, and Bell Mobility Certified)

- IP68 (2 m, 4 hr)

- ADP Privacy - Single Key (Q667)

- Radio Packet Data (Q947)

- Software Key (QA01749)

- GPS Software & Hardware (QA00782)

- Enhanced Zone Bank (QA01768)

- Adaptive Audio Engine

- Dual High Dynamic Range Microphones

- Alias Update over LMR

- One Touch/Status Message (H46)

- Radio Trace/Remote Monitor (H43)

- Data Logging & Self-checks

- Hazard Zone Mode

- Intelligent Noise Reduction (QA010089) with 2025.2 or later release

- ViQi Voice Control

Standard Radio configuration includes the following:

- IMPRES 2 Battery 3400 mAh IP68 UL DIV 2 (PMNN4812)

- NOTE: APX NEXT XN battery is only compatible with NNTN9199 Single Unit Charger and NNTN9115 6-Slot Multi Unit Charger.

- All-Band Flexible Antenna (AN000417A01)

- Side Connector Dust Cover (HW002967A01)

- Plastic Carry Holster (PMLN8601A) with 2.5" Belt Clip (PMLN8602A)

- 12-Pin Interface-to-10-Pin RFDC Adapter (PMKN4262)

APX NEXT XN radios provide customers with a new ownership experience that allows radio configurations to be set up in a cloud hosted RadioCentral programming tool, even before the radios have physically arrived. On first power up, the APX NEXT XN radios will automatically connnect over WiFi or LTE to the RadioCentral cloud database and download the preset codeplug configuration.

Default radio codeplugs are loaded into the customer's specific cloud database called Provisioning Agency, before the radios ship from the Motorola Solutions factory. A Provisioning Agency will automatically be set up for every customer the first time they purchase APX NEXT XN radios.

When an APX NEXT XN radio is first ordered, the email address of the administrator for the Provisioning Agency has to be entered. That person will receive an email from Motorola Solutions inviting him/her to access the RadioCentral portal and set up other users with access to the Provisioning Agency, so they can program radios going forward.

Information that you will need to place an order:

- Name and Email address of the customer's Technical Contact

- Provisioning Agency name (if the customer has multiple)

- Specify End User Type of who will be the users of the radios for FirstNet Service Eligibility verification (US customers only).
Available categories are: Police Protection; Fire Protection; Ambulance or Other (describe in free-form text)

- System ID for the system on which the APX NEXT XN radios will be deployed. If not known, use "FFFF"

If this is the first time you are quoting APX NEXT XN to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX NEXT XN radios and enable the customer system to support the required application services.

#### To ensure accuracy of APX NEXT XN configuration, please create Quotes and Request Orders in CPQ (access through https://motorolasolutions.my.salesforce.com).

### Configuration

1: Base Radio $15,108.42 List $8,309.63 Disc $7,309.63 w/Trade

Every APX NEXT XN radio now ships with the APX NEXT XN MSI 12-PIN INTERFACE-TO-10-PIN RFDC ADAPTER (P/N PMKN4262A) in accordance to the NFPA 1802-2021 Section 6.10.1.1 requirement. The List Price (see table below) for the RFDC ADAPTER should be added to the order for every APX NEXT XN radio.

Description | Full Description | Nomenclature | APC | Price
APX NEXT XN; ALL-BAND MODEL 4.5 PORTABLE | 3.6" Touch Display, All Band (VHF, UHF, 7/800MHz), LTE, WiFi, GPS, BT, IP68 | H55TGU9PW8AN | 0621 | $11,172.00
APX NEXT XN MSI 12-PIN INTERFACE-TO-10-PIN RFDC ADAPTER |  | PMKN4262A | 742 | inc.
ADD: SMARTZONE OPERATION |  | H38DA | 0437 | inc.
ADD: P25 9600 BAUD TRUNKING |  | Q361CD | 0437 | inc.
ADD: ASTRO DIGITAL CAI OPERATION |  | Q806CH | 0437 | inc.
ADD: TDMA OPERATION |  | QA00580BA | 0437 | inc.
ADD: VIQI VC RADIO OPERATION |  | QA09028AA | 0437 | inc.
ADD: ENHANCED DATA |  | QA03399AK | 0437 | inc.
ADD: DVRS PSU ACTIVATION |  | QA00631AL | 0437 | inc.
ADD: PROGRAMMING OVER P25 (OTAP) |  | G996 | 655 | inc.
ADD: HW KEY SUPPLEMENTAL DATA |  | QA01648AA | 0655 | inc.
ADD: CPS ENABLEMENT. |  | QA08853AA | 0437 | inc.
ADD: WIFI CAPABILITY |  | QA09001AM | 0437 | inc.
ADD: OUT OF THE BOX WIFI PROVISIONING |  | QA09007 | 0437 | inc.
ADD: CPS ENABLEMENT. |  | QA08853AA | 0621 | inc.

#### 1a. Remote Speaker Microphone or 12-Pin GCAI Adapter (Required)

APX NEXT XN is tested with the XVN500 RSM as a system to meet the latest standards in the fire service. Only the following versions of XVN500 RSM are available that meet the NFPA 1802-2021 certification requirements when used with the APX NEXT XN radio. The total quantity of either XVN500 RSMs should match the total quantity of APX NEXT XN devices you plan to order and must be entered in the space provided in the CPQ Order Configuration page

Description | Full Description | Nomenclature | APC | Price
XVN500 REMOTE SPEAKER MIC, HIGH IMPACT GREEN WITHOUT KNOB | XVN500 REMOTE SPEAKER MIC IMPACT GREEN WITHOUT KNOB | PMMN4138A | 372 | $775.00
ACCESSORY KIT,XVN500 REMOTE SPEAKER MIC, HIGH IMPACT GREEN WITH KNOB | XVN500 REMOTE SPEAKER MIC IMPACT GREEN WITH KNOB | PMMN4162 | 372 | $871.00

#### Carry Accessory (Optional)

APX NEXT XN ships standard with the PLASTIC HOLSTER (PMLN8601) with 2.5" BELT CLIP (PMLN8602) You may select an alternate carry solution from the list below.

NOTICE: Motorola has certified the APX NEXT XN radio with the carry solutions for NFPA and FCC compliance purposes and are the only carry solutions approved by Motorola for use with the APX NEXT XN radio. Use of non-approved accessories may void the radio’s warranty and may affect continued compliance with NFPA standards and FCC regulations. By selecting “No Carry Solution,” the customer acknowledges receipt of this Notice.

NOTE: A radio strap is not included with the Boston Leather carry solution and must be ordered separately.

Description | Full Description | Nomenclature | APC | Price
ALT: PLASTIC CARRY HOLSTER WITH 3 INCH CLIP | ALT: PLASTIC CARRY HOLSTER WITH 3 INCH CLIP | QA09283AA | 0621 | $0.00
ADD: LEATHER CARRY CASE XN | PMLN8328A - APX NEXT XN BOSTON LEATHER CARRY CASE | QA08852AA | 0621 | $122.00
DEL: DELETE BELT CLIP/BASIC CARRY XE | This option deletes the APX NEXT XN carry holder, PMLN8601, and belt clip. | H301DJ | 0437 | ($10.00)

System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 Trunking (Q361) | QA01767 | 655 | $118.00

Algorithm Types (Required)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

Description | Full Description | Nomenclature | APC | Price
CHIFFRAGE AES | Requires digital operation. P25 CAP Compliant option. Includes ADP. | Q629 | 655 | $523.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | Q667BB | 0430 | $0.00

Multikey Types (Optional)

Description | Full Description | Nomenclature | APC | Price
ENH: MULTIKEY | Required when purchasing more than one encryption algorithm or encryption key? "Requires MultiKey". | H869 | 655 | $363.00
MULTICLE OTAR ASTRO P25 | Includes Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. | Q498 | 655 | $814.00
ADD: MULTI SYSTEM OTAR | Requires Q498 ASTRO 25 OTAR W/ MULTIKEY | QA07680AA | 0655 | $177.00

#### Packaging Selection (Optional)

APX NEXT XN ships standard in Bulk (10 radios per box). Select H842 if you wish to have radios packaged in Individual boxes.

Description | Full Description | Nomenclature | APC | Price
ADD: SINGLE UNIT PACKING | - | H842BT | 0437 | $0.00

#### Factory Configuration (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799BH | 0437 | $12.00

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
RadioManagement (On-Prem) | See “How to Order” section in the below Ordering Guide. | N/A | N/A | N/A

#### Device Management Services (DMS)

Includes hardware repair, tech support, firmware updates and MyView access, with the option to add Accidental Damage. Can select 3, 5 or 7 years of coverage. Ordered per device.

Description | Full Description | Nomenclature | APC | Price
APX NEXT DMS Essential | Provides HW repair, tech support, firmware updates and MyView | LSV01S03446A | 723 | $76.94
APX NEXT DMS Essential with Accidental Damage | Provides accidental damage and HW repair, tech support, firmware updates and MyView | LSV01S03447A | 723 | $150.31

###

###

### Application Services

If this is the first time you are quoting APX NEXT to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX NEXT radios and enable the customer system to support the required application services.

BYOS (Bring Your Own SIM) is an optional new offering where the customer can order APX NEXT or APX N70 without MSI managed LTE service. The limitation is that the customer has to procure their own LTE service from AT&T FirstNet, Verizon (w/ Priority & Preemption), or Bell Canada.

ViQi Virtual Partner and SmartIncident are not available in Canada.

SmartIncident requires SmartLocate and SmartMapping Application Services to be ordered as well.

Refer to the End-to-End ordering guide below for more details.

Description | Nomenclature | Duration | Single App Service | Bundle of 4+ App Svcs | APC
SMARTPROGRAMMING (US Gov) | SSV01S01407A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTCONNECT (US Gov) | SSV01S01406A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTLOCATE (US Gov) | SSV01S01476A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTMESSAGING (US Gov) | SSV01S01906A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTMAPPING (US Gov) | SSV01S01907A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTINCIDENT (US Gov) | SSV01S04311A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTVIDEO (US Gov) | SSV01S05746A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMART PROGRAMMING (FedRAMP) | SWV01S03742A | 1 - 7 years | $166.00 / year | $87.00 / year | 712
SMARTCONNECT (FedRAMP) | SWV01S03743A | 1 - 7 years | $166.00 / year | $87.00 / year | 712
SMARTLOCATE (FedRAMP) | SWV01S03744A | 1 - 7 years | $166.00 / year | $87.00 / year | 712
SMARTMAPPING (FedRAMP) | SWV01S04243A | 1 - 7 years | $166.00 / year | $87.00 / year | 712

#### Application Services (BYOS and/or WiFi)

Description | Nomenclature | Duration | Single App Service | Bundle of 4+ App Svcs | APC
SmartProgramming BYOS/WiFi (US Gov) | SSV01S02190A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartConnect BYOS/WiFi (US Gov) | SSV01S02186A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartLocate BYOS/WiFi (US Gov) | SSV01S02188A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartMapping BYOS/WiFi (US Gov) | SSV01S02242A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartIncident BYOS/WIFI (US Gov) | SSV01S04312A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartMessaging BYOS/WiFi (US Gov) | SSV01S02192A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartVideo BYOS/WiFI (US Gov) | SSV01S05748A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartProgramming BYOS/WiFi (FedRAMP) | SWV01S03745A | 1 - 7 years | $111.00 / year | $87.00 / year | 712
SmartConnect BYOS/WiFi (FedRAMP) | SWV01S03746A | 1 - 7 years | $111.00 / year | $87.00 / year | 712
SmartLocate BYOS/WiFi (FedRAMP) | SWV01S03747A | 1 - 7 years | $111.00 / year | $87.00 / year | 712
SmartMapping BYOS/WiFi (FedRAMP) | SWV01S04244A | 1 - 7 years | $111.00 / year | $87.00 / year | 712

#### Application Services Add-On for Fielded APX NEXT Devices

If a customer wishes to add application services to their existing Service Contract for fielded APX NEXT devices, please engage with your APX NEXT App Service Inside Sales representative found here who will assist with submitting the add-on request.

#### Please refer to the End-to-End ordering guides below to see all components required to enable Application Services.

- SmartConnect
- SmartLocate
- SmartMessaging
- SmartMapping
- SmartIncident
- SmartVideo

### Billing Options

Service Activation Delay

To accomodate the lead time sometimes required for new system deployments and radio configuration, customers may elect to delay the start of the Application Services and Device Managed Services contracts.

Service Activation Delay is available for 30 days after the shipment of radios.

Billing Options

Device purchases are invoiced at the time of shipment.

Service billing options are: Immediate, Annually, Monthly in Arrears (Federal only)

### Software and Provisioning

APX NEXT™ XN Out of the Box Provisioning

RadioCentral™ Factory default codeplugs for all APX NEXT XN radios will be made available to you in a secure cloud application. Motorola Solutions will set up a default account for your agency upon initial device purchase and invite you by email to access MyView (https://myview.motorolasolutions.com) to set up user accounts and download the RadioCentral programming application client.

If you already have an existing log-in for Motorola Command Central, you can use the same credentials to access RadioCentral via https://radiocentral.motorolasolutions.com. If this is the 1st time you will receive an email from Motorola how to set up your initial account.

Follow these steps after your RadioCentral account is activated:

1- Log into RadioCentral. Use the CommandCentral credentials to login RadioCentral URL. You will see the factory default codeplugs for your recently purchased APX NEXT radios

2- Install the R35.00.00 or later CPS on the computer you would like to access RadioCentral. CPS will be utilized as template editor during the Edit/Publish flow in RadioCentral.

3- Build new codeplug or reuse a legacy APX codeplug using RadioCentral. You can pick a proper base factory default codeplug to launch CPS editor, and then launch another CPS to open the reference APX legacy codeplug to drag/drop/copy/paste to reuse whatever configurations to build a new codeplug for your NEXT/N70 radios.

4- Schedule a programming job. Apply the radio configuration to your devices.NOTE: To assure proper device deployment please ensure that your organization has received the radios before scheduling specific programming jobs.

5- Remove the radio from the box, insert a battery and turn on the radio.

APX NEXT XN radios are enabled with LTE service and preset with default Wi-Fi SSID, to wirelessly download radio configurations and updates.

a.Upon power up, the radio will scan for the "Customer1" Network SSID access point with WPA/WPA2 security password of "MotorolaSolutions".

b.If "Customer1" is found, the radio will connect to secure hosted RadioCentral database and download any scheduled configuration. NOTE: Wi-Fi must be connected to the open Internet. If using a firewall, open port 443 for radio programming traffic.

c.If "Customer1" access point cannot be found, the radio will attempt to connect to LTE.

d.LTE connections are open to the internet by default, so if the radio is in LTE coverage, it will connect to secure RadioCentral database and download any pending configuration.

e.If neither Wi-Fi nor LTE is found, the radio will continue scanning for a broadband connection.

For security reasons, it is recommended that the first radio configuration update over "Customer1" access point would remove all default SSIDs and replace them with an agency secure network SSID and password.

For assistance, please call 800-MSI-HELP (800-674-4375).

Special Note for United States - State & Local Markets Only
In accordance with FCC mandate, the APX NEXT XN is restricted to12.5 KHz operation only and does NOT support 25 KHz in the VHF and UHF Bands (excluding T-Band). This applies to customers under Rule Part 90. Customers with FCC waivers can contact their Business Development Representative.

The following LMR features are not supported in APX NEXT XN at this time

H02 | TACTICAL RADIO STW-STUN/KILL
QA09012 | MISSION CRITICAL GEOFENCING
QA00982 | SITE SELECTABLE ALERT FOR P25 TRUNKING
QA09008 | GROUP SERVICES OPTION IS OBSOLETE FOR APX. (The device firmware download is only available through SmartProgramming for APX NEXT. OTA Alias Updates and LMR Group Texting are included in standard configuration)
Display Color Change on channel change |
Transmit Inhibit |
Tactical Inhibit Stun/Kill for Portable (Encode & Decode) |
Phone Encode / Decode (Call/Notification) |
LMR Phone Call from Contacts |
Dynamic ID |
Operational Message |
Inactivity timer for overlay |
Responder Alert -Sensor Hub |
Responder Alert Enhanced Data Delivery |
Responder Alert- Local User, Low Batt and Taser Holder |
Responder Alert - Weapon Fired |
Responder Alert - Vest Piercing via Emergency |
Cached Event Tag upon Reconnect |
Conventional RSSI |
Radio Lock, Change Password, Secure Auto Log-on |

### Self-Quieting Spurs

7/800 MHz | 7/800 MHz | VHF | VHF | UHF | UHF
Radio Alone | Radio + XVN500 RSM | Radio Alone | Radio + XVN500 RSM | Radio Alone | Radio + XVN500 RSM
- | - | 136.8625 | 138.5125 | 410.4 | 410.4
- |  | 138.5 | 172.8 | 441.6 | 415.55
- |  |  |  | 456 | 467.4875
- |  |  |  | 467.4875 | 480
- |  |  |  | 480 | 501.6
- |  |  |  | 501.6 | 518.4
- |  |  |  | 518.4 |

### HazLoc Approved Accessories (UL Div 2) - Not for use in Hazard Zone Mode

This information is subject to change. For the latest information on accessories approved for HazLoc environments, please refer to the UL manuals and addendums that ship with every HazLoc approved APX NEXT XN radio.

Audio Accessories | Model
ACCESSORY KIT,SMART 2 WIRE W/TRANS TUBE BLACK | PMLN6129A
ACCESSORY KIT,SMART 2 WIRE W/TRANS TUBE BIEGE | PMLN6130A
ACCESSORY KIT,IMPRES 2 WIRE SURVEILLANCE BLACK | PMLN6127A

### Compatible RSM but not for use in Hazard Zone Mode

Remote Speaker Microphones | Model
XVE500 REMOTE SPEAKER MIC, HIGH IMPACT GREEN WITH KNOB | PMMN4132A
XVE500 REMOTE SPEAKER MICROPHONE, BLACK WITH KNOB | PMMN4132ABLK
XVE500 REMOTE SPEAKER MICROPHONE, HIGH IMPACT GREEN, NO CHANNEL KNOB | PMMN4137A
XVE500 REMOTE SPEAKER MICROPHONE, BLACK, NO CHANNEL KNOB | PMMN4137ABLK
XE500 REMOTE SPEAKER MIC, HIGH IMPACT GREEN, WITH CHANNEL KNOB | PMMN4106D
XE500 REMOTE SPKR MIC WITH CHANNEL KNOB, HIGH IMPACT BLACK | PMMN4106CBLK
XE500 REMOTE SPKR MIC WITHOUT CHANNEL KNOB, HIGH IMPACT GREEN | PMMN4107C
XE500 REMOTE SPKR MIC WITHOUT CHANNEL KNOB, BLACK | PMMN4107BBLK