Back

##### Pop25_for_trunking_and_conventional

###### Product Catalog

##### Jump to ...

- Model
- Ordering Information
- Ship Card

Back

##### Pop25_for_trunking_and_conventional

### Model

Programming Over P25 (POP25)
for ASTRO® 25 Trunking
Integrated Voice & Data (IV&D) Systems

### Ordering Information

#### General Information

Motorola's POP25 solution is a feature that is offered on the ASTRO 25 Trunking and Conventional Integrated Voice & Data (IV&D) System. The POP25 feature allows a customer to configure a radio remotely from his/her enterprise network by sending a sequence of commands over-the-air via the ASTRO 25 IV&D system. It is expected that POP25 will significantly reduce the operational costs of IV&D radios by configuring personalities, talkgroups, channels, sites, etc in a radio without physically touching the radio. POP25 can update a radio that is available anywhere within the coverage area of the radio's home system.

System Components:

The POP25 Solution consists of the following components:

1. ASTRO 25 Integrated Voice & Data (IV&D) System: The POP25 solution uses the ASTRO 25 IV&D system's data pipe to transport the radio configuration information.

2. Compatible POP25 XTS & XTL Subscribers: POP25 will initially be supported on the XTS/XTL 5000 and XTS/XTL 2500. This feature is also supported on the XTS/XTL 1500. The Packet Data and POP25 options must be enabled in the subscriber radio to allow POP25 capability.

3. CPS: The latest version of CPS (R09.00.00 or later) must be running on a PC in the customer network. For Conventional systems CPS version R12.00.00 or later is required.

4. Advanced System Key: The Advanced System Key is a physical hardware key that grants access to the POP25 feature. It is connected to a parallel port or USB port of the PC running the Customer Programming Software (CPS). The CPS will verify the proper key is attached before every read, write, and clone operation.

5. ASTRO 25 Presence Notifier Application: The ASTRO Presence Notifier Application provides the presence, absence, and routing information of two-way portable and mobile subscriber radios to any compatible data applications located in the Customer Enterprise Network (CEN). It interfaces with data applications and subscriber radios using User Datagram Protocol / Internet Protocol (UDP/IP).

Refer to the Presence Notifier Services document for more information which can be obtained here.

#### Ordering Instructions

These pages will lead you through the necessary ordering steps required to enable POP25 on an ASTRO 25 Trunking IV&D System.

NOTE: The information provided is from a system level. Provided below is the MINIMUM system compatibility requirements. For more product level details, please refer to each of the individual product pages.

ASTRO 25 IV&D System (REQUIRED) The POP25 feature uses the ASTRO 25 Trunking IV&D system's data pipe to transport the messaging information. For ASTRO 25 IV&D Systems, a Data Infrastructure is REQUIRED, some of components include, but are not limited to the following:
Trunking | Conventional
Packet Data Gateway (PDG) | Radio Network Controller (RNC)
GSM Gateway Support Node (GGSN) | Wireless Network Gateway (WNG)

ASTRO 25 Portable and Mobile Subscribers- UPFRONT The POP25 feature is available on select ASTRO 25 portable two-way and mobile subscriber radios and MUST have Customer Programming Software (CPS) and Radio Software Version R09.00.00 or later for trunking IV&D systems and Radio Software Version R12.00.00 or later for Conventional IV&D systems. STEP 1: Order the XTS 5000/2500/1500 Portable Radio(s). Click on the links below to be redirected to the XTS 5000/2500/1500 price pages. · ASTRO Digital XTS 2500 700/800MHz · ASTRO Digital XTS 2500 VHF · ASTRO Digital XTS 2500 UHF · ASTRO Digital XTS 5000 UHF · ASTRO Digital XTS 5000 VHF · ASTRO Digital XTS 5000 700/800MHz · ASTRO Digital XTS 1500 900MHz · ASTRO Digital XTS 1500 700/800MHz · ASTRO Digital XTS 1500 VHF · ASTRO Digital XTS 1500 UHF NOTE: - POP25 is supported on all XTS 5000/2500/1500 models ( I / 1.5 / II / III) - XTS 1500 does not support POP25 capability on Conventional systems - REQUIRED to order ASTRO Digital CAI Operation (Q806), SmartZone Operation (H38) - REQUIRED to order for XTS 5000 is ASTRO Project 25 Trunking Software Enhancement (Q361) - REQUIRED to order for XTS 2500/1500 is ASTRO Project 25 Trunking Software (Q574) - REQUIRED to order Packet Data Interface (Q947) - REQUIRED to order POP25 Capability (G996) to enable the POP25 feature - REQUIRED to order encryption for Conventional IV&D systems, not required for Trunking systems. - ADP encryption is not supported for POP25 operation on conventional systems. Order the XTL 5000/2500/1500 Mobile Radio(s). Click on the links below to be redirected to the XTL 2500/5000/1500 price pages. · ASTRO Digital XTL 2500 700/800MHz · ASTRO Digital XTL 2500 UHF R1 Mid Power · ASTRO Digital XTL 2500 UHF R2 Mid Power · ASTRO Digital XTL 2500 VHF Mid Power · ASTRO Digital XTL 2500 UHF R1 High Power · ASTRO Digital XTL 2500 VHF High Power · ASTRO Digital XTL 5000 O5/O3 Control Head Mobiles · ASTRO Digital XTL 5000 W 3/4/5/7/9 Control Head Mobiles · ASTRO Digital XTL 1500 700/800MHz · ASTRO Digital XTL 1500 UHF R1 Mid Power · ASTRO Digital XTL 1500 UHF R2 Mid Power · ASTRO Digital XTL 1500 VHF Mid Power NOTE: - POP25 is supported on all XTL 5000/2500/1500 models -XTL 1500 does not support POP25 capability on Conventional systems. - REQUIRED to order for XTL 5000/2500 is ASTRO Digital CAI Operation (G806); SmartZone Operation (G51), and ASTRO Project 25 Trunking Software Enhancement (G361) - REQUIRED to order for XTL 5000/2500 Packet Data Interface (Q947) - REQUIRED to order for XTL 1500 is the 9600 ASTRO DIGITAL ENHANCED package (G964) which includes the Packet Data Interface functionality - REQUIRED to order POP25 Capability (Q996) to enable the POP25 feature - REQUIRED to order encryption for Conventional IV&D systems, not required for Trunking systems. - ADP encryption is not supported for POP25 operation on conventional systems

ASTRO 25 Portable and Mobile Subscribers - Fielded Upgrades Requirements for UPGRADING an existing mobiles and portables to support POP25 STEP 2: If adding POP25 to an XTS/XTL 5000/2500 radio that already exists in the field, click on the below links to be redirected to the FLASHport Aftermarket Upgrade price pages. NOTE: - The upgrade to add POP25 (G996) is software ONLY. - The subscriber is required to have ASTRO 25 Trunking IV&D and Packet Data capability. If not, the subscriber needs to be updated to include this functionality. PORTABLES · ASTRO Digital XTS 5000 FLASHport Upgrade · ASTRO Digital XTS 2500 FLASHport Upgrade · ASTRO Digital XTS 1500 FLASHport Upgrade MOBILES · ASTRO Digital XTL 5000 FLASHport Upgrade · ASTRO Digital XTL 2500 FLASHport Upgrade · ASTRO Digital XTL 1500 FLASHport Upgrade

Advanced System Key The Advanced System Key is a physical hardware key that grants access to the POP25 feature. It is connected to a parallel port or USB port of the PC running the Customer Programming Software (CPS). The CPS will verify the proper key is attached before every read, write, and clone operation. For more information on the Advanced System Key refer to the following presentation. STEP 3: Order the Advanced System Key kit using the ASK price page.

ASTRO 25 Presence Notifier Application The ASTRO Presence Notifier Application provides the presence, absence, and routing information of two-way portable and mobile subscriber radios to any compatible data applications located in the Customer Enterprise Network (CEN). STEP 4: Order the Presence Notifier using the Presence Notifier price page.

#### Manuals

When ordering QUANTAR FLASHport Upgrades use one the following model numbers:

- SQM01SUM0130 Software & Hardware Upgrades
- T6693 Software Only Upgrades

More information on these model numbers can be found in the following eCat Price Pages:

- Main folder: Software Upgrades & FLASHport
- Infrastructure FLASHport Upgrades Folder
- QUANTAR Software & Hardware Upgrade Folder
- Software Upgrades/FLASHport
- Software & Hardware Upgrades/FLASHport

For copies of the User Guides and Manuals associated with POP25, visit Motorola Online and download the appropriate documents.

Downloading instructions:

Ø Go to Motorola Online https://motonline.mot.com/Login.aspx

ü Select Resource Center from the Top Panel

Ø Click on Resource Center

Ø Search for a User Guide and/or Manual from the list:

· ASTRO® 25 Presence Notifier Application User Guide (6880309S69)

### Ship Card

Data Not Available

####