Back

##### APX 6000 UHF

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Software and Services
- Ship Card

Back

##### APX 6000 UHF

### Model

APX™ 6000 P25 Portable Radio
UHF Range 1
UHF Range 2
P25 Phase 2 Single Band Capable Radio

### Updates

#### Special Note for United States - State & Local Markets only:

In accordance to a FCC mandate, VHF (150-174 MHz) and UHF (421- 450 MHz) products operating on Part 90 frequencies will be restricted to 12.5 kHz or narrower operations on Jan. 1, 2013.

#### Announcements

DHS

Project 25 Compliance Assessment Program (CAP) has defined a "CAP Encryption Requirements compliant radio" as a radio that can be ordered without encryption or one that can be ordered with AES256. << Click to learn more>>

Please note the APX 6000 Legacy (AN) Models are no longer available. Please see the BN models listed below.

Effective October 2016, if H499 is selected, the standard battery is PMNN4485A.

In August 2016, the APX 6000 evolved to support newer technologies like Wi-Fi, Adaptive Audio Engine, Bluetooth ® 4.0 wireless technology, and IMPRES 2 Batteries.

Please review the new ordering process for the enhanced APX 6000 VHF models. The enhanced APX 6000 VHF models must use these model numbers:

H98UCD9PW5BN

H98UCF9PW6BN

H98UCH9PW7BN

Please note the new APX 6000 models will not share the same codeplugs as the previous APX 6000 models (H98UCD9PW5AN, H98UCF9PW6AN, H98UCH9PW7AN). Direct cloning will not be available. New features, such as Wi-Fi, Bluetooth 4.0, and the Adaptive Audio Engine will not be available as a FLASHport upgrade on the previous APX6000 models (H98UCD9PW5AN, H98UCF9PW6AN, H98UCH9PW7AN).

IMPRES 2 Battery Information
Effective August 2016, IMPRES 2 Batteries are available on all APX 6000 models. Previous IMPRES batteries offered with the APX 6000 will no longer be orderable, but they will still operate. IMPRES 2 batteries offer an increase in capacity with no increase in size. With IMPRES 2 batteries and chargers, you can charge your batteries up to two times faster, and they can be recharged 60 percent more times than with a traditional Li-Ion battery, extending the life of your battery. Gaining the benefits of this IMPRES 2 technology requires both IMPRES 2 batteries and IMPRES 2 chargers. The APX 6000 will now come standard with the PMNN4485 Slim IMPRES 2 Li-Ion 2550MaH battery. Please see below for additional IMPRES 2 battery options available for the APX 6000.

Effective Feb. 22, 2016, APX 6000 Radio Sales Model Price will increase by $150.

Effective Feb. 22, 2016, the APX 6000 will ship standard with GPS Activation (QA00782). GPS requires Q947 (already included standard) and Q806 (digital) in order to operate.

Effective Feb. 1, 2016, for user guides, manuals and other product information, please visit motorolasolutions.com and search for this product using the name or manual number. To add a manual, please order H88.

Effective Jan. 1, 2016, Factory Mutual (FM) Certification is no longer available.

Effective Jan. 1, 2016 the three-year Service from the Start (SfS) Lite option must be selected when ordering an APX 7000/7500, APX 6000/6500, SRX or APX 8000/XE device. This is the minimum requirement under the new warranty enhancement initiative. This rule does not apply for the APX4500/4000, APX3000, and APX1500/1000.

Effective February 2015, APX 6000 now ships standard with Radio Packet Data (Q/W947), Mission Critical Bluetooth (QA00583), and Software Key (QA01749).

### Ordering Information

Ordering Guide

#### Features

All APX 6000 P25 Portable Radio models include the following features:

- Dual microphone
- 0.5 watt rated audio
- Integrated GPS hardware capable*
- Mission-critical wireless Bluetooth® 4.0 (LE)¹
- Integrated mission-critical wireless Bluetooth (Hardware/Software)
- Detachable belt clip for top display model
- Li-ion 2550mAh IMPRES 2 Battery (PMNN4485), on all models Aug. 1, 2016
- Antenna (dependent on frequency band and type)
- Intelligent lighting
- IP68 ships standard with every radio model¹
  Adaptive audio engine (includes extreme one-sided noise reduction)*¹
- 3 watt rated audio*¹

- Three programmable side buttons
- Orange programmable button
- 16-position mode rotary select switch
- Wi-Fi® 802.11 b/g/n*¹
- Angled on/off volume knob
- Low battery alert tone
- Noise cancellation software
- One top-mounted programmable three-position toggle switch
- Top display: one line of text, one line of icons, zero menu lines (8 characters)
- Advanced Digital Privacy (ADP) hardware/ software encryption ships standard w/ single key
- Emergency Find Me¹

APX 6000 P25 Portable Radio Limited Keypad and Full Keypad with Dual Display Model also includes:

- Universal carry holder
- Unified call list
- Front color display: four lines of text, two lines of icon (14 characters)

- Radio profiles
- Full keypad: 4x3 alphanumeric 3 programmable button, four-way navigation, home and data buttons

*Must purchase Software to ENABLE.

¹Features only available on the following models (Ship Acceptance August 6th, 2016): H98KGD9PW5BN, H98KGF9PW6BN, H98KGH9PW7BN

New RFID enabled volume knobs (QA04526) available for portable radios. See RFID Enabled Volume Knob section below for more information. See RFID Solution Partner link below for information on partners that can provide customers with scanner hardware and back end asset management solutions.

All APX 6000 P25 Portable Radios are part of the FLASHport® program and ship standard with a FLASH EE Prom, which allows for feature and system upgrades (contingent upon remaining within the current RF capabilities of the radio)

****NOTE: APX Portable and Mobile Radios ship standard with the Software Key (QA01749). The Hardware Key (QA01648) is available as an alternative option to purchase. The System ID is required to be entered as supplemental data when ordering the Hardware Key (QA01648). It is CRITICAL that the CORRECT SYSTEM ID is entered when placing the order as this will impact the radios’ ability to operate on the intended system. If an incorrect System ID is entered, a FLASHport upgrade will be required in order to fix this error. The Master Key Start-Up Kit (DVN4046) is required to use the Hardware Key (QA01648) or to operate on a third-party trunking system if the customer does not already possess one, or if theirs has expired. Please CLICK HERE for further details regarding the DVN4046 Kit.

ASK (Advanced System Key)

#### General Information

Operating Modes

APX 6000 P25 Portable Radio Models are capable of operating in FOUR different voice communication modes:

1. Normal analog (clear voice)
2. 3.6 kB ASTRO digital (both clear and coded voice)
3. 9.6 kB ASTRO 25 digital (both clear and coded voice)
4. 9.6 kB 12.5kHz two-slot digital TDMA (both clear and coded voice)

TDMA
FDMA (Frequency Division Multiple Access) is a proven technology that is widely used today in radio systems and is part of Project 25 Phase 1 standard. FDMA carries one call per channel. TDMA (Time Division Multiple Access) is part of P25 Phase 2 standard and provides double the voice capacity as 2 calls can share 1 channel. Customers can add more users to their systems without the need of additional frequencies or infrastructure. The APX radios support both P25 Phase 1 and TDMA technologies seamlessly. Using Motorola's unique Dynamic Dual Mode (DDM) capability, the radios dynamically switch between FDMA and TDMA without the user having to change channels. This provides interoperability on demand with existing and future networks.

Please note: TDMA X2 is not supported on the APX6000

#### New to APX6000 Models

Wi-Fi

APX 6000 supports Wi-Fi 802.11 b/g/n with WPA2/WPA (PSK), and WEP security protocols. Wi-Fi can be used with the Radio Management SW in order to do codeplug updates, firmware refreshes, and FLASHport upgrades over a Wireless Network (WLAN). The radio will only connect to available Wi-Fi networks which have been pre-provisioned in the radio codeplug via CPS. The radio can be pre-provisioned with up to 20 SSIDs.
The Wi-Fi feature requires ordering option QA09001. The Wi-Fi feature is also available aftermarket as a FLASHport upgrade if not ordered out of the factory.

Radio Management (RM) is required in order to take advantage of the Wi-Fi capabilities on APX 6000.

Out-of-the-box Wi-Fi Provisioning
If a radio is ordered the Wi-Fi option (QA09001) and the customer wishes to provision the radios out of the box using Wi-Fi, the radio must also be ordered with the Out of the Box Wi-Fi Provisioning option (QA09007).
A radio ordered with the Wi-Fi option and the Out of the Box Provisioning over Wi-Fi option will come with the following default codeplug configuration relative to Wi-Fi:
a. Wi-Fi will be enabled.
b. There will be one pre-configured network with the Network SSID set to “MyNetwork” and security type will be set to “None”.
c. The default state of Wi-Fi will be “on”.
A Wi-Fi router is required for connecting the Wi-Fi capable radio to the Device Programmer. The Wi-Fi router is to be procured by the agency programming the radios and must be provisioned with the Network SSID set to “MyNetwork” (case sensitive) with no password enabled.

For more details regarding the Out of the Box Wi-Fi Provisioning process, please refer to the Out of the Box Wi-Fi Provisioning Leaflet.

Bluetooth 4.0 & Emergency Find Me
With Bluetooth 4.0 wireless technology and our APX™ Mission Critical Wireless portfolio, users can now connect a variety of Bluetooth audio accessories and data devices with their APX™ radio.

Bluetooth 4.0 also enables Emergency Find Me, a feature providing personnel with an added level of security by improving response time in emergencies. Once an emergency is activated on the APX 6000, a Bluetooth beacon signals other Bluetooth-enabled APX radios within range. Based on bluetooth signal strength, nearby APX radios will receive an emergency alert via intelligent lighting and a text message with users Radio ID along with signal strength status (excellent, poor, fair) to determine proximity, and will guide the nearest personnel to the user in distress.

Adaptive Audio Engine
By selecting QA09006, the Adaptive Audio Engine option, the APX 6000 is equipped with a 3-watt speaker, 3 integrated microphones and the Adaptive Audio Engine. This changes the level of noise suppression, microphone gain, windporting and speaker equalization to produce clear and loud audio in any environment. QA09006 must be ordered in order to receive this feature.

IMPRES 2
Effective August 2016, the APX6000 comes standard with Q712AY, PMNN4485 SLIM IMPRES 2 LIION 2550MAH battery. Please see below for additional IMPRES 2 Battery Options available for the APX6000. The benefits of this IMPRES 2 technology requires both IMPRES 2 Batteries & IMPRES 2 Chargers. Please see the Accessories Catalog and Accessories ECAT pages for more information on IMPRES 2 technology.

Please note: QA01837 (NNTN7038), QA02021 (PMNN4403), QA00781 (NNTN7034), H335 (NNTN7037), QA02726 (NNTN7573) and Q393 (NNTN7036) are no longer be available on the APX6000.

RUGGED

The RUGGED option (H499JX) is ordered with APX 6000 Enhanced Model Numbers will now meet MIL-STD 512.X/I, IP68 submersion standards for 2 meters for 4 hours. Effective October, 2016, if H499 is selected, the standard battery is still PMNN4485A. If HAZLOC certification is required, please see the HAZLOC battery options below. The following APX6000 batteries are tested for Delta-T/Rugged standards when H499 is ordered: PMNN4485, PMNN4486, PMNN4487, PMNN4494A, NNTN8930, NNTN8921.

#### FLASHport AFTERMARKET UPGRADES

**PLEASE NOTE: The new APX6000 models will not share the same codeplugs as the previous APX6000 models (H98UCD9PW5AN, H98UCF9PW6AN, H98UCH9PW7AN). Direct cloning will not be available. New features, such as Wi-Fi, Bluetooth 4.0, and the Adaptive Audio Engine will not be available as a FLASHport upgrade on the previous APX6000 models (H98UCD9PW5AN, H98UCF9PW6AN, H98UCH9PW7AN).**

The APX 6000 P25 Portable Radios are part of the FLASHport Program. This means that APX 6000 hardware models can be loaded with different software packages that provide the features and functionalities that our customers require.

System Enhancement Options can be loaded at the time of radio purchase or at a later date through the use of software field upgrades (a USB cable is required for all software upgrades.) The APX 6000 portable can be upgraded electronically in the field with new features in the current system or to new systems operation (contingent upon remaining within the same RF sub-band) by ordering upgrade kits.

A new way to upgrade radios in the field launched in early 2015. The previous method, which makes use of the FLASHport USB dongle, will be supported, but for those looking for a more convenient way, a new online method will be supported in Radio Management (RM). For more information, please select APX 6000/APX 6000XE FLASHport in the pulldown select list above.

#### RADIO MANAGEMENT

Radio Management (RM) is a suite of software applications shipping with the APX Customer Programming Software (CPS) that provides the ability to manage your entire fleet of ASTRO APX radios through one central database.

Radio Management (RM) can help reduce fleet programming time and improve overall radio asset management. Radio Management allows:

- Manage and track radio codeplugs through a central database
- Make changes to a shared codeplug template and push to multiple radios
- Manage and update radios without taking them out of service
- Schedule programming updates to radios ahead of time

Note: Radio Management is available only with Customer Programming Software Release 7.12, version R08.02.00 and later and can only be used with ASTRO® Digital APX radios. For more details regarding Radio Management and the Ordering Process, please refer to the ASTRO Radio Management page.

#### FCC Information

#### H98QDD9PW5BN, H98QDF9PW6BN, H98QDH9PW7BN, H98SDD9PW5BN, H98SDF9PW6BN, H98SDH9PW7BN Model Information

Band/Model | Power Output | Transmitter Certification | Emissions | Applicable Rules
--- | --- | --- | --- | ---
UHF Range 1 (380-470 MHz) | 1-5W | AZ489FT7077 | 11K0F3E, 16K0F3E, *k10F1D, 8K10F1E, 8K10F1W | 90
UHF Range 2 (450-520 MHz) | 1-5W | AZ489FT7085 | 11K0F3E, 8K10F1D, 8K10F1E, 8K10F1W | 90

The FCC is mandating all Public Safety and Industrial/Business licensees convert existing 25 kHz efficiency operations in the VHF and UHF bands to minimum 12.5 kHz efficiency analog or digital operation, and that going forward they implement no more 25 kHz efficiency systems. To implement this mandate, the FCC developed rules and deadlines that impact both radio users and equipment providers.

APX 6000 Enhanced Two-way Radio Specifications Sheet
Enhancement Level Reference Guide
ASTRO 25 Subscriber At A Glance Brochure

RSA Comprehensive

RSA
Portable Accessories Catalog
PSM User Guide

Radio Applications \ Advanced System Key
Fleet Management Ordering Guide
Fleet Management Program Download Information
RFID Solution Partner Information

Fleet Management software was previously distributed on DVDs shipped out of Elgin. It is now downloadable from motsolutions.com at the link below. Look at the right edge of the page under Resources Spotlight. The first link is the Order Guide which tells you what you need. The second link is a free trial version that they can download and evaluate free for 90 days. The third link is the actual program. You need to purchase a license to use it (explained in the order guide).

Accessories for APX 6000 can now be found in the select list pulldown above.

### Configuration

####

#### Models

1: Main Model (Must Select One)

PLEASE NOTE: The APX6000 Legacy (AN) Models models are no longer available. Please see the BN models listed below.

Ship Acceptance Received August, 2016. New Features Only Available on the Models Below.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
APX6000 UHF R1 MODEL 1.5 PORTABLE | - | H98QDD9PW5BN | 481 | $3,506.00
APX6000 UHF R1 MODEL 2.5 PORTABLE | - | H98QDF9PW6BN | 481 | $3,924.00
APX6000 UHF R1 MODEL 3.5 PORTABLE | - | H98QDH9PW7BN | 481 | $4,479.00
APX6000 UHFR2 MODEL 1.5 PORTABLE | - | H98SDD9PW5BN | 481 | $3,506.00
APX6000 UHF R2 MODEL 2.5 PORTABLE | - | H98SDF9PW6BN | 481 | $3,924.00
APX6000 UHF R2 MODEL 3.5 PORTABLE | - | H98SDH9PW7BN | 481 | $4,479.00

#### Options

2: Operation Mode (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANALOG OPERATION | Requires either a H35, H37, or H38 | Q241 | 481 | $0.00
ADD: ASTRO DIGITAL CAI OPERATION | Requires either a H35, H37, or H38 | Q806 | 481 | $607.00

3: System Enhancement Software (Refer to ordering guide for help)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: CONVENTIONAL OPERATION | - | H35 | 481 | $589.00
ADD: SMARTZONE OPERATION | A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | H38 | 481 | $1,412.00
ADD: SMARTZONE OMNILINK | Requires H38 SmartZone and Q806 Digital Operation (required for 3600 baud only trunked systems.) APX 6000 digital radios require Advanced System Keys (ASK - DVN4046A) to be configured to operate on a trunking system. | Q173 | 481 | $0.00
ADD: P25 9600 BAUD TRUNKING | Requires H38 and Q806. INCLUDED at 'NO Charge' Q173-OminLink. APX 6000 digital radios require Advanced System Keys (ASK- DVN4046A) to be configured to operate on a trunking system. | Q361 | 481 | $353.00

4: System Key Software

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: HW KEY SUPPLEMENTAL DATA | The SOFTWARE KEY is the default Advance System Key option that ships standard on all APX products. You cannot order software key QA01749. The HARDWARE KEY QA01648 can be ordered instead. Be sure to enter the CORRECT SYSTEM OWNER ID in the supplemental data. If an INCORRECT ID is entered, a FLASHport order is required to fix the error. Order HARDWARE KEY (QA01648) if required to operate/program on a trunking system. Not compatible with conventional. | QA01648AA | 0655 | $6.42

5: System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 Trunking (Q361) | QA01767 | 481 | $118.00
ADD: TDMA OPERATION | For APX6000 and APX6000XE, QA00580 requires Q806, H38, Q361. If ordering an APX6000Li, QA00580 requires QA02756. A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | QA00580 | 481 | $530.00
ADD: PROGRAMMING OVER P25 (OTAP) | Requires Digital and IV&D. Compatible with P25 Trunking and Conventional Operation. POP25 requires AES encryption for ASTRO Conventional operation. To do in field POP25 programming must use Advanced System Key (DVN4046A). | G996AU | 0481 | $118.00
ADD: MULTICAST VOTING SCAN | - | Q387 | 481 | $235.00
ADD: ENHANCED DATA APX | Digital (Q806/G806), Smartzone (H38/G51), IV&D (Q947) and P25 Trunking (Q361/G361) are required when ordering QA03399 (Enhanced Data) | QA03399 | 656 | $177.00
ADD: DVRS PSU ACTIVATION | Enables DVRS Enhanced PSU functionality on APX Mobile Radios. Requires Digital Operation. QA00631 is to be ordered for radios that are not connected directly to a DVR. If you are connecting your radio directly to a DVR then order GA00631. | QA00631 | 655 | $118.00
ENH: RADIO TRACE/ REMOTE MONITOR | Requires Q806 and either H37, H38, or H35. | H43 | 481 | $83.00
ENH: ONE TOUCH/STATUS MSG | Compatible on models 1.5, 2.5 and 3.5. | H46 | 481 | $83.00
ADD: FRONT PANEL PROGRAMMING & CLONING | Compatible with Model 3.5 Radios only. Requires FPP HW dongle (NNTN7526A)to be purchased. | Q53 | 481 | $165.00
ADD: FRONT PANEL PROGRAMMING & CLONING (FEDERAL) | Compatible with Model 3.5 Radios only. | Q52 | 481 | $165.00
ADD: SITE SELECTABLE ALERT FOR P25 TRUNKING | - | QA00982 | 656 | $165.00
ADD: MISSION CRITICAL GEOFENCING | Requires GPS (QA00782). | QA09012 | 426 | $177.00
ADD: DIGITAL TONE SIGNALING | - | QA09000 | 656 | $177.00
SOFTWARE LICENSE ENH: ENHANCEMENT LEVEL 2 | Model 1.5 Radios require Enhanced Zone Bank to be ordered so additional channels can be accessed. Please reference the Enhancement Level Reference Guide for more details. This option allows for a few parameters (ZONES, CHANNELS, SYSTEMS PERSONALITIES, UCL ENTRIES, VOICE ANNOUNCMENT, ENCRYPTION KEYS) on the mid tier to go to a high tier | QA01771AB | 0481 | $235.00
ADD: EXTREME 1-SIDED NOISE REDUCTION | Compatible with all APX6000 Radios. Comes standard on APX6000XE. | QA01833AH | 0481 | $30.00
ADD: GROUP SERVICES | Group Services offers Conventional Alias updates, Trunking Alias updates and Trunking Group Messaging. This option requires G/Q806 for Conventional only capabilities and G/Q361 for any Trunking only capabilities. You can now also do Over the Air Firmware Updates with this feature. (requires digital) | QA09008 | 655 | $177.00
ADD: MANDOWN OPERATION | APX6000 customers ONLY- with radios using tanapas with revision A or B will also need to order the APX6000 MAN DOWN UPGRADE HW KIT in addition to the Man Down SW flashport option QA01843AB. Please contact your sales representative for further details. | QA01843 | 481 | $177.00
ADD: APX Personnel Accountability | This feature now also allows the user to use a side button of the radio as a method to transmit the acknowledgement of an Evacuation instead of using PTT button. | Q445 | 481 | $177.00
ENH: TACTICAL RADIO STW-STUN/KILL | Tactical Stun Kill is not compatible with DVRs QA00631. | H02 | 481 | $89.00
ENH: ENHANCED ZONE BANK | This option will increase the channel/talkgroup capacity on a Model 1 and Model 1.5 from 96 to 1000. Zone Up/Zone Down, Zone Bank Up/Zone Bank Down will be unlocked with this option. | QA01768 | 481 | $89.00

NEW SYSTEM ENHANCEMENT OPTIONS (EFFECTIVE AUGUST 2016)

These new system enhancement options are only available on the following models: H98UCD9PW5BN, H98UCF9PW6BN, H98UCH9PW7BN

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: WIFI CAPABILITY | Enables Wi-Fi capability in the radio. Supports codeplug updates, firmware refreshes, and FLASHport upgrades over pre-provisioned wireless networks. Requires Radio Management SW (ordered separately). Must order Out of the Box Wi-Fi Provisioning option (QA09007) if provisioning the radios out of the box using Wi-Fi is desired. | QA09001 | 579 | $353.00
ADD: OUT OF THE BOX WIFI PROVISIONING | Requires Wi-Fi (QA09001). Must be added if provisioning the radios out of the box using Wi-Fi is desired. Refer to the 'Out of the Box Wi-Fi Provisioning' section above for details. | QA09007 | 579 | $0.00
ADD: ADAPTIVE NOISE SUPPRESSION | Adaptive Noise Suppression is available on APX6000/XE and SRX2200 BN Models only. Adaptive Noise Suppression is not available on any APX6000Li models, or on APX6000/XE and SRX2200 AN Models. | QA09006AA | 0579 | $177.00

6: Algorithm Options (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: MULTIKEY | Required when more then one encryption is "purchased". (encryption algorithm or encryption key) "Requires MultiKey". | H869 | 481 | $363.00
ADD: TACTICAL OTAR | This feature REQUIRES IV&D (Q947) AND Digital Encryption ? AES (Q629) or DES, DES-XL, DES-OFB (Q625), AES/DES (Q15) to operate. Incompatible with MDC/ASTRO P25 OTAR with Multikey. Tactical OTAR is not compatible with DVRs QA00631. | H04AT | 0481 | $412.00
ENH: ASTRO 25 OTAR W/ MULTIKEY | Incompatible with the H04 option since Tactical OTAR is included with the Q498 option. Tactical OTAR can only be utilized when IV&D is purchased. | Q498 | 481 | $814.00
ENH: DVP-XL ENCRYPTION AND ADP | Compatible with Digital and Analog (25kHZ Only) operations. ADP Privacy ships standard with Single Key. Multikey is required for multiple algorithms, such as ADP/AES or ADP/DES . | H797 | 481 | $574.00
ENH: DES,DES-XL,DES-OFB ENCRYPTION AND ADP | Compatible with Analog 25kHZ/DES-OFB Digital 12.5kHZ Only. ADP Privacy ships standard with Single Key. Multikey is required for multiple algorithms, such as ADP/AES or ADP/DES | Q625 | 481 | $659.00
ENH: AES ENCRYPTION AND ADP | ADP Privacy ships standard with Single Key. Multikey is required for multiple algorithms, such as ADP/AES or ADP/DES | Q629 | 481 | $523.00
ADD: AES/DES-XL/DES-OFB ENCRYPTION AND ADP | - | Q15AK | 0481 | $941.00
ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | - | QA05751AA | 0655 | $0.00

7: Antenna (Optional- Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: GPS STUBBY ANTENNA (NAG4000) | Deletes Standard Antenna and ADDS GPS ONLY antenna. | QA00785 | 481 | $21.00
ALT: UHFR2 GPS STUBBY ANTENNA (FAF5260) | Only Compatible with - H98SDD9PW5AN, H98SDF9PW6AN, H98SDH9PW7AN, H98SDD9PW5BN, H98SDF9PW6BN, H98SDH9PW7BN This UHF R2 Stubby antenna is compatible with Public Safety Microphone accessory. The APX radio requires GPS antenna (NAG4000) when Public Safety Microphone is attached. | QA02017 | 481 | $28.00
DEL: DELETE STANDARD ANTENNA | For APX6000/Li/XE, deletes standard antenna. NAF5085 (7/800), NAR6593 (VHF) or PMAE4065 (UHF). | H112 | 481 | ($10.00)

8: Battery (Optional- Can Only Select One)

IMPRES 2 BATTERIES

APX6000 New Standard Battery PMNN4485 (Effective August, 2016)

UL/TIA-4950 Battery

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ALT: LI-ION IMPRES 2 UL/CSA 2650MAH (NNTN8930A) | This option will delete the standard battery and replace it with LIION IMPRES 2650mAh(NNTN8930). | QA05574 | 655 | $110.00
ALT: LI-ION IMPRES 2 4500 MAH UL/CSA (NNTN8921A) | This option will delete the standard battery and replace it with LIION IMPRES 4500MAH (NNTN8921). | QA05575 | 655 | $165.00
ALT: LI-ION IMPRES 2 UL/CSA RUGGED 2650MAH (NNTN8930) | Requires H499 to be selected. This option will delete the standard battery and replace it with LIION IMPRES 2650mAh(NNTN8930). | QA06305 | 579 | $50.00
ALT: LI-ION IMPRES 2 4500 MAH UL/CSA RUGGED (NNTN8921) | Requires H499 to be selected. This option will delete the standard battery and replace it with LIION IMPRES 4500MAH (NNTN8921). | QA06304 | 579 | $75.00

Not Compatible if HAZLOC Certification is Required.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
DEL: DELETE STANDARD BATTERY | Deletes the standard SLIM IMPRES 2 LIION 2550MAH battery for the APX6000/Li AN/BN Models, or the standard LIION IMPRES 2 LIION 2650MAH battery for the APX6000XE AN/BN Models. | H207 | 481 | ($30.00)
ALT: LI-ION IMPRES 2 IP68 3400 MAH | This option will delete the standard battery and replace it with IMPRES 2 LIION 3400MAH(PMNN4486). Compatible with all APX6000/XE/Li & SRX2200 AN & BN model numbers. Compatible with the APX7000XE. | QA05570 | 562 | $124.00
ALT: LI-ION IMPRES 2 IP68 4850 MAH | This option will delete the standard battery and replace it with IMPRESS 2 LIION 4850MAH (PMNN4487). | QA05571 | 655 | $143.00
ALT: LI-ION IMPRES 2 IP68 5100MAH | This option will delete the standard battery and replace it with IMPRESS 2 LIION 5100MAH (PMNN4494). | QA05573 | 655 | $167.00

9: Belt Clips (Optional-Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
DEL: DELETE BELT CLIP/ BASIC CARRY | - | H301CN | 0481 | $0.00
ALT: BASIC CARRY HOLDER (PMLN7901) | This carry holder equipped with a 2.5 in. belt clip ships standard with the Dual Display models. It is an alternative to the Belt Clip that ships standard with the Top Display model. | QA00779 | 481 | $34.00
ADD: BELT CLIP 3.0" (HLN6875) | Replaces the standard 2.5 in. belt clip that ships with the Model 1.5 radio with a 3 in.. Model 1.5 radios in 700/800 and VHF will ship standard with the 2.5 in. belt clip, and UHF radios will ship with the 3 in. belt clip. | QA01222 | 481 | $14.00

10: Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX DATA CABLE | PMKN4012B- Used to program the radio with Customer Programming Software and Tuner Software. PMKN4013C - Used to program and service the radio with Customer Programming Software and Tuner Software. Compatible on ALL APX Portable Radios | Q157 | 655 | $89.00

11: RFID Enabled Volume Knob (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: RFID KNOB | Compatible with APX6000, APX7000 & APX8000. Portable radio volume knob with embedded RFID tag making it easier to track assets. When option is ordered, RFID Volume knob will come in the box with the portable radio and other ordered accessories but RFID knob will not be assembled to the radio. AFTERMARKET purchase through Parts department for fielded radios NNTN8646 (APX6000/APX7000/APX8000) and NNTN8647 (APX6000XE/APX7000XE/APX8000XE). See RFID Solution Partner link for information on partners that can provide customers with scanner hardware and back end asset management solutions. | QA04526 | 655 | $30.00

12: Housing (Optional-Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SUBMERSIBLE (DELTA T) | IF AN INTRISICALLY SAFE SOLUTION IS REQUIRED THEN PLEASE SEE THE 'UL' REPLACEMENT QA06305 & QA06304. | H499 | 481 | $177.00
ALT: PUBLIC SAFETY YELLOW HOUSING | APX6000 comes standard IP67 unless ordered with H499 Delta T option. APX6000XE comes Delta T standard. | H64 | 481 | $30.00
ALT: IMPACT GREEN HOUSING | APX6000 comes standard IP67 unless the H499 Delta-T option is ordered. APX6000XE comes standard Delta-T. | QA01427 | 481 | $30.00

13: Service Options (Optional- Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 3Y ESSENTIAL SERVICE | Provides 3 years of hardware coverage beginning at time of purchase. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | H885BK | 185 | $133.00
ADD: 3Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 3 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00022AB | 185 | $272.00
ADD: 5Y ESSENTIAL SERVICE | Provides 5 years of hardware coverage beginning at time of shipment. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | Q887 | 185 | $222.00
ADD: 5Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 5 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00025AG | 185 | $454.00
ADD: 3Y ESSENTIAL SVC CANADA | Upgrades the standard warranty period to a full three (3) years of hardware service coverage on the internal components of your radio equipment. Repairs will be made only at Motorola authorized service centers. No discounts are allowed on this option. | HA00048 | 386 | $184.00
ADD: 5Y ESSENTIAL SVC CANADA | Upgrades the standard warranty period to a full five (5) years of hardware service coverage on the internal components of your radio equipment. Repairs will be made only at Motorola authorized service centers. No discounts are allowed on this option. | HA00049 | 185 | $307.00

14: Manual (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: USER GUIDE,CD,APX 7K/6K USER CDROM | - | H88 | 655 | $30.00
ADD: DATA LINK MANAGER APP CD- PORTABLES | Option provides the NVN5424 Data CD. Please order this option if you would like the Data CD, and are unable to obtain it through other sources such as MOL. | QA00205 | 655 | $0.00

15: Packaging (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SINGLE UNIT PACKING | - | H842 | 481 | $0.00

16: Test Results (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799 | 481 | $12.00

### Software and Services

RADIO WIDE FEATURES
Maximum Modes
APX 6000 Top Display | 96 | 96 | 96 | 96
APX 6000 Limited Keypad | 1000 | 1000 | 1000 | 1000
APX 6000 Full Keypad | 1000 | 1000 | 1000 | 1000
Analog and Digital Operation | Yes | Yes | Yes | Yes
6.25/12.5/20/25 KHz Programmable Channels | Yes | Yes | Yes | Yes
Secure Capable | No | Yes (Digital Only) | Yes (Digital Only) | Yes (Digital Only)
One Touch Operation | Yes | Yes | Yes | Yes
Real Time Clock | Yes | Yes | Yes | Yes
Surveillance Mode | Yes | Yes | Yes | Yes
Keypad Lock | Yes | Yes | Yes | Yes
Radio Lock | Yes | Yes | Yes | Yes
Smart Battery | Yes | Yes | Yes | Yes
Radio Wide Transmit Inhibit | Yes | Yes | Yes | Yes
Time Out Timer | Yes | Yes | Yes | Yes
FLASHport | Yes | Yes | Yes | Yes
ANALOG CONVENTIONAL FEATURES
Conventional Features are additional radio wide features beyond those specified above.
CSQ/PL/DPL | Yes | Yes | Yes | Yes
Dual Priority Channel Scan | Yes | Yes | Yes | Yes
Adaptive Power Control | No | Yes | Yes | Yes
Repeater/Talkaround Operation | Yes | Yes | Yes | Yes
Scan (Auto, Pre-programmed, Operator Selectable) | Yes | Yes | Yes | Yes
Smart PTT | Yes | Yes | Yes | Yes
Monitor | Yes | Yes | Yes | Yes
DTMF Tone Generation | Yes | Yes | Yes | Yes
DTMF Signaling | Future | Future | Future | Future
Quick-Call Signaling | Yes | Yes | Yes | Yes
DIGITAL CONVENTIONAL SIGNALING FEATURES
These features are APCO Project 25 Conventional Interoperable Features when used in the ASTRO Digital CAI Mode (Q806).
Unaddressed Voice Call (Dispatch Call) | Yes | Yes | Yes | Yes
Talk Group Call | Yes | Yes | Yes | Yes
Group Call Alert™ | Yes | Yes | Yes | Yes
Talk Group Identification (TGID) | Yes | Yes | Yes | Yes
Selective Call (Individual Voice Call) | MDC-1200 Only | Yes | Yes | Yes
Selective Call Decode (Individual Voice Call) | MDC-1200 Only | Yes | Yes | Yes
PTT ID (Individual Identification) | MDC-1200 Only | Yes | Yes | Yes
Call Alert Encode/Decode | MDC-1200 Only | Yes | Yes | Yes
Emergency Alarm w/Channel Revert & Ack. | MDC-1200 Only | Yes | Yes | Yes
Telephone Interconnect | Yes | Yes | Yes | Yes
Manual Phone Number Entry | Dual Display Only | Dual Display Only | Dual Display Only | Dual Display Only
Selective Radio Inhibit | MDC-1200 Only | Yes | Yes | Yes
Radio Check | MDC-1200 Only | Yes | Yes | Yes
Status/Message | MDC-1200 Only | Yes | Yes | Yes
Trunking Type II Only Features
Maximum Number of Trunked Systems-20 | Yes | Yes | Yes | Yes
Talkgroup Calls | Yes | Yes | Yes | Yes
PTT ID | Yes | Yes | Yes | Yes
Call Alert Encode/Decode | Yes | Yes | Yes | Yes
Analog/Digital Dual Mode Scan | No | Yes | Yes | Yes
Failsoft by Talkgroup | Yes | Yes | Yes | Yes
Telephone Interconnect Encode/Decode | Yes | Yes | Yes | Yes
System Wide Call (Receive Only) | Yes | Yes | Yes | Yes
Selective Radio Inhibit | Yes | Yes | Yes | Yes
Priority Monitor Scan | Yes | Yes | Yes | Yes
Dynamic Regrouping | Yes | Yes | Yes | Yes
Status/Message | Yes | Yes | Status Only | Status Only
Private/Enhanced Conversation Encode/Decode | Yes | Yes | Yes | Yes
Remote Monitor/Radio Trace | Yes | Yes | Yes | Yes
Reprogram Request | Yes | Yes | Yes | Yes

Trunking Type II Only Features
Voice on Control | - | - | - | -
SmartZone Automatic Site Registration | Yes | Yes | Yes | Yes
SmartZone RSSI Operation | Yes | Yes | Yes | Yes
SmartZone Preferred Site | Yes | Yes | Yes | Yes
SmartZone Forced Site Search | Yes | Yes | Yes | Yes
SmartZone Site Lock/Unlock | Yes | Yes | Yes | Yes
SmartZone Adjacent Control Channel OSW | Yes | Yes | Yes | Yes
Emergency Alarm Call Receive Indication | Yes | Yes | Yes | Yes

Channel Spacing

There are no maximum frequency separation conditions that must be adhered to on the APX 6000 P25 portable radio. Separation of frequencies can be as wide as the allowable band per radio model with no degradation of any performance specifications. If an incorrect antenna is used, degraded performance may be experienced.

Zoned Operation

This option converts APX 6000 P25 portable radios to Zone Operation radios.

For Top Display radios, a maximum of 16 channels (conventional RX and TX pairs or trunking talkgroups) are accessible in a zone. There is a maximum of six accessible zones (96 channels) when zone selection operation is programmed on the 3 position toggle switch and the Zone Bank feature is programmed on a button. The Zone Bank feature allows the 3 position toggle switch to access zones 1-3 or 4-6.

For the Top Display radio there is a maximum of 6 accessible zones, and 16 accessible channels per zone with the overall maximum of 96 channels. For the Dual Display Radios with Limited keypad or Full Keypad, there is a maximum of 50 zones, 625 channels per zone with the overall maximum of 1000 channels. These radios provide "ZONE" and "CHAN" menus that allows access to zones and channels not accessible via the switches.

*Note: Top Display Radio code plugs can be programmed with the same zone/channel configuration as the Dual Display Radios even though not all of the zones and channels are accessible. This is useful for having a common zone/channel template that can be shared between the different radio models.

Project 25 Encryption

Encryption is available for Project 25 voice (Phase 1 FDMA and Phase 2 TDMA) and data communications. The mode of operation is programmed on a channel-by-channel basis. With the coded/clear switch set to the clear mode, the APX 6000 P25 Portable Radio is capable of transmitting clear analog voice or clear (unencrypted) ASTRO Digital voice, depending on the channel programming. With the coded/clear switch set to the coded mode, the APX 6000 P25 Portable Radio is capable of transmitting encrypted CVSD (analog) voice or encrypted ASTRO Digital encryption voice, depending on the channel programming.

An encryption option is not required for either clear analog operation or clear ASTRO Digital operation. Encryption can be ordered with the APX 6000 P25 Portable Radio either as a factory installed option or separate from the radio for later field installation. APX 6000 P25 Portable Radio functions include selected ASTRO digital signaling and digital speech coding.

When ordering any of the Encryption Algorithms:

- The DES-OFB and AES encryption algorithms offered are compliant with Project 25 standards, neither of which support CVSD (analog) encryption operation. These algorithms require ASTRO Digital CAI (Q806) to operate.
- The ADP, DES-XL, and DVP-XL encryption algorithms can operate in CAI digital mode, but will not be compliant with the APCO Project 25 standard.
- The DES, DES-XL, and DVP-XL encryption algorithms can operate in CVSD (analog) mode.
- If ordering multiple encryption options, the Multikey (H869) option is required for purchase.

Additional encryption algorithms can be ordered later via APX MACE Upgrades:

1. If using a KVL 4000, please click here.
2. If using a KVL 3000 Plus, please click here.

FIPS140-2 Compliance

Encryption Modules equipped with AES are FIPS 140-2 compliant. Details regarding the certification, and copies of the relevant certificates, can be obtained on the NIST website at: http://csrc.nist.gov/groups/STM/cmvp/validation.html.

Further information regarding FIPS 140-2 certification may be found using the following link - FIPS 140-2 Crypto Module Validation Program (CMVP) http://csrc.nist.gov/groups/STM/cmvp/index.html

Hazardous Location

UL
The APX 6000 is certified by Underwriters' Laboratory when properly equipped with alternate battery options QA05574, QA005575, QA06304, or QA06305. When equipped with Motorola Batteries NNTN8930A or NNTN8921A, the APX6000 models are certified as intrinsically safe for use in ANSI/TIA 4950-A and CAN/CSA C22.2 NO. 157-92; Classification Rating Class I, Division 1, Groups C, D; Class II, Division 1, Group E, F, G; Class III, Hazardous (Classified) Locations. ANSI/ISA 12.12.01-2015 and CAN/CSA C22.2 No.213-15; Class I, Division 2, Groups A, B, C, D; T3C. Tamb = -25° C to +60° T3C.

APX Series Hazloc Fact Sheet

ASTRO Text Messaging Service
ASTRO Text Messaging Service will be available on APX 6000 Dual Display Portable radios. Text Messaging Service (TMS) allows subscriber users to send and receive text messages to other subscribers or dispatch operators. Users can select messages and addresses from a predefined list or enter freeform text messages and addresses via the keypad. Text Messaging Service is available on ASTRO P25 Conventional and Trunked IV&D Systems and Subscribers.

Text Message is NOT supported on APX 6000 Top Display (Model 1.5) Portable radio.

Ordering ASTRO Text Messaging for APX 6000 Portable Requires:

- APX 6000 Dual Display

- ASTRO Digital CAI Operation (Q806)

- Conventional Operation (H35)

OR

- APX 6000 Dual Display

- ASTRO Digital CAI Operation (Q806)

- SmartZone Operation (H38)

- ASTRO Project 25 Trunking Software (Q361)

NOTE: There is no specific option to order for the Text Messaging Service on the subscribers as the functionality is included in the Packet Data option. Please order Digital Operation to receive Text Messaging ability as Packet Data is a standard feature on APX Portable and Mobile Radios.

Outdoor Personnel Location Global Positioning Satellite (GPS) Feature

The personnel outdoor location tracking GPS feature enables a dispatcher the ability to locate on-foot patrols and out of the vehicle officers who are involved in life threatening situations. The radio user’s GPS position information is sent over the ASTRO 25 Integrated Voice & Data (IV&D) network and is delivered to the dispatch operator using a third party mapping display application at the dispatch center (Mapping Application is not yet available through Motorola at this time, however an Application Developers Tool Kit is available for 3rd party vendors to use to modify existing applications. See link below for more details.) On the Dual Display model only it is possible to the user to determine their own location (latitude/longitude) through the use of the location menu.

During normal operation the radio battery capacity will be reduced by 10 to 16 percent.

In order to obtain an initial GPS fix position, the radio must be located in an open sky, outdoor environment with no barriers that could affect the signal around you or above you. During this initial fix, the radio should NOT be worn on the body as this may affect the process of acquiring signal and/or add additional time to first fix.

Note Limitations of Use:

GPS works best in an open sky (clear view of the sky with no obstructions) environment. Due to the limitations of the technology, there are certain situations which prevent GPS coverage. These situations include but are not limited to:

- Underground locations (tunnels, subways, etc.)
- Inside of buildings, elevators, parking garages, trains, other covered vehicles, etc.
- Under metal or concrete roof structures
- Urban canyons (between tall buildings or under dense tree coverage)

***GPS Performance may be degraded when the radio is worn against the body and/or against the body within a vehicle.

Due to the limitations mentioned above, GPS should only be utilized as a method to assist the user with location information but not as a means for mission critical communication. Therefore, in any emergency situation, the location should always be verbally reported to the dispatcher.

Ordering GPS for APX 6000 P25 Portable Radios requires:

- APX GPS Activation (QA00782)

#### UHF Self-quieting Spurs

UHFR1 Models (1.5, 2.5, 3.5) | AN Model Frequencies | BN Model Frequencies
UHFR2 Models (1.5, 2.5, 3.5) | AN Model Frequencies | BN Model Frequencies

CPS 3-Year Subscription Update

In addition to the traditional 3 Year DVD CPS software subscription (RVN5224 - List $399), we will offer a download-only 3 Year CPS software subscription (HKVN4289A, - List $299) which will provide access to CPS software through your Motorola Online account. Only one subscription per MOL account is needed. The original price of $375 for RVN5224 will increase to $399 on July 1, 2015.

How to order DVD CPS Subscription (RVN5224) through COF:

1. Sign and return the Software License Agreement

2. Order the software part number (RNN5224)

3. New releases on disk will be automatically sent for a three-year period.

How to order Download-Only CPS Subscription (HKVN4289A) through MOL:

1. Call 1-800-422-4210, option 4 (MOL Support Team) to request an MOL account or to add a CPS subscription to an existing account.

2. Sign and return the Software License Agreement through MOL

3. Order HKVN4289A

4. Provide a valid email address; as the 3 year subscription period ends subscription renewal reminders will be sent to this email address.

CPS downloads are only available on MOL for North America. Please see your regional MOL page for information on receiving CPS in other regions.

### Ship Card

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
APX_PORTABLE | US1 | G996AU | ADD: PROGRAMMING OVER P25 (OTAP) | 0481 |
APX_PORTABLE | US1 | H04AT | ADD: TACTICAL OTAR | 0481 |
APX_PORTABLE | US1 | H301CN | DEL: DELETE BELT CLIP/ BASIC CARRY | 0481 |
PORTABLES | FSC | H98QDD9PW5BN | APX6000 UHF R1 MODEL 1.5 PORTABLE | 481 | 89
PORTABLES | FSC | H98QDD9PW5BN | APX6000 UHF R1 MODEL 1.5 PORTABLE | 481 | 3
PORTABLES | FSC | H98QDF9PW6BN | APX6000 UHF R1 MODEL 2.5 PORTABLE | 481 | 10
PORTABLES | FSC | H98QDF9PW6BN | APX6000 UHF R1 MODEL 2.5 PORTABLE | 481 | 1
PORTABLES | FSC | H98QDH9PW7BN | APX6000 UHF R1 MODEL 3.5 PORTABLE | 481 | 30
PORTABLES | FSC | H98QDH9PW7BN | APX6000 UHF R1 MODEL 3.5 PORTABLE | 481 | 5
PORTABLES | FSC | H98SDD9PW5BN | APX6000 UHFR2 MODEL 1.5 PORTABLE | 481 | 65
PORTABLES | FSC | H98SDF9PW6BN | APX6000 UHF R2 MODEL 2.5 PORTABLE | 481 | 33
PORTABLES | FSC | H98SDH9PW7BN | APX6000 UHF R2 MODEL 3.5 PORTABLE | 481 | 90
APX_PORTABLE | US1 | Q15AK | ADD: AES/DES-XL/DES-OFB ENCRYPTION AND ADP | 0481 |
APX_PORTABLE | US1 | Q15AK | ADD: AES/DES-XL/DES-OFB ENCRYPTION AND ADP | 0481 |
APX_PORTABLE | US1 | QA01648AA | ADD: HW KEY SUPPLEMENTAL DATA | 0655 |
APX_PORTABLE | US1 | QA01771AB | SOFTWARE LICENSE ENH: ENHANCEMENT LEVEL 2 | 0481 |
APX_PORTABLE | US1 | QA01833AH | ADD: EXTREME 1-SIDED NOISE REDUCTION | 0481 |
APX_PORTABLE | US1 | QA05751AA | ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | 0655 |
APX_PORTABLE | US1 | QA09006AA | ADD: ADAPTIVE NOISE SUPPRESSION | 0579 |