Back

##### APX 6000 Family

###### Product Catalog

##### Jump to ...

- Models
- Updates
- Configuration
- Software and Services
- Ship Card

Back

##### APX 6000 Family

### Models

·

·

·

·

·

·

·

APX™ 6000 P25 Portable Radio P25 Phase 2 Single Band Capable Radio

### Updates

#### Announcements

- CLICK HERE to see the Latest lead Time Estimates

NEW: Beginning September 2023 APX radios can be ordered with the New Feature/Latest release or the Baseline release firmware. The Baseline release is defined as a single major software release (i.e. 202X.1) to ship from the factory for a 1 year duration. The first major release each year will be the Baseline Release. A New Feature Release is defined as the second and third major releases each year (202X.2 and 202X.3) and is required for customers to access new feature content and/or products. New Feature releases contain the current year’s Baseline content as well as content from the previous New Feature release.

IMPORTANT! Radios that are ordered via COF must add the Baseline Release option (QA09113) if the Baseline firmware is desired. If the Baseline option (QA09113) is not added to COF orders, radios will ship with the Latest Release and cannot be rolled back to the Baseline Release. Most quotes and orders should keep the default Baseline Firmware (QA09113) unless a customer desires new functionality only provided in a New Feature release. More information about the Baseline and New Feature Release strategy can be found in MTN-0111-23-NA.

- Effective October 5th, 2020: All U.S. orders will require an encryption selection. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. G193/Q667 ADP only is also available at $0. Please see encryption section for AES and other encryption options that come with ADP. Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.
- NOTE: APX radios always ship with the MACE installed
- If the QA05751 “Clear Radio No ADP option is NOT ordered, you will be required to order an encryption algorithm option.
- As long as a radio doesn't ship with the QA05751 “Clear Radio No ADP option, additional encryption options can be ordered and installed in the field as upgrades in the future.
- If AES is ordered, it will be installed on the radio in the factory along with ADP. CPS provides some programming options for determining how the radio uses encryption.
- AES by itself cannot be disabled but you can disable hardware (MACE) secure operation in the radio via CPS.
- AES will not work unless hardware secure operation is enabled.
- You can select software secure operation which will program the radio to use software ADP encryption.
- You can disable secure operation altogether.
- You can remove AES from the radio using a KVL but it will be deleted permanently. If you want to reinstall it, you will need to purchase an AES upgrade.

- PMNN4547 IMPRES 2 LIION 3100 MAH will be available as an option, QA07577 or QA07578, on the APX 6000. This battery is slightly larger and will require a new holster, PMLN7901. This holster is now the standard carry holster for the Models 2.5 and Models 3.5 and will fit all of the current batteries in the portfolio. The legacy holster, PMLN5709 is no longer available
- Battery options QA05574 and QA06305, which provided for NNTN8930, will no longer be available.
- The new standard 7/800 MHz whip antenna on the APX6000 will be PMAF4040 instead of NAF5085. PMAF4040 is has a slightly thinner and more flexible form factor. PMAF4040A supports GPS operation.
- High Cap Battery NNTN8921 (QA05575 & QA06304) has been replaced by PMNN4573 (QA07576 & QA07739)

### Ordering Information

#### Standard Features

All ASTRO Digital APX 6000 models include the following features:

- GPS Software & Hardware (QA00782)

- Mission Critical Wireless Bluetooth® 4.0 (LE) (QA00583)

- Radio Packet Data (Q947)

- Software Key (QA01749)

- 3 Programmable Side Buttons
- Orange Programmable Button
- 16 Position Mode Rotary Select Switch
- Angled On/Off Volume Knob
- 1 Top Mounted Programmable 3 Position Toggle Switch

- Top Display: 1 line of text, 1 line of icons, 0 menu lines
- Dual Microphone

- 3 Watt Rated Audio (Requires QA09006 to enable)

- Detachable Belt Clip (Model 1.5) / Carry Holder (Models 2.5 & 3.5)

- IMPRES 2 Battery (PMNN4485)

- IP68 (2m, 2hr)

- Single-Band Antenna (dependent on model/frequency selected)

- Models 2.5 & 3.5:

- Unified Call List
- Front Color Display: 4 Lines of Text, 2 Lines of Icons
- Radio Profiles
- 3 Programmable Buttons
- 4-Way Navigation
- Home & Data Buttons

- Model 3.5: 4 X 3 Alpha-Numeric Keypad

#### Additional Ordering Information for Service Options

SmartConnect End to End Ordering Guide

### Configuration

#### Models

1: Base Radio $8,060.42 List $4,433.23 Disc $3,183.23 w/Trade

Description | Full Description | Nomenclature | APC | Price
APX6000 700/800 MODEL 3.5 PORTABLE | - | H98UCH9PW7BN | 481 | inc
ADD: SMARTZONE OPERATION |  | H38 | 481 | inc
ADD: P25 9600 BAUD TRUNKING |  | Q361 | 481 | inc
ADD: ASTRO DIGITAL CAI OPERATION |  | Q806 | 481 | inc
ADD: TDMA OPERATION |  | QA00580 | 481 | inc
ADD: PROGRAMMING OVER P25 (OTAP) |  | G996AU | 0481 | inc
ADD: ENHANCED DATA APX |  | QA03399 | 656 | inc
ADD: DVRS PSU ACTIVATION |  | QA00631 | 655 | inc
ENH: RADIO TRACE/ REMOTE MONITOR |  | H43 | 481 | inc
ADD: GROUP SERVICES |  | QA09008 | 655 | inc
ADD: SMARTCONNECT |  | QA07682AA | 0579 | inc
ADD: HW KEY SUPPLEMENTAL DATA |  | QA01648AA | 0655 | inc

Housing (Optional)

Description | Full Description | Nomenclature | APC | Price
ENH: SUBMERSIBLE (DELTA T) | High Cap Battery NNTN8921 (QA05575 & QA06304) has been replaced by PMNN4573 (QA07576 & QA07739). | H499 | 481 | $177.00
ALT: PUBLIC SAFETY YELLOW HOUSING | APX6000 comes with standard IP67 unless ordered with the H499 Delta T option. This option allows the selection of housing color to Safety Yellow and Impact Green, respectively. | H64 | 481 | $30.00
ALT: IMPACT GREEN HOUSING | APX6000 comes standard IP67 unless the H499 Delta-T option is ordered. APX6000XE comes standard Delta-T. | QA01427 | 481 | $30.00

RFID Enabled Volume Knob (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: RFID KNOB | Compatible with APX6000, APX7000 & APX8000. Portable radio volume knob with embedded RFID tag making it easier to track assets. When option is ordered, RFID Volume knob will come in the box with the portable radio and other ordered accessories but RFID knob will not be assembled to the radio. AFTERMARKET purchase through Parts department for fielded radios NNTN8646 (APX6000/APX7000/APX8000) and NNTN8647 (APX6000XE/APX7000XE/APX8000XE). See RFID Solution Partner link for information on partners that can provide customers with scanner hardware and back end asset management solutions. | QA04526 | 655 | $30.00

System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 9600 Trunking | QA01767 | 481 | $118.00
ADD: WIFI CAPABILITY | Enables Wi-Fi capability in the radio. Supports codeplug updates, firmware refreshes, and FLASHport upgrades over pre-provisioned wireless networks. Requires Radio Management SW (ordered separately). Must order Out of the Box Wi-Fi Provisioning option (QA09007) if provisioning the radios out of the box using Wi-Fi is desired. | QA09001 | 579 | $353.00
ADD: OUT OF THE BOX WIFI PROVISIONING | Requires Wi-Fi (QA09001). Must be added if provisioning the radios out of the box using Wi-Fi is desired. Refer to the 'Out of the Box Wi-Fi Provisioning' section above for details. | QA09007 | 579 | $0.00

Algorithm Types (one must be selected)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

Description | Full Description | Nomenclature | APC | Price
ENH: AES ENCRYPTION AND ADP | Requires digital operation. P25 CAP Compliant option. Includes ADP. | Q629 | 481 | $523.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | Q667BB | 0430 | $0.00

Multikey Types (Optional)

Description | Full Description | Nomenclature | APC | Price
ENH: MULTIKEY | Required when using more than one encryption algorithm or encryption key | H869 | 481 | $363.00
ENH: ASTRO 25 OTAR W/ MULTIKEY | Not compatible with ADP-Only. Includes multikey, trunking OTAR, and Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. | Q498 | 481 | $814.00
ADD: MULTI SYSTEM OTAR | Requires Q498 ASTRO 25 OTAR W/ MULTIKEY | QA07680AA | 0655 | $177.00

Antenna (Optional)

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE STANDARD ANTENNA | For APX6000/Li/XE, deletes standard antenna. PMAF4040 (7/800), NAR6593 (VHF) or PMAE4065 (UHF). | H112 | 481 | ($10.00)
ALT: 1/4- WAVE 7/800 GPS STUBBY (NAR6595A | 7/800 Models Only | H122 | 481 | $28.00

#### Battery (Optional- Can Only Select One)

HAZLOC Approved

Description | Full Description | Nomenclature | APC | Price
ALT: TIA4950 BATT IMPRES 2 LIION 4600MAH | This option will delete the standard battery and replace it with TIA4950 BATT IMPRES 2 LIION 4600MAH (PMNN4573A) | QA07576 | 673 | $204.00
ALT: TIA4950 BATT IMPRES 2 LIION 4600MAH | Requires H499 to be selected. This option will delete the standard battery and replace it with TIA4950 BATT IMPRES 2 LIION 4600MAH (PMNN4573A) | QA07739 | 673 | $93.25
ALT: BATT IMPRES 2 LIION TIA4950 IP68 3100T STD | This option will delete the standard battery and replace it with LIION IMPRES 3100MAH (PMNN4547). | QA07577 | 481 | $167.00
ALT: BATT IMPRES 2 LIION TIA4950 R IP68 3100T | Requires H499 to be selected. This option will delete the standard battery and replace it with LIION IMPRES 3100MAH (PMNN4547). | QA07578 | 481 | $93.25

Not Compatible if HAZLOC Certification is Required.

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE STANDARD BATTERY | Deletes the standard SLIM IMPRES 2 LIION 2550MAH battery for the APX6000/Li AN/BN Models, or the standard LIION IMPRES 2 LIION 2650MAH battery for the APX6000XE AN/BN Models. | H207 | 481 | ($30.00)
ALT: LI-ION IMPRES 2 IP68 3400 MAH | This option will delete the standard battery and replace it with IMPRES 2 LIION 3400MAH(PMNN4486). Compatible with all APX6000/XE/Li & SRX2200 AN & BN model numbers. Compatible with the APX7000XE. | QA05570 | 562 | $124.00
ALT: LI-ION IMPRES 2 IP68 4850 MAH | This option will delete the standard battery and replace it with IMPRESS 2 LIION 4850MAH (PMNN4487). | QA05571 | 655 | $143.00
ALT:SLIM LIION 2550MAH BATTERY(PMNN4485) | SLIM LIION 2550MAH BATTERY(PMNN4485) | QA02021 | 481 | $98.75

Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: APX DATA CABLE | PMKN4012B- Used to program the radio with Customer Programming Software and Tuner Software. PMKN4013C - Used to program and service the radio with Customer Programming Software and Tuner Software. Compatible on ALL APX Portable Radios | Q157 | 655 | $89.00

Belt Clips (Optional-Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE BELT CLIP/ BASIC CARRY | - | H301CN | 0481 | $0.00
ALT: BASIC CARRY HOLDER (PMLN7901) | This carry holder equipped with a 2.5 in. belt clip ships standard with the Dual Display models. It is an alternative to the Belt Clip that ships standard with the Top Display model. | QA00779 | 481 | $34.00
ADD: BELT CLIP 3.0" (HLN6875) | Replaces the standard 2.5 in. belt clip that ships with the Model 1.5 radio with a 3 in.. Model 1.5 radios in 700/800 and VHF will ship standard with the 2.5 in. belt clip, and UHF radios will ship with the 3 in. belt clip. | QA01222 | 481 | $14.00

Packaging (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: SINGLE UNIT PACKING | - | H842 | 481 | $0.00

#### Programming Solutions

#### Service Options (Must Select One)

Description | Full Description | Nomenclature | APC | Price
EHN: STD 1 YR WARRANTY APPLIES | Provides no extended repair coverage after the standard warranty period expires. | QA05100AA | 0185 | $0.00
ADD: 3Y ESSENTIAL SERVICE | Provides 3 years of hardware coverage beginning at time of purchase. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | Q58 | 185 | $184.00
ADD: 3Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 3 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00022AC | 185 | $347.00
ADD: 5Y ESSENTIAL SERVICE | Provides 5 years of hardware coverage beginning at time of shipment. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | Q887 | 185 | $306.00
ADD: 5Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 5 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00025AH | 185 | $578.00
ADD: 7Y ESSENTIAL SERVICE HTP | Provides 7 years of hardware coverage beginning at time of shipment. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00690 | 185 | $386.00
ADD: 7Y ESSENTIAL W ACC DMG HTP | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 7 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00691 | 185 | $729.00

Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
RadioManagement (On-Prem) | See “How to Order” section in the Ordering Guide below. | N/A | N/A | N/A

Documentation (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: USER GUIDE,CD,APX 7K/6K USER CDROM | - | H88 | 655 | $30.00
ADD: DATA LINK MANAGER APP CD- PORTABLES | Option provides the NVN5424 Data CD. Please order this option if you would like the Data CD, and are unable to obtain it through other sources such as MOL. | QA00205 | 655 | $0.00
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799 | 481 | $12.00

### Software and Services

Wi-Fi

APX 6000 supports Wi-Fi 802.11 b/g/n with WPA2/WPA (PSK), and WEP security protocols. Wi-Fi can be used with the Radio Management SW in order to do codeplug updates, firmware refreshes, and FLASHport upgrades over a Wireless Network (WLAN). The radio will only connect to available Wi-Fi networks which have been pre-provisioned in the radio codeplug via CPS. The radio can be pre-provisioned with up to 20 SSIDs.
The Wi-Fi feature requires ordering option QA09001. The Wi-Fi feature is also available aftermarket as a FLASHport upgrade if not ordered out of the factory.

Radio Management (RM) is required in order to take advantage of the Wi-Fi capabilities on APX 6000.

Out of the Box WiFi Provisioning

If a radio is ordered the Wi-Fi option (QA09001) and the customer wishes to provision the radios out of the box using Wi-Fi, the radio must also be ordered with the Out of the Box Wi-Fi Provisioning option (QA09007).
A radio ordered with the Wi-Fi option and the Out of the Box Provisioning over Wi-Fi option will come with the following default codeplug configuration relative to Wi-Fi:
a. Wi-Fi will be enabled.
b. There will be one pre-configured network with the Network SSID set to “MyNetwork” and security type will be set to “None”.
c. The default state of Wi-Fi will be “on”.
A Wi-Fi router is required for connecting the Wi-Fi capable radio to the Device Programmer. The Wi-Fi router is to be procured by the agency programming the radios and must be provisioned with the Network SSID set to “MyNetwork” (case sensitive) with no password enabled.

For more details regarding the Out of the Box Wi-Fi Provisioning process, please refer to the Out of the Box Wi-Fi Provisioning Leaflet

Bluetooth 4.0 & Emergency Find Me

With Bluetooth 4.0 wireless technology and our APX™ Mission Critical Wireless portfolio, users can now connect a variety of Bluetooth audio accessories and data devices with their APX™ radio.

Bluetooth 4.0 also enables Emergency Find Me, a feature providing personnel with an added level of security by improving response time in emergencies. Once an emergency is activated on the APX 6000, a Bluetooth beacon signals other Bluetooth-enabled APX radios within range. Based on bluetooth signal strength, nearby APX radios will receive an emergency alert via intelligent lighting and a text message with users Radio ID along with signal strength status (excellent, poor, fair) to determine proximity, and will guide the nearest personnel to the user in distress.

#### Self-Quieting Spurs

7/800 Frequencies | VHF Frequencies | UHF R1 Frequencies | UHF R2 Frequencies
768 | 136.8 | 384 | 456
775.2 | 144 | 396.8 | 480
866.4 | 153.6 | 403.2 | 493.545