Back

##### KVL 4000

###### Product Catalog

##### Jump to ...

- Model
- Ordering Information
- Configuration
- Ship Card

Back

##### KVL 4000

### Model

KVL 4000
Key Variable Loader

THE KVL 5000 IS NOW AVAILABLE. THE KVL 5000 WILL REPLACE THE KVL 4000. TO ORDER YOUR NEXT GENERATION KEY LOADER CLICK HERE.

### Ordering Information

#### General Information

PLEASE NOTE: The Standard Support Period for the 7.11 Release ends on June 30, 2017. Any software and hardware expansions on this release will no longer be supported after this date.
Click here for additional information.

LINK TO ORDERING GUIDE

KVL 4000 Description & Details

The KVL 4000 is a two piece handheld key fill device (PDA and security adaptor) that allows customers to create, store, and deliver encryption keys, authentication keys, and algorithms into their security compatible radios, devices, and other secure communication infrastructure equipment. The KVL (Key Variable Loader) is required to load keys for all secure equipped products (subscriber and infrastructure) containing AES, DES, ADP, DES-XL, DES-OFB, DVP-XL and DVI-XL cryptographic algorithms.

The KVL 4000 has three modes of operation available: ASTRO 25 Mode, Radio Authentication Mode, and ASN Mode.

ASTRO 25 Mode
is required for P25 compliant systems, for ASTRO 25 (Conventional and Tactical) OTAR, and for any interactions with the Key Management Facility (KMF). ASTRO 25 mode provides Common Key Reference (CKR) key management. CKR key management eliminates the need to place a key in a specific memory location. All secure products that support CKR™ will access the same encryption keys independent of physical storage capabilities of the product.

NOTE: An Over-the-Air Rekeying (OTAR) system is a secure communications system in which encryption keys, managed by Key Management Facility (KMF), can be sent to subscriber units via radio transmission to a subscriber to load keys. Tactical OTAR allows the user, without the KMF, to wirelessly rekey radios within range of a radio modem connected to a KVL.

NOTE: If purchasing a KVL 4000 for use in LTE, you are required to use ASTRO 25 Mode.

Radio Authentication Mode
is required to enable the ability for the KVL to generate and send radio authentication keys. In Radio Authentication Mode The KVL 4000 generates a unique authentication key for each radio and synchronizes the authentication key information with the ASTRO 25 system remotely over a secure Virtual Private Network (VPN) connection without requiring the operator to travel to the ASTRO 25 core location.

The Radio Authentication key is aA unique 128 bit AES key, defined by the Project 25 standard, is required for the authentication key. It is generated by the KVL 4000 and stored in the Authentication Center (AuC). To maximize integrity, the authentication key is never sent over the air and it cannot be read from the radio.

The Radio Authentication Center is a central database that stores the authentication keys for all radios in the system.

See
Solution Brief
for more details.

Advanced Securenet (ASN) Mode
is for customers utilizing Physical Identifier (PID) key management. ASN mode provides PID key management. PID key management identifies a physical memory slot where a key variable is stored in a unit. All products that support PID key management access the same encryption keys dependent on the physical storage capability of the product. PID key management provides support for all SECURENET, Secure ASTRO, and Secure ASTRO®25 systems

[NOTE: Regarding DIMETRA: The Dimetra (Air Interface Encryption-AIE) KVL 3000 Plus Key Variable Loader is used to store and transfer encryption keys from the Authentication Centre to Dimetra System infrastructure devices (i.e. Zone Controller, Tetra Site Controller, and the Base Radio Controller) and Mobile Stations.]

[NOTE: To keyload CRYPTRmicro you must have KVL 4000 version B; on the security adapter label it must read T7537B.]

When to quote KVL 4000

Quote a KVL 4000 to your customer if:

- The customer is going to use encryption on their radio channels
- They have a KMF
- They want to use OTAR
- They need to load encryption algorithms, aftermarket, on to their radios

Customer Considerations

Things for the customer to consider:

- What encryption algorithm you will need
- How many KVLs you will need

1. How many locations will need to be able to load keys
2. How many traveling technicians will need to be able to load keys
3. Backup units

- Do you use Radio Authentication in your system?
- Do you use ASN Mode?
- If you are using in an LTE system order ASTRO 25 Mode
- What cables you will need to keyload your radios

1. A list is provided; however, your specific radio manual with provide the most specific and accurate information on the keyloading cable needed

#### Ordering Requirements

Ordering KVL 4000 for ASTRO / P25

The following are
REQUIRED
to order KVL 4000 for ASTRO / P25,select the KVL 4000 (T7537B),
ASTRO 25 Mode Software (U239AD),
AES Encryption
(CA00182AP),
and applicable line cord.

REQUIRED KVL 4000 PARTS AND OPTIONS

Part Number | Description
--- | ---
T7537B | KVL 4000 (called KVL PDA Snap-On)
U239AD | ASTRO 25 Mode
CA00182AP | AES Encryption Software

The following options are
OPTIONAL
when ordering a KVL 4000:

ADDITIONAL OPERATION MODES

Part Number | Description
--- | ---
QA01767AA | Radio Authentication Mode Compatible with, and requires, ASTRO 25 Mode (U239AD)
X795AJ | ASN (Advanced Securenet) Mode Required for PID (Physical Identifier) Key Management

ADDITIONAL ALGORITHM OPTIONS

Part Number | Description
--- | ---
C793BM | DVI-XL ENCRYPTION SOFTWARE
CA00243AG | ADP PRIVACY
X423AF | DES/DES-XL/DES-OFB ENCRYPTION
X769AD | DVP-XL ENCRYPTION SOFTWARE

AC LINE CORDS (Picking one is required at time of order of KVL 4000)

Part Number | Description
--- | ---
DDN3094 | PWR SUPPLY ADAPTOR PWR BRICK AC DC 3A UNDERGROUND 5.4V 16W (REQUIRED)
DDN3095 | CABLE ASSEMBLY PWR 5.4VDC 3A PWR (REQUIRED)
XXX | ADD APPROPRIATE COUNTRY LINE CORD - SCROLL DOWN FOR PART NUMBERS

Part Number | Description
--- | ---
C542 | ADD: CABLE FOR KVL TO KMC (KEYLOADING) Cable for CIU, SYNTOR, SYNTOR X, KMC.
C543 | ADD: CABLE FOR RNC, DIU, MGEG Keyloading cable for KMF, MCC 7500, MGEG, CDEM, RNC, DIU 3000, and XTL 5000 Consolette.
C724 | CABLE, KEYLOAD Keyloading cable for XTS 5000, XTS 2500, and XTS 3000. Not for XTS 4000
C725AA | ADD: KEYLOAD CABLE FOR APX PORTABLE Keyloading cable for APX 7000 and APX6000
CA01603AA | Communication (USB)/ Charging cable with cup for MC55 PDA
CA02186 | ADD: KEYLOAD CABLE FOR CRYPTR MICRO
CA02187 | ADD: KEYLOADING CABLE ADAPTER (GCAI)

To add a sleeve cover when ordering a KVL 4000 order:

Part Number | Description
--- | ---
CA01803 | KVL 4000 SLEEVE COVER

Order KVL 4000 for LTE

The following are
REQUIRED
to order KVL 4000 for LTE systems,select the KVL 4000 (T7537B),
ASTRO 25 Mode Software (U239AD),
AES Encryption
(CA00182AP),
and applicable line cord.

REQUIRED KVL 4000 PARTS AND OPTIONS

Part Number | Description
--- | ---
T7537B | KVL 4000 (called KVL PDA Snap-On)
U239AD | ASTRO 25 Mode
CA00182AP | AES Encryption Software

The following options are
OPTIONAL
when ordering a KVL 4000:

Part Number | Description
--- | ---
QA01767AA | Radio Authentication Mode Compatible with, and requires, ASTRO 25 Mode (U239AD)
X795AJ | ASN (Advanced Securenet) Mode Required for PID (Physical Identifier) Key Management

ADDITIONAL ALGORITHM OPTIONS

Part Number | Description
--- | ---
C793BM | DVI-XL ENCRYPTION SOFTWARE
CA00243AG | ADP PRIVACY
X423AF | DES/DES-XL/DES-OFB ENCRYPTION
X769AD | DVP-XL ENCRYPTION SOFTWARE

Part Number | Description
--- | ---
C542 | ADD: CABLE FOR KVL TO KMC (KEYLOADING) Cable for CIU, SYNTOR, SYNTOR X, KMC.
C543 | ADD: CABLE FOR RNC, DIU, MGEG Keyloading cable for KMF, MCC 7500, MGEG, CDEM, RNC, DIU 3000, and XTL 5000 Consolette.
C724 | CABLE, KEYLOAD Keyloading cable for XTS 5000, XTS 2500, and XTS 3000. Not for XTS 4000
C725AA | ADD: KEYLOAD CABLE FOR APX PORTABLE Keyloading cable for APX 7000 and APX6000
CA01603AA | ADD: USB COMM/CHARGE CABLE W/ CUP Communication (USB)/ Charging cable with cup for MC55 PDA
CA02186 | ADD: KEYLOAD CABLE FOR CRYPTR MICRO
CA02187 | ADD: KEYLOADING CABLE ADAPTER (GCAI)

To add a sleeve cover when ordering a KVL 4000 order:

Part Number | Description
--- | ---
CA01803 | KVL 4000 SLEEVE COVER

*ENCRYPTION--All encryption products, kits, software, and technology require an approved export license prior to shipment. Review the following link http://exportcontrols.mot.com/ for any possible licensing restriction. The international use of encryption algorithms (except for DES, DES-XL, & DES-OFB) are highly restricted by the U. S. Federal Government. License approvals are considered for export to a limited selection of countries and end users. Review the above link, for a list of contacts, for the Global Trade Compliance Organization, for licensing information before submitting bids, proposals, or accepting orders for algorithm based encryption products.

### Configuration

#### Models

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
KVL 4000 PDA SNAP-ON | - | T7537B | 201 | $4,900.00
RUGGED USB CLIENT TO ETHERNET ADAPTER WITH USB CABLE BUILT IN. | - | DSPSA1U1EE | 708 | $193.00
KVL 4000 OS HARDENING SW | - | T7672 | 201 | $103.00

#### Options

Operation Mode

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ASN MODE | This option provides the ASN mode of operation and basic operating system software. This option is compatible with ASTRO 25 mode. This option is required for PID key management. | X795AJ | 201 | $600.00
ADD: KVL RADIO AUTHENTICATION | Requires U239AD- ASTRO 25 Mode. | QA01767AA | 201 | $500.00
ADD: ASTRO 25 MODE | ASTRO 25 Mode is required for P25 compliant systems. This option is required to perform CKR key management and is required for Conventional ASTRO 25 OTAR operation and the MGEG. NOTE: ASTRO 25 Mode includes KMF feature. | U239AD | 201 | $250.00

Algorithm Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ADD: DVI-XL ENCRYPTION SOFTWARE | Requires an Export Licence see Export Control Requirements section above. | C793BM | 201 | $825.00
ADD: DES/DES-XL/DES-OFB ENCRYPTION | - | X423AF | 201 | $825.00
ADD: ADP PRIVACY | ADP Privacy is not compatible with option X795, if U239 option is not ordered. Not compatible with KMF. ADP Privacy is not FIPS compliant - ADP Privacy not supported by OTAR - ADP is digital P25 conventional / P25 trunking only. | CA00243AG | 201 | $330.00
ADD: DVP-XL ENCRYPTION SOFTWARE | - | X769AD | 201 | $825.00
ADD: AES ENCRYPTION SOFTWARE | - | CA00182AP | 201 | $750.00

Cable(s)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: KEYLOAD CABLE FOR CRYPTR MICRO | - | CA02186 | 201 | $196.00
CABLE, KEYLOAD | Keyloading cable for XTS 5000, XTS 2500, and XTS 3000. Not for XTS 4000. | C724 | 201 | $75.00
ADD: CABLE FOR RNC, DIU, MGEG | Keyloading cable for KMF, MCC 7500, MGEG, CDEM, RNC, DIU 3000, and XTL 5000 Consolette. | C543 | 620 | $86.50
ADD: CABLE FOR KVL TO KMC (KEYLOADING) | Cable for CIU, SYNTOR, SYNTOR X, KMC. | C542 | 201 | $86.50
ADD: USB COMM/CHARGE CABLE W/ CUP | Communication (USB)/ Charging cable with cup for MC55 PDA. | CA01603AA | 201 | $118.00
ADD: KEYLOADING CABLE ADAPTER (GCAI) | - | CA02187 | 201 | $42.75
ADD: KEYLOAD CABLE FOR APX PORTABLE | Keyloading cable for APX 7000 and APX6000. | C725AA | 201 | $77.25

Power Supply Cable(s)

REQUIRED: DDN3094, DDN3095 plus the country's line cord

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
LINE CORD 18 AWG 250V 1.8M AC EUROPE | Europe Line Cord | DDN3121 | 201 | $25.00
PWR SUPPLY ADAPTOR PWR BRICK AC DC 3A UNDERGROUNDED 5.4V 16W | - | DDN3094 | 201 | $72.75
CABLE ASSEMBLY PWR 5.4VDC 3A PWR | (REQUIRED) CABLE ASSEMBLY PWR 5.4VDC 3A PWR | DDN3095 | 201 | $17.25
CORD PWR 18AWG 10A 250V UL PWR | UK CORD PWR 18AWG 10A 250V UL PWR | DDN3096 | 201 | $25.00
AC PWR CORD FOR US/ROHS PWR | AC PWR CORD FOR US/ROHS PWR | DDN3097 | 201 | $31.25
3FT US AC LINE CORD/3 WIRE FOR PWR PWRS | 3FT US AC LINE CORD/3 WIRE FOR PWR PWRS | DDN3098 | 201 | $17.00
PWR CORD 18AWG 10A 250V PWR AUSTRALIA | PWR CORD 18AWG 10A 250V PWR AUSTRALIA | DDN3099 | 201 | $17.00
CORD PWR CHINA PWR | CORD PWR CHINA PWR | DDN3100 | 201 | $17.00
CORD AC PWR 18AWG 3 PLUG BLK PWR 10A BRAZIL | CORD AC PWR 18AWG 3 PLUG BLK PWR 10A BRAZIL | DDN3101 | 201 | $25.00

Carrying Case(s)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: KVL 4000 SLEEVE COVER | - | CA01803 | 201 | $77.25

#### Accessories

Cable(s)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
CABLE KEYLOAD MX | Cable for transferring keys between two KVL units. | TKN8209 | 085 | $75.00
CABLE FOR RNC, DIU MGEG | Keyloading cable for APX 7500, XTL 5000, XTL 2500, and ASTRO Spectra. Correct keyloading cable adaptor must be ordered seperately: -HKN6182 for APX 7500, XTL 5000 (O series control head), and XTL 2500. -TRN7414 for XTL 5000 (W series control head) and ASTRO Spectra. | TKN8531C | 362 | $358.00
KVL 3000 DB-9/MODEM CABLE | DB9 -DB25 Cable for KMF Store and Forward via RS232 modem, Cable Part No. 3082013X02. | CKN6324 | 272 | $75.00
KVL CABLE FOR XTS3000 AND MTS2000 | Keyloading cable for XTS 2500, XTS 3000, XTS 5000. Not for XTS 4000. | TDN9390 | 644 | $108.00
KEYLOAD CABLE FOR APX7000 | Keyloading cable for APX 7000 and APX6000. | WPLN6904A | 795 | $119.00
U.S. ROBOTICS USB FAX MODEM - REQD FOR KVL-KMF REMOTE COMMUNICATION | USB MODEM REQUIRED FOR KVL-KMF COMMUNICATION REMOTELY | DSUSR5637MODEM | 708 | $250.00

Case

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
WEATHER CASE FOR KVL | - | NNTN8120A | 201 | $399.00

UNDEFINED

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
KVL 4000 SLEEVE COVER | - | 37009265001 | 201 | $81.00

####

### Ship Card

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
ACCESSORY | CDP | 37009265001 | KVL 4000 SLEEVE COVER | 201 | 15
SYSPERIPH | SCB | CKN6324 | KVL 3000 DB-9/MODEM CABLE | 272 | 15
QUOTEDS | ING | DDN3094 | PWR SUPPLY ADAPTOR PWR BRICK AC DC 3A UNDERGROUNDED 5.4V 16W | 201 | 30
QUOTEDS | ING | DDN3095 | CABLE ASSEMBLY PWR 5.4VDC 3A PWR | 201 | 30
QUOTEDS | ING | DDN3096 | CORD PWR 18AWG 10A 250V UL PWR | 201 | 30
QUOTEDS | ING | DDN3097 | AC PWR CORD FOR US/ROHS PWR | 201 | 30
QUOTEDS | ING | DDN3098 | 3FT US AC LINE CORD/3 WIRE FOR PWR PWRS | 201 | 30
QUOTEDS | ING | DDN3099 | PWR CORD 18AWG 10A 250V PWR AUSTRALIA | 201 | 30
QUOTEDS | ING | DDN3100 | CORD PWR CHINA PWR | 201 | 30
QUOTEDS | ING | DDN3101 | CORD AC PWR 18AWG 3 PLUG BLK PWR 10A BRAZIL | 201 | 30
QUOTEDS | ING | DDN3121 | LINE CORD 18 AWG 250V 1.8M AC EUROPE | 201 | 30
QUOTEDS | SHK | DSPSA1U1EE | INFRASTRUCTURE EQUIPMENT,RUGGED USB CLIENT TO ETHERNET ADAPTER WITH US | 708 | 14
QUOTEDS | PCW | DSUSR5637MODEM | U.S. ROBOTICS USB FAX MODEM - REQD FOR KVL-KMF REMOTE COMMUNICATION | 708 | 10
FIXEDSTN | CDP | NNTN8120A | WEATHER CASE FOR KVL | 201 | 14
PORTABLES | SCB | T7537B | KVL 4000 PDA SNAP-ON | 201 | 51
PORTABLES | SCB | T7672 | KVL 4000 OS HARDENING SW | 201 | 51
PORTABLES | CDP | TDN9390 | KVL CABLE FOR XTS3000 AND MTS2000 | 644 | 9
PORTABLES | CDP | TDN9390 | KVL CABLE FOR XTS3000 AND MTS2000 | 644 | 9
PORTABLES | CDP | TDN9390 | KVL CABLE FOR XTS3000 AND MTS2000 | 644 | 9
PARTS | SCB | TKN8209 | CABLE KEYLOAD MX | 085 | 3
PARTS | SCB | TKN8209 | CABLE KEYLOAD MX | 085 | 3
PARTS | SCB | TKN8209 | CABLE KEYLOAD MX | 085 | 3
PARTS | SCB | TKN8209 | CABLE KEYLOAD MX | 085 | 17
PARTS | SVS | TKN8209 | CABLE KEYLOAD MX | 085 | 4
SYSPERIPH | SVS | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 29
SYSPERIPH | SVS | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 29
SYSPERIPH | SVS | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 29
SYSPERIPH | SVS | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 29
SYSPERIPH | SVS | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 29
SYSPERIPH | SVS | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 29
SYSPERIPH | SVS | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 29
SYSPERIPH | SCB | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 3
SYSPERIPH | SVS | TKN8531C | CABLE FOR RNC, DIU MGEG | 362 | 13
PARTS | SCB | TRN7414 | CBL ADAPTER SPECTRA/SPECTRO | 201 | 63
PORTABLES | PDC | WPLN6904A | KEYLOAD CABLE FOR APX7000 | 795 | 21
PORTABLES | PDC | WPLN6904A | KEYLOAD CABLE FOR APX7000 | 795 | 21
PORTABLES | PDC | WPLN6904A | KEYLOAD CABLE FOR APX7000 | 795 | 9
PORTABLES | CDP | WPLN6904A | KEYLOAD CABLE FOR APX7000 | 795 | 3