Back

##### APX NEXT XE Single Band (4G LTE)

###### Product Catalog

##### Jump to ...

- APX NEXT™ XE Single Band (4G LTE)
- Configuration
- Application Services
- Billing Options
- Software and Provisioning
- HazLoc Approved Accessories (UL Div 2)
- Update History
- Ship Card

Back

##### APX NEXT XE Single Band (4G LTE)

### APX NEXT™ XE Single Band (4G LTE)

Introducing APX NEXT XE Single Band, a radio that allows the flexibility of single or dual band configurations. APX NEXT XE builds on the core and values of APX XE to deliver new and groundbreaking capabilities

MISSION-CRITICAL DEVICE

APX NEXT is designed to military standards for intrinsic ruggedness. The Gorilla Glass 3 touchscreen, combined with a user interface purpose-built for public safety, works with or without gloves - in heat, rain, or snow. Every interaction is simple, fast, and logical, so you can stay focused on what matters most - your mission and your safety.

MOBILE CONNECTION TO INTELLIGENCE

SmartConnect automatically switches between LMR and LTE to extend radio communication beyond the boundaries of the radio system, so users can concentrate on their mission and not worry about coverage.

SmartLocate let’s dispatchers see where everyone under their care is, so they can stay focused on critical situations.

SmartMapping enhances situational awareness by enabling radio users to see their own location on the radio front display, find an address, drop waypoints, and view the locations other colleagues at a glance, then tap the screen to instantly communicate with them.

SmartIncident is a CAD client that gives frontline responders a clear, consolidated view of assignments, unit status updates, map views and multimedia – right on their radio.

SmartMessaging is a secure and convenient way to share texts, images, videos and voice notes across an extended team.

SmartVideo is designed for SVX users to offload critical video to CommandCentral DEMS via the APX NEXT’s LTE. It also allows for users to livestream into CommandCentral Aware via the LTE in APX NEXT.

STREAMLINED OWNERSHIP EXPERIENCE

Radio Central, the cloud based provisioning system, lets you prepare radios before they even arrive and SmartProgramming allows for radio updates to be delivered over broadband regardless of geographic location.

CustomerHub provides direct access to subscriptions, entitlements, warranties and licenses to administer your fleet, and a range of services help you to manage your operations.

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

- New Application service!! SMARTVIDEO is now available on APX NEXT family with the release SR2025.3.

- ViQi Virtual Partner is no longer orderable for new customers. For existing customer add-on orders, contact Order Management. The ViQi Voice Control (QA09028) option will now be included at $0 when ordering separately.

- To arrange for Short Term APX NEXT Customer Demos (60 Days or Less) or Sales Funded APX NEXT Trial Units for Customers, see instructions at: https://drive.google.com/file/d/1vLcX-EQjEq955NmgWJPv1bm4vK0mVYzr/view

- Core Bundle includes AES + ADP encryption (Q629); however, when selecting Custom Configuration, be aware that, effective October 5th, 2020, all U.S. orders will require an encryption selection. Q667 ADP Only is available at $0. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 cost. Please see the encryption section for AES and other encryption options that includes ADP.
- WARNING: Radios shipped with QA05751 Clear Radio No ADP are NOT field-upgradable for encryption, and any changes will require the units to be sent to a Motorola depot.

- Trunking System Key clarification: Software System Key (QA01749) is the default selection for all APX radios. APX NEXT radios ordered with Software Keys (QA01749), can be programmed with either Software keys, Hardware keys or a combination of Software and Hardware keys. APX NEXT radios ordered with Hardware System Key (QA01648), can only be programmed when all Hardware keys are loaded into RadioCentral. Ensure that you make the correct selection based on the type of System Keys your customer is using, as they CANNOT be changed in the field after the radios ship.
- Recommended APX NEXT training classes for new customers:
- APX NEXT Overview ($0) Direct Link to class: AST4002
- APX NEXT Radio Central Overview ($0) Direct Link to class: AST0137
- APX NEXT Features & Service ($0) Direct Link to class: AST4012

Standard Features

All ASTRO Digital APX NEXT™ XE models include the following features:

- Supported bands (700/800MHz, VHF, UHF)

- Front Display: 3.6” TFT Transflective, 24-bit Full Color

- User Interface: Capacitive Touch, immune to false actuation from water, snow, dirt, or grease

- Top Color Display: 1 line of icons, 2 lines of text, 14 characters per line

- 16 Position Mode Rotary Select Switch
- Angled On/Off Volume Knob

- 4 Programmable Side Buttons

- Orange Programmable Button

- Top Mounted Programmable 3 Position Toggle Switch

- 3 Watt Rated Audio

- Wireless Bluetooth® 5.0 (LE) (QA00583)

- LTE (AT&T FirstNet, Verizon, and Bell Mobility Certified)

- ADP Privacy - Single Key (Q667)

- Radio Packet Data (Q947)

- Software Key (QA01749)

- GPS Software & Hardware (QA00782)

- Enhanced Zone Bank (QA01768)

- Adaptive Audio Engine

- 2 High Dynamic Range Microphones

- One Touch/Status Message (H46)

- Radio Trace/Remote Monitor (H43)

- Alias Update over LMR

- Intelligent Noise Reduction (QA010089) with 2025.2 or later release

- ViQi Voice Control

- IP68 (2 m, 2 hr)

Standard Radio configuration includes the following:

- IMPRES 2 Battery 4400 mAh IP68 UL DIV 2 (NNTN9217)*

- All-Band Flexible Antenna (AN000297A01)

- Plastic Carry Holster (PMLN8208A) with 2.5" Belt Clip (NTN8266)

- Side Connector Dust Cover (HW001924A01)

*NOTE: APX NEXT / APX NEXT XE batteries are only compatible with NNTN9199 Single Unit Charger and NNTN9115 6-Slot Multi Unit Charger.

APX NEXT XE radios provide customers with a new ownership experience that allows radio configurations to be set up in a cloud hosted RadioCentral programming tool, even before the radios have physically arrived. On first power up, the APX NEXT XE radios will automatically connnect over WiFi or LTE to the RadioCentral cloud database and download the preset codeplug configuration.

Default radio codeplugs are loaded into the customer's specific cloud database called Provisioning Agency, before the radios ship from the Motorola Solutions factory. A Provisioning Agency will automatically be set up for every customer the first time they purchase APX NEXT XE radios.

When an APX NEXT XE radio is first ordered, the email address of the administrator for the Provisioning Agency has to be entered. That person will receive an email from Motorola Solutions inviting him/her to access the RadioCentral portal and set up other users with access to the Provisioning Agency, so they can program radios going forward.

Information that you will need to place an order:

- Name and Email address of the customer's Technical Contact

- Provisioning Agency name (if the customer has multiple)

- Specify End User Type of who will be the users of the radios for FirstNet Service Eligibility verification (US customers only).
Available categories are: Police Protection; Fire Protection; Ambulance or Other (describe in free-form text)

- System ID for the system on which the APX NEXT XE radios will be deployed. If not known, use "FFFF"

If this is the first time you are quoting APX NEXT or APX NEXT XE to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX NEXT / APX NEXT XE radios and enable the customer system to support the required application services.

#### To ensure accuracy of APX NEXT XE configuration, please create Quotes and Request Orders in CPQ (access through https://motorolasolutions.my.salesforce.com).

### Configuration

####

#### 1. Main Model (Required)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
PORTABLE RADIO APX NEXT SINGLE BAND MODEL 4.5 | 3.6" Touch Display, ( 7/800MHz, VHF, UHF ), LTE, WiFi, GPS, BT, IP68 | H45TGT9PW8AN | 0142 | $7,106.00

#### 1. a. XE Housing (Must Select QA02006 for APX NEXT XE)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX NEXT XE M4.5 RUGGED RADIO | - | QA02006AE | 0437 | $824.00
ALT: APX NEXT XE HOUSING GREEN | - | QA01427AK | 0437 | $30.00

#### 1. b. Primary Band Selection (Required)

Primary band MUST be selected

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 7/800MHZ BAND | 700/800MHz Primary Band | QA00569AP | 0142 | $0.00
ADD: VHF BAND | VHF Primary Band | QA00570AT | 0142 | $0.00
ADD: UHF BAND | UHF Primary band (380-520MHz) | QA00571AR | 0142 | $0.00

#### 1. c. Secondary Band Selection (Optional)

Select one of the secondary band options below for dual-band configurations

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 7/800MHZ BAND+ | 700/800MHz Secondary Band | QA00569AR | 0142 | $856.00
ADD: VHF BAND+ | VHF Secondary Band | QA00570AW | 0142 | $856.00
ADD: UHF BAND+ | UHF Secondary band (380-520MHz) | QA00571AS | 0142 | $856.00

#### 2. Software Bundles (Required)

Core Trunking Bundle must be selected. Security, Operational, and Tactical bundles are optional

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: CORE BUNDLE | Includes: • DIGITAL TRUNKING - SN/SZ P25 Phase I Interop (Q361, Q806; Q173, H38) • TDMA OPERATION (QA00580) • AES ENCRYPTION (Q629) • WIFI CAPABILITY (QA09001) • OUT OF THE BOX WIFI PROVISIONING (QA09007) • ENHANCED DATA (QA03399) • MULTICAST VOTING SCAN (Q387) • ViQi VOICE CONTROL (QA09028) • SUBMERSIBLE DELTA-T (H499) | BD00001AA | 0437 | $3,323.00
ADD: SECURITY BUNDLE | Includes: • ASTRO 25 OTAR W/ MULTIKEY (Q498 and H869) • DES,DES-XL,DES-OFB ENCRYPTION (Q625) • P25 LINK LAYER AUTHENTICATION (QA01767) • DVP-XL ENCRYPTION (H797) • MS OTAR (QA07680) | BD00010AB | 0437 | $1,227.00
ADD: OPERATIONAL BUNDLE | Includes: • DVRS PSU ACTIVATION (QA00631) • MANDOWN OPERATION (QA01843) | BD00015AA | 0437 | $221.00
ADD: TACTICAL BUNDLE | Includes: • PERSONNEL ACCOUNTABILITY (Q445) • DIGITAL TONE SIGNALING (QA09000) | BD00020AA | 0437 | $265.00
ADD: PROVISIONING FEDERAL BUNDLE | Includes PROGRAMING OVER P25 - OTAP (G996) ᐧ FRONT PANEL PROGRAMMING & RADIO TO RADIO ZONE CLONING - FEDERAL (Q52) - MULTIPLE CODEPLUG SUPPORT (QA09772) | BD00040AC | 0437 | $353.00
ADD: PROVISIONING NON-FEDERAL BUNDLE | Includes PROGRAMING OVER P25 - OTAP (G996) ᐧ FRONT PANEL PROGRAMMING & RADIO TO RADIO ZONE CLONING (Q53) - MULTIPLE CODEPLUG SUPPORT (QA09772) | BD00040AD | 0437 | $353.00

Use the link below to see standalone radio software options. Standalone software options CANNOT be combined with the Core Trunking, Security or Operational Assurance bundles above.

- CLICK HERE to see standalone radio software options

#### System Key Software (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: HW KEY SUPPLEMENTAL DATA | WARNING: Software System Key (QA01749) is the default selection for all APX radios. APX NEXT radios ordered with Software Keys (QA01749), can be programmed with either Software keys, Hardware keys or a combination of Software and Hardware keys. APX NEXT radios ordered with Hardware System Key (QA01648), can only be programmed when all Hardware keys are loaded into RadioCentral. Be certain that you are making the correct selection, based on the type of System Keys that your customer is using, as it CANNOT be changed in the field after the radios ship. | QA01648AA | 0655 | $6.42

#### Antenna (Optional)

APX NEXT XE ships standard with the All-Band Flexible antenna (AN000297A01). You may select an alternate antenna from the list below.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ALT: STUBBY 7-800MHZ 6CM ANTENNA | - | QA07710AA | 0437 | $0.00
DEL: DELETE STANDARD ANTENNA | - | H112MC | 0437 | $0.00
ALT: STUBBY UHF 1 380-470MHZ 9CM | 380 - 470 MHz | QA08246AA | 0437 | $0.00
ALT: STUBBY UHF 2 450-527MHZ 9CM | 470 - 520 MHz (when used with APX NEXT XE) | QA08247AA | 0437 | $0.00
ALT: 7/800 MHZ WHIP ANTENNA (762-870MHZ) | Whip Antenna 7/800 MHz (762-870MHz) 16 cm | QA08243AA | 0142 | $0.00
ALT: UHF WHIP ANTENNA (380-520MHZ) | Whip Antenna UHF (380-520MHz) 14 cm | QA08245AA | 0142 | $0.00

#### Battery Selection (Optional)

APX NEXT XE ships standard with the LI-ION IMPRES 2 IP68 4400 mAh UL DIV 2 battery (NNTN9217). You may select an alternate battery from the list below.

NOTE: APX NEXT batteries are only compatible with NNTN9199 Single Unit Charger and NNTN9115 6-Slot Multi Unit Charger.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ALT: BATTERY LI-ION IMPRES 2 IP68 5500T UL DIV 2 XE | PMNN4896A UL2054 DIV 2 IMPRES 2, LiIon, IP68, 5550 mAh Battery | QA10128AB | 0437 | $181.26

#### Carry Accessory (Optional)

APX NEXT XE ships standard with the PLASTIC HOLSTER (PMLN8208A) with 2.5" BELT CLIP (NTN8266) You may select an alternate carry solution from the list below.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ALT: PLASTIC CARRY HOLSTER WITH 3 INCH CLIP | Consists of: PMLN8208A APX NEXT XE PLASTIC HOLSTER and PMLN7965B 3" BELT CLIP | Q698AF | 0437 | $0.00
DEL: DELETE BELT CLIP/BASIC CARRY XE | This option deletes the APX NEXT XE carry holder, PMLN8208, and belt clip. | H301DJ | 0437 | ($10.00)

#### Packaging Selection (Optional)

APX NEXT XE ships standard in Bulk (10 radios per box). Select H842 if you wish to have radios packaged in Individual boxes.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SINGLE UNIT PACKING | - | H842BT | 0437 | $0.00

#### Factory Configuration (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799BH | 0437 | $12.00

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
RadioCentral + CPS Programming (US Gov) | Provides access to RadioCentral programming tool and technical support (annual subscription, order one per radio) | LSV01S03082A | 724 | $32.00
RadioCentral + CPS Programming (FedRAMP) | Provides access to RadioCentral programming tool and technical support (annual subscription, order one per radio) | LSV01S03741A | 724 | $37.00
RadioManagement (MSI Hosted) | Provides access to MSI hosted RM, tech support and software license (requires both part numbers to be ordered) | LSV01S03197A LSV01S03198A | 724 | $32.00
RadioManagement (On-Prem) | See “How to Order” section in the below Ordering Guide. | N/A | N/A | N/A

- Radio Management (On-Prem) Ordering Guide

#### DMS OnSite Setup

Initial onboarding is included with the first time device purchase for APX NEXT and APX N70 and is designed to help customers get started with their programming solution by providing a brief overview and basic training.

We strongly recommend OnSite setup for all new Radio Management (RM) customers which in addition to initial onboarding, also provides initial set-up, deployment and provisioning of their Radio Management system along with hands on training to use the programming tool.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
DMS ONSITE SETUP | Provides customers help with initial set-up provisioning and programming processes, as well as training on the Radio Management tool. | LSV01S02014A | 700 | $30,000.00

#### Device Management Services (DMS)

Includes hardware repair, tech support, firmware updates and MyView access, with the option to add Accidental Damage. Can select 3, 5 or 7 years of coverage. Ordered per device.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
APX NEXT DMS Essential | Provides HW repair, tech support, firmware updates and MyView | LSV01S03446A | 723 | $76.94
APX NEXT DMS Essential with Accidental Damage | Provides accidental damage and HW repair, tech support, firmware updates and MyView | LSV01S03447A | 723 | $150.31

#### Device Managed Services Training (Optional)

Device Management Training provides detailed instruction for radio technicians on how to use our programming solutions, and how to manage a fleet of devices. Upon completing the training, participants will be able to provision and program their APX NEXT radio fleet with confidence. Training includes access to an online overview course, as well as a two-day instructor led workshop.

The instructor led workshop can be delivered in three different ways for each of our Programming Solutions:

#### RadioCentral - Device Management Training

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
APX NEXT DMS TRAINING VIRTUAL (1 SEAT) | RADIOCENTRAL PROGRAMMING VIRTUAL ONLINE TRAINING (1 SEAT) | PSV01S01742A | 0943 | $1,700.00
APX NEXT DMS TRAINING MSI SITE (1 SEAT) | RADIOCENTRAL PROGRAMMING TRAINING AT MOTOROLA SOLUTIONS FACILITY (1 SEAT) | PSV01S01743A | 0943 | $1,700.00
APX NEXT DMS TRAINING CUST SITE (12 SEATS) | RADIOCENTRAL PROGRAMMING TRAINING AT CUSTOMER SITE (12 SEATS) | PSV01S01744A | 0943 | $19,200.00

#### Radio Management - Device Management Training

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
APX DMS TRAINING VIRTUAL (1 SEAT) | RADIO MANAGEMENT PROGRAMMING VIRTUAL ONLINE TRAINING (1 SEAT) | PSV01S01987A | 0943 | $1,500.00
APX DMS TRAINING MSI SITE (1 SEAT) | RADIO MANAGEMENT PROGRAMMING TRAINING AT MOTOROLA SOLUTIONS FACILITY (1 SEAT) | PSV01S01988A | 0943 | $1,500.00
APX DMS TRAINING CUST SITE (12 SEATS) | RADIO MANAGEMENT PROGRAMMING TRAINING AT CUSTOMER SITE (12 SEATS) | PSV01S01989A | 0943 | $18,000.00

### Application Services

If this is the first time you are quoting APX NEXT or APX NEXT XE to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX NEXT / APX NEXT XE radios and enable the customer system to support the required application services.

BYOS (Bring Your Own SIM) is an optional new offering where the customer can order APX NEXT or APX N70 without MSI managed LTE service. The limitation is that the customer has to procure their own LTE service from AT&T FirstNet, Verizon (w/ Priority & Preemption), or Bell Canada.

ViQi Virtual Partner and SmartIncident are not available in Canada.

SmartIncident requires SmartLocate and SmartMapping Application Services to be ordered as well.

Refer to the End-to-End ordering guide below for more details.

Description | Nomenclature | Duration | Single App Service | Bundle of 4+ App Svcs | APC
--- | --- | --- | --- | --- | ---
SMART PROGRAMMING (US Gov) | SSV01S01407A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTCONNECT (US Gov) | SSV01S01406A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTLOCATE (US Gov) | SSV01S01476A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTMESSAGING (US Gov) | SSV01S01906A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTMAPPING (US Gov) | SSV01S01907A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTINCIDENT (US Gov) | SSV01S04311A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTVIDEO (US Gov) | SSV01S05746A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMART PROGRAMMING (FedRAMP) | SWV01S03742A | 1 - 5 years | $166.00 / year | $87.00 / year | 712
SMARTCONNECT (FedRAMP) | SWV01S03743A | 1 - 5 years | $166.00 / year | $87.00 / year | 712
SMARTLOCATE (FedRAMP) | SWV01S03744A | 1 - 5 years | $166.00 / year | $87.00 / year | 712
SMARTMAPPING (FedRAMP) | SWV01S04243A | 1 - 5 years | $166.00 / year | $87.00 / year | 712

#### Application Services (BYOS and/or WiFi)

Description | Nomenclature | Duration | Single App Service | Bundle of 4+ App Svcs | APC
--- | --- | --- | --- | --- | ---
SmartProgramming BYOS/WiFi (US Gov) | SSV01S02190A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartConnect BYOS/WiFi (US Gov) | SSV01S02186A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartLocate BYOS/WiFi (US Gov) | SSV01S02188A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartMapping BYOS/WiFi (US Gov) | SSV01S02242A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmasrtIncident BYOS/WIFI (US Gov) | SSV01S04312A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartMessaging BYOS/WiFi (US Gov) | SSV01S02192A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartVideo BYOS/WiFI (US Gov) | SSV01S05748A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartProgramming BYOS/WiFi (FedRAMP) | SWV01S03745A | 1 - 5 years | $111.00 / year | $87.00 / year | 712
SmartConnect BYOS/WiFi (FedRAMP) | SWV01S03746A | 1 - 5 years | $111.00 / year | $87.00 / year | 712
SmartLocate BYOS/WiFi (FedRAMP) | SWV01S03747A | 1 - 5 years | $111.00 / year | $87.00 / year | 712
SmartMapping BYOS/WiFi (FedRAMP) | SWV01S04244A | 1 - 5 years | $111.00 / year | $87.00 / year | 712

#### Application Services Add-On for Fielded APX NEXT Devices

If a customer wishes to add application services to their existing Service Contract for fielded APX NEXT devices, please engage with your APX NEXT App Service Inside Sales representative found here who will assist with submitting the add-on request.

#### Please refer to the End-to-End ordering guides below to see all components required to enable Application Services.

- SmartConnect
- SmartLocate
- SmartMessaging
- SmartMapping
- SmartIncident
- SmartVideo

### Billing Options

Service Activation Delay

To accommodate the lead time sometimes required for new system deployments and radio configuration, customers may elect to delay the start of the Application Services and Device Managed Services contracts.

Service Activation Delay is available for 30 days after the shipment of radios.

Billing Options

Device purchases are invoiced at the time of shipment.

Service billing options are: Immediate, Annually, Monthly in Arrears (Federal only)

### Software and Provisioning

APX NEXT™ XE Out of the Box Provisioning

RadioCentral™ Factory default codeplugs for all APX NEXT XE radios will be made available to you in a secure cloud application. Motorola Solutions will set up a default account for your agency upon initial device purchase and invite you by email to access MyView (https://myview.motorolasolutions.com) to set up user accounts and download the RadioCentral programming application client.

If you already have an existing log-in for Motorola Command Central, you can use the same credentials to access RadioCentral via https://radiocentral.motorolasolutions.com. If this is the 1st time you will receive an email from Motorola how to set up your initial account.

Follow these steps after your RadioCentral account is activated:

1- Log into RadioCentral. Use the CommandCentral credentials to login RadioCentral URL. You will see the factory default codeplugs for your recently purchased APX NEXT radios

2- Install the R35.00.00 or later CPS on the computer you would like to access RadioCentral. CPS will be utilized as template editor during the Edit/Publish flow in RadioCentral.

3- Build new codeplug or reuse a legacy APX codeplug using RadioCentral. You can pick a proper base factory default codeplug to launch CPS editor, and then launch another CPS to open the reference APX legacy codeplug to drag/drop/copy/paste to reuse whatever configurations to build a new codeplug for your NEXT/N70 radios.

4- Schedule a programming job. Apply the radio configuration to your devices.NOTE: To assure proper device deployment please ensure that your organization has received the radios before scheduling specific programming jobs.

5- Remove the radio from the box, insert a battery and turn on the radio.

APX NEXT XE radios are enabled with LTE service and preset with default Wi-Fi SSID, to wirelessly download radio configurations and updates.

a.Upon power up, the radio will scan for the "Customer1" Network SSID access point with WPA/WPA2 security password of "MotorolaSolutions".

b.If "Customer1" is found, the radio will connect to secure hosted RadioCentral database and download any scheduled configuration. NOTE: Wi-Fi must be connected to the open Internet. If using a firewall, open port 443 for radio programming traffic.

c.If "Customer1" access point cannot be found, the radio will attempt to connect to LTE.

d.LTE connections are open to the internet by default, so if the radio is in LTE coverage, it will connect to secure RadioCentral database and download any pending configuration.

e.If neither Wi-Fi nor LTE is found, the radio will continue scanning for a broadband connection.

For security reasons, it is recommended that the first radio configuration update over "Customer1" access point would remove all default SSIDs and replace them with an agency secure network SSID and password.

For assistance, please call 800-MSI-HELP (800-674-4375).

Special Note for United States - State & Local Markets Only
In accordance with FCC mandate, the APX NEXT XE is restricted to12.5 KHz operation only and does NOT support 25 KHz in the VHF and UHF Bands (excluding T-Band). This applies to customers under Rule Part 90. Customers with FCC waivers can contact their Business Development Representative.

The following LMR features are not supported in APX NEXT XE at this time

H02 | TACTICAL RADIO STW-STUN/KILL
QA09012 | MISSION CRITICAL GEOFENCING
QA00982 | SITE SELECTABLE ALERT FOR P25 TRUNKING
H43 | TRUNKED REMOTE MONITOR
QA09008 | GROUP SERVICES OPTION IS OBSOLETE FOR APX. (The device firmware download is only available through SmartProgramming for APX NEXT. OTA Alias Updates and LMR Group Texting are included in standard configuration)
Display Color Change on channel change |
Transmit Inhibit |
Tactical Inhibit Stun/Kill for Portable (Encode & Decode) |
Phone Encode / Decode (Call/Notification) |
LMR Phone Call from Contacts |
Dynamic ID |
Operational Message |
Inactivity timer for overlay |
Responder Alert -Sensor Hub |
Responder Alert Enhanced Data Delivery |
Responder Alert- Local User, Low Batt and Taser Holder |
Responder Alert - Weapon Fired |
Responder Alert - Vest Piercing via Emergency |
Cached Event Tag upon Reconnect |
Radio Lock, Change Password, Secure Auto Log-on |

### Self-Quieting Spurs

7/800 Mhz | 7/800 Mhz | VHF | VHF | UHF | UHF
--- | --- | --- | --- | --- | ---
Radio Alone | Radio + XVE500 RSM | Radio Alone | Radio + XVE500 RSM | Radio Alone | Radio + XVE500 RSM
- | - | - | 138.5375 | 410.4000 | 403.2000
- |  |  | 142.8250 | 411.2125 | 410.4000
- |  |  | 142.8750 | 428.5250 | 415.5500
- |  |  | 153.6000 | 428.5500 | 415.6000
- |  |  | 160.1125 | 445.8625 | 422.4000
- |  |  | 172.8000 | 456.0000 | 441.6000
- |  |  |  | 460.8000 | 445.8625
- |  |  |  | 463.1500 | 467.4875
- |  |  |  | 467.4875 | 467.5375
- |  |  |  | 471.8250 | 467.5875
- |  |  |  | 480.0000 | 476.1625
- |  |  |  | 489.1375 | 480.0000
- |  |  |  | 501.6000 | 493.4750
- |  |  |  | 506.4250 | 501.6000
- |  |  |  | 506.4750 | 510.8125
- |  |  |  | 518.4000 | 518.4000
- |  |  |  |  | 519.4375

### HazLoc Approved Accessories (UL Div 2)

This information is subject to change. For the latest information on accessories approved for HazLoc environments, please refer to the UL manuals and addendums that ship with every HazLoc approved APX NEXT XE radio.

Audio Accessories | Model
--- | ---
ACCESSORY KIT,SMART 2 WIRE W/TRANS TUBE BLACK | PMLN6129A
ACCESSORY KIT,SMART 2 WIRE W/TRANS TUBE BIEGE | PMLN6130A
ACCESSORY KIT,IMPRES 2 WIRE SURVEILLANCE BLACK | PMLN6127A

Antennas | Model
--- | ---
ANTENNA STUBBY (760-870 MHZ) 65mm | AN000296A01
ANTENNA STUBBY UHF1 (380-470 MHZ) 90mm | AN000369B01
ANTENNA STUBBY UHF2 (450-527 MHZ) 90mm | AN000369B02
ANTENNA WHIP ALLBAND 200mm | AN000297A01
ANTENNA WHIP (762-870MHZ) WHIP 160mm | AN000392A01
ANTENNA WHIP UHF (380-520MHZ) 140mm | AN000393A01

Batteries | Model
--- | ---
BATT, IMPRES GEN2, LIION, IP68, 4400T, UL2054 Div 2 | NNTN9217A
BATT, IMPRESS GEN2 LIION, 1P68 5550T, UL2054 Div 2 | PMNN4896A

### Update History

### Ship Card

- CLICK HERE to see the Latest Lead Time Estimates