Back

##### APX Transportable Base Station

###### Product Catalog

##### Jump to ...

- Model
- Ordering Information
- Configuration
- Ship Card

Back

##### APX Transportable Base Station

### Model

Motorola APX
Transportable Station

### Ordering Information

Note:

- This product is delivered UNASSEMBLED. The radio and its components (which are ordered separately) must be assembled/tested with the Transportable Station by the end user.
- Compatible with APX 8500/6500/4500 Mobiles (ordered separately)
- Compatible with O2, O3, E5, and O7 Control Heads (ordered separately)
- Compatible with 7.5 watt detachable speaker (HSN4038A ordered separately)
- Compatible with magnetic low profile antenna (PAN6003A ordered separately)

#### General Information

The APX™ Transportable Station is a highly versatile, lightweight, rugged, rapid deployment product. It can be deployed as a temporary base station (law enforcement command posts, military deployment, surveillance operations, emergency response teams, fire fighting support). It can also be installed in vehicles when mobile installation without permanent installation is a requirement (rental car) or when mobile covert communication is desired.

The unit is packaged in a lightweight, horizontal, black powder coated, lockable aluminum suitcase. This product provides customers with the versatility of a “Jump and Run” communications package and the flexibility of a semi-fixed or transportable RF station.

It utilizes a standard mid-power APX 7500/6500/4500 mobile, O2/O3/O5/O7 control head, mobile antenna and a mobile speaker (all ordered separately). Two RF ports are available to support dual band. Audio ports are also available for headset, headphone and record operation. Record operation is only supported on the O3 CH configuration.

The APX Transportable Station operates with 110/220VAC or 12VDC power input. The suitcase is equipped with a “mouse-hole” exit for cable routing outside the case, allowing for covert closed case operation.

NOTE: For the O2 CH configuration the speaker cable between the transceiver and the control head must be detached during installation.

#### Features

APX Transportable Station Features

- Carbide Black Powder Coated Aluminum Case 7" tall x 13" deep x 21"wide
- Combination Locking Case
- AC Power Supply Auto Switching 85-250VAC (49-61 Hz)
- AC Power Cable (110VAC)
- 12VDC Vehicle Accessory Power Cable Included

- Closed Case Covert Operation
- Accessory Storage Pouch
- Optional 13' O3 Microphone extension cable(APX7500/6500 mobiles only)

Control Panel Includes

- AC and DC Power Receptacles
- Type "UHF" Female SO 239 Antenna Connectors
- Mobile Radio Mount
- Speaker Receptacle

- Headset Jack (6-pin Hirose)
- Headphone Jack (1/4" Audio Jack)
- Tape Recorder Jack with Plug (Mini-XLR 5 pin)
- Microphone Clip

This case also has a mouse hole exit for cable routing outside the case, allowing for closed case operation.
Ordering: Part number P2096B

### Configuration

#### Models

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
RADIOS SALES MODEL,APX TRANSPORTABLE STATION | APX8500/7500/6500 | P2096B | 570 | $4,500.00

#### Options

####

####

### Ship Card

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
PORTABLES | FSA | P2096 | RADIOS SALES MODEL,APX TRANSPORTABLE STATION | 570 | 204
PORTABLES | FSA | P2096B | RADIOS SALES MODEL,APX TRANSPORTABLE STATION | 570 | 204