Back

##### Mini Mag Antennas

###### Product Catalog

##### Jump to ...

- Model
- Ordering Information
- Configuration
- Ship Card

Back

##### Mini Mag Antennas

### Model

Mini Mag (TM) Antennas

### Ordering Information

#### Features

#### Electrical Specifications

Frequency Range | 806-860 MHZ., 824-895 MHZ., 890-960 MHZ.
Band Width | 60 MHZ.
Gain | 3 dB
Power | 15 Watts Maximum (Intermittent Duty)
VSWR | <2:1
Impedance | 50 Ohms Nominal

#### Mechanical Specifications

Material | Elastomer
Cable Length | 12 Foot RG174/U
Connector | Choice of Mini-UHF, SMA, BNC or TNC
Height | 8.3 Inches
Weight | 5.5 oz.
Base Diameter | 2.3 Inches

#### General Information

The Mini Mag(TM) antenna comes factory tuned and ready to install. The magnetic mount not only provides quick installation, but also quick removal when going through car washes or switching vehicles. ItÕs ideal for applications requiring no holes drilled in the vehicle body. The low profile whip and the small strong magnet are excellent choices for low clearance applications. The single piece elastomer housing means there are no moving parts to install or break. It has been environmentally tested for temperature, humidity, and corrosion. Applications include conventional and trunked mobile radios operating in 800 MHz and 900 MHz. The Mini Magª antenna is covered by a Two Year Limited Warranty. All Warranty claims and questions should be directed to 1-800-422-4210.

### Configuration

#### Models

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ANTENNA 800MHZ MINI MAGNET BLACK | 824-895 MHz., Mini-UHF Connector, Black | RAF4036AMM | 554 | $50.75

####

### Ship Card

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
PARTS | CDP | RAF4036AMM | ANTENNA 800MHZ MINI MAGNET BLACK | 554 | 19