Back

##### CPS Programming Cables

###### Product Catalog

##### Jump to ...

- General Information

Back

##### CPS Programming Cables

### General Information

#### Mobile Data, Programming and Keyloading Cables

Part Number | Description | Used For
--- | --- | ---
HKN6182 | GCAI Cable Adapter For Keyloader | For use with Keyloading Cable TKN8531 to adapt for use with GCAI Port on XTL or APX Moibile Radios.
TKN8531 | Keyload Cable | For use with KVL and XTL or APX Mobiles. Requires HKN6182.
HKN6183 | GCAI RS232 Program/ Flashport Cable (XTL Only) | Programming Mid or High Power Radios through control head or TIB GCAI connector on transceiver.
HKN6184 | GCAI USB Programming/ Flashport Cable | Programming APX and XTL Radios through Microphone GCAI Connector on the M5/O5/O9. On XTL through the GCAI TIB connector on the transceiver for High Power Radios Only. On APX through the GCAI TIB connector on the transceiver for All Mid and High Power Radios. Note: Recommended for High Power O3 Control Heads for Programming. Not recommended as a Data Cable. Not compatible with O9 Control Head for Data.
HKN6122 | RS232 Data cable (XTL Only) | Can also be used for programming Remote Mount Mid or High Power Radio through the J600 TIB Connector.
HKN6160 | 6 ft. RS232 Data Cable (XTL Only) | Data cable and can be used to program Mid Power radios through the J2 Accessory Connector on rear of the radio. Can also program both remote mount Mid Power and High Power radios though the J2 Accessory Connector on the rear of the M5/O5. Cannot be used on a High Power radio with an O3 Control Head. Note: On Dash Mount O5 radios this cable needs to be pinned out if using Speaker or Ignition Sense.
HKN6161 | 20 ft. RS232 Data Cable (XTL Only) | Data cable and can be used to program Mid Power radios through the J2 Accessory Connector on rear of the radio. Can also program both remote mount Mid Power and High Power radios though the J2 Accessory Connector on the rear of the M5/O5. Cannot be used on a High Power radio with an O3 Control Head. Note: On Dash Mount O5 radios this cable needs to be pinned out if using Speaker or Ignition Sense.
HKN6163 | 6 ft. USB Data Cable (APX and XTL) | Data cable and can be used to program Mid Power radios through the J2 Accessory Connector on rear of the radio. Can also program both remote mount Mid Power and High Power radios though the J2 Accessory Connector on the rear of the M5/O5/O9. Cannot be used on a High Power radio with an O3 Control Head. Note: On Dash Mount O5 radios this cable needs to be pinned out if using Speaker or Ignition Sense.
HKN6172 | 15 ft. USB Data Cable (APX and XTL) | Data cable and can be used to program Mid Power radios through the J2 Accessory Connector on rear of the radio. Can also program both remote mount Mid Power and High Power radios though the J2 Accessory Connector on the rear of the M5/O5/O9. Cannot be used on a High Power radio with an O3 Control Head. Note: On Dash Mount O5 radios this cable needs to be pinned out if using Speaker or Ignition Sense.
HKN6177 | 6 ft. USB Data Cable | HPD 1000 - Can also be used as Program/ Flashport Cable
HKN6178 | 16.5 ft. USB Data Cable | HPD 1000 - Can also be used as Program Cable
HKN6180 | RS232 Data Cable | HPD 1000 - Can also be used as Program/ Flashport Cable