Back

##### APX N70

###### Product Catalog

##### Jump to ...

- APX N70™
- Configuration
- Application Services
- Billing Options
- Software and Provisioning
- HazLoc Approved Accessories (UL Div 1)
- Ship Card

Back

##### APX N70

### APX N70™

·

·

·

·

·

Introducing APX N70, a next generation single band portable

Safety and focus on the frontline is paramount. Reliable and intuitive communications, that are rugged and easy to use, are non negotiable for first responders. Clear communications have proven to be lifesaving in critical moments.

Reliable P25 radios must evolve to offer the opportunities for sophisticated features that work within a larger public safety ecosystem. They must deliver actionable intelligence to provide increased situational awareness during any incident.

We’ve designed our APX N70 smart radio explicitly for this purpose. It provides police officers and other public safety personnel the mission-critical communications and real-time information they need to stay connected and respond and safely in any situation.

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

- New Application service!! SMARTVIDEO is now available on APX N70 with the release SR2025.3 MR

- ViQi Virtual Partner is no longer orderable for new customers. For existing customer add-on orders, contact Order Management. The ViQi Voice Control (QA09028) option will now be included at $0 when ordering separately.

- To arrange for Short Term APX N70 Customer Demos (60 Days or Less) or Sales Funded APX N70 Trial Units for Customers, see instructions at: https://drive.google.com/file/d/1vLcX-EQjEq955NmgWJPv1bm4vK0mVYzr/view

- Core Bundle includes AES + ADP encryption (Q629), however when selecting Custom Configuration be aware that all U.S. orders will require an encryption selection. Q667 ADP Only is available at $0. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. Please see the encryption section for AES and other encryption options that include ADP.
- WARNING: Radios shipped with QA05751 Clear Radio No ADP are NOT field-upgradable for encryption and any changes will require the units to be sent to a Motorola depot.

- Trunking System Key clarification: Software System Key (QA01749) is the default selection for all APX radios. APX N70 radios ordered with Software Keys (QA01749), can be programmed with either Software keys, Hardware keys or a combination of Software and Hardware keys. APX N70 radios ordered with Hardware System Key (QA01648), can only be programmed when all Hardware keys are loaded into RadioCentral. Be certain that you are making the correct selection, based on the type of System Keys that your customer is using, as it CANNOT be changed in the field after the radios ship.

- Provisioning Bundles (BD00040AC/BD00040AD) have been updated to include the MULTIPLE CODEPLUG SUPPORT (QA09772) option. When this bundle is selected, the ENH LEVEL 2 (QA01771) option will be added as a separate line item automatically at a 25% discount to match bundle pricing discount.

Standard Features

All ASTRO Digital APX N70™ models include the following features:

- Supported bands (700/800MHz, UHF and VHF)

- ADP Privacy - Single Key (Q667)

- Radio Packet Data (Q947)

- Software Key (QA01749)

- Enhanced Zone Bank (QA01768)

- GPS Software & Hardware (QA00782)

- Wireless Bluetooth® 5.0 (LE) (QA00583)

- ViQi Voice Control

- LTE (AT&T FirstNet, Verizon and Bell Mobility Canada Certified)

- Front Display: 3.0” TFT Transflective, 24-bit Full Color

- User Interface: Capacitive Touch, immune to false actuation from water, snow, dirt or grease

- Top Color Display: 1 line of icons, 2 lines of text, 14 characters per line

- 16 Position Mode Rotary Select Switch
- Angled On/Off Volume Knob

- 4 Programmable Side Buttons

- 6 Programmable Front Buttons

- Orange Programmable Button

- Top Mounted Programmable 3 Position Toggle Switch

- 2 High Dynamic Range Microphones

- IP68 (2 m, 2 hr)

Standard Radio configuration includes the following:

- IMPRES 2 Battery 3200 mAh IP68 (PMNN4816)

- Single Band Antenna (Band dependent)

- Plastic Carry Holster (PMLN8371) with 2.5" Belt Clip (PMLN8507)

- Side Connector Dust Cover (PMHN4429A)

APX N70 radios provide customers with a new ownership experience that allows radio configurations to be set up in a cloud hosted RadioCentral programming tool, even before the radios have physically arrived. On first power up, the APX N70 radios will automatically connnect over WiFi or LTE to the RadioCentral cloud database and download the preset codeplug configuration.

Default radio codeplugs are loaded into the customer's specific cloud database called Provisioning Agency, before the radios ship from the Motorola Solutions factory. A Provisioning Agency will automatically be set up for every customer the first time they purchase APX N70 radios.

When an APX N70 radio is first ordered, the email address of the administrator for the Provisioning Agency has to be entered. That person will receive an email from Motorola Solutions inviting them to access the RadioCentral portal and set up other users with access to the Provisioning Agency, so they can program radios going forward.

Information that you will need to place an order:

- Name and Email address of the customer's Technical Contact

- Provisioning Agency name (if the customer has multiple)

- Specify End User Type of who will be the users of the radios for FirstNet Service Eligibility verification (US customers only).
Available categories are: Police Protection; Fire Protection; Ambulance or Other (describe in free-form text)

- System ID for the system on which the APX N70 radios will be deployed. If not known, use "FFFF"

If this is the first time you are quoting APX N70 to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX N70 radios and enable the customer system to support the required application services.

#### To ensure accuracy of APX N70 configuration, please create Quotes and Request Orders in CPQ (access through https://motorolasolutions.my.salesforce.com).

#### Models

1: Base Radio $8,769.00 List $4,822.95 Disc $3,822.95 w/Trade

Description | Full Description | Nomenclature | APC | Price
PORTABLE RADIO APX N70 7/800 MODEL 4.5 |  | H35UCT9PW8AN | 0022 |
ADD: SMARTZONE OPERATION |  | H38DA | 0437 |
ADD: P25 9600 BAUD TRUNKING |  | Q361CD | 0437 |
ADD: ASTRO DIGITAL CAI OPERATION |  | Q806CH | 0437 |
ADD: DVRS PSU ACTIVATION |  | QA00631AL | 0437 |
ADD: ENHANCED DATA |  | QA03399AK | 0437 |
ADD: TDMA OPERATION |  | QA00580BA | 0437 |
ADD: VIQI VC RADIO OPERATION |  | QA09028AA | 0437 |
ADD: PROGRAMMING OVER P25 (OTAP) |  | G996AU | 0481 |
SOFTWARE LICENSE ENH: TRUNKED RADIO TRACE/ REMOTE MO |  | H43BJ | 0426 |

#### 2. Delete LTE (Optional)

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE LTE | LTE functionality is removed via Software. *Please note, while the hardware will still be LTE capable, the upgrade process to activate a SIM with the device is being developed* | QA08909AA | 0022 | ($500.00)

#### System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: ADAPTIVE NOISE SUPPRESSION | - | QA09006AA | 0579 | $177.00
ADD: ADAPTIVE SPEAKER VOLUME | Includes Rx Volume Leveling & Noise Sensing Volume Control (NSVC) | QA08676AA | 0411 | $177.00
ADD: EXTREME 1-SIDED NOISE REDUCTION | - | QA01833AH | 0481 | $30.00
ADD: P25 LINK LAYER AUTHENTICATION | - | QA01767BL | 0437 | $118.00
ADD: WIFI CAPABILITY | The APX N70 and APX N70 XE radios are enabled with LTE service. However, if LTE coverage is not available, the radios can use a preset default Wi-Fi SSID to wirelessly download radio configurations and updates. • Includes Out of Box Provisioning over WiFi (QA09007) | QA09001AM | 0437 | $353.00
INT: OUT OF THE BOX WIFI PROVISIONING | Requires Wi-Fi (QA09001) | QA09007AL | 0437 | $0.00
SOFTWARE LICENSE ENH: ENHANCEMENT LEVEL 2 | This option increases the limits of some codeplug parameters (ZONES, CHANNELS, SYSTEMS PERSONALITIES, UCL ENTRIES, VOICE ANNOUNCEMENT, ENCRYPTION KEYS). Please refer to the Software Catalog for more details. | QA01771AB | 0481 | $235.00
ADD: INTELLIGENT NOISE REDUCTION | Enhanced audio processing improves speech clarity by reducing ambient noise. Available with 2025.2 | QA10089AA | 0437 | $177.00

#### Encryption Algorithm Types (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | Q667BB | 0430 | $0.00
SOFTWARE LICENSE ENH: AES ENCRYPTION AND ADP | Requires digital operation. P25 CAP Compliant option. Includes ADP. | Q629BD | 0437 | $560.00

#### Multikey Types (Optional)

Description | Full Description | Nomenclature | APC | Price
SOFTWARE LICENSE ENH: MULTIKEY | Required when using more than one encryption algorithm or encryption key | H869DB | 0437 | $388.00
SOFTWARE LICENSE ENH: ASTRO 25 OTAR W/ MULTIKEY | Not compatible with ADP-Only. Includes multikey, trunking OTAR, and Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. | Q498BN | 0437 | $871.00
ADD: MULTI SYSTEM OTAR | Requires Q498 ASTRO 25 OTAR W/ MULTIKEY | QA07680AA | 0655 | $177.00

#### Antenna (Optional)

The APX N70 ships with a standard antenna dependent on frequency [7/800 MHz: AN000411A01, UHF (380-520MHz): AN000452A01, VHF (136 -174MHz): AN000414A01]. You may select an alternate antenna from the list below.

Description | Full Description | Nomenclature | APC | Price
ALT: 7800 STUBBY 762-870MHZ | Replaces 7/800 whip antenna (AN000411A01) with 7/800 stubby antenna (AN000418A01) 10 cm. Will be available October, 2023. | QA08821AA | 0022 | $30.60

#### Battery Selection (Optional)

APX N70 ships standard with the LI-ION IMPRES 2 IP68 3200 mAh battery (PMNN4816). You may select an alternate battery from the list below.

NOTE: APX N70 batteries are only compatible with PMPN4604 Single Unit Charger and PMPN4591 6-Slot Multi Unit Charger.

Description | Full Description | Nomenclature | APC | Price
ALT: BATT IMPRES LIION IP68 4400T | PMNN4817 IMPRES 2, LiIon, IP68, 4400mAh Battery | QA08817AA | 0022 | $217.64
ALT: BATT IMPRES 2 LIION TIA4950 IP68 3650T | PMNN4818 IMPRES 2, LiIon, IP68, TIA4950, 3650mAh Battery. Will be available end of October, 2023. | QA08818AA | 0022 | $243.64
DEL: DELETE BATTERY | - | QA08819AA | 0022 | $0.00

#### Carry Accessory (Optional)

APX N70 ships standard with the PLASTIC HOLSTER (PMLN8371) with 2.5" BELT CLIP (PMLN8507) You may select an alternate carry solution from the list below.

Description | Full Description | Nomenclature | APC | Price
ALT: 3.0" HOLSTER | Consists of: PMLN8317A APX N70 PLASTIC HOLSTER and PMLN8508A 3" BELT CLIP | QA08824AA | 0022 | $13.77
DEL: BELT CLIP | - | QA08825AA | 0022 | ($10.00)

#### Packaging Selection (Optional)

APX N70 ships standard in Bulk (10 radios per box). Select QA08827 if you wish to have radios packaged in Individual boxes.

Description | Full Description | Nomenclature | APC | Price
ADD: SINGLE UNIT PACKAGING | - | QA08827AA | 0022 | $0.00

#### Factory Configuration (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799BH | 0437 | $12.00
ADD: SINGLE UNIT PACKAGING | - | QA08827AA | 0022 | $0.00

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
RadioManagement (On-Prem) | See “How to Order” section in the Ordering Guide below. | N/A | N/A | N/A

#### Device Management Services (DMS)

Includes hardware repair, tech support, firmware updates and MyView access, with the option to add Accidental Damage. Can select 3, 5 or 7 years of coverage. Ordered per device.

Description | Full Description | Nomenclature | APC | Price
APX N70 DMS Essential | Provides HW repair, tech support, firmware updates and MyView | LSV01S03060A | 723 | $68.69
APX N70 DMS Essential with Accidental Damage | Provides accidental damage and HW repair, tech support, firmware updates and MyView | LSV01S03061A | 723 | $133.02

### Application Services

If this is the first time you are quoting APX NEXT to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX NEXT radios and enable the customer system to support the required application services.

BYOS (Bring Your Own SIM) is an optional offering where the customer can order APX NEXT or APX N70 without MSI managed LTE service. The limitation is that the customer has to produce their own LTE service from AT&T FirstNet, Verizon (w/ Priority & Preemption), or Bell Canada.

ViQi Virtual Partner and SmartIncident are not available in Canada.

SmartIncident requires SmartLocate and SmartMapping Application Services to be ordered as well.

Refer to the End-to-End ordering guide below for more details.

#### Application Services (with MSI-provided LTE service)

Description | Nomenclature | Duration | Single App Service | Bundle of 4 App Svcs | APC
SMART PROGRAMMING (US Gov) | SSV01S01407A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTCONNECT (US Gov) | SSV01S01406A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTLOCATE (US Gov) | SSV01S01476A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTMESSAGING (US Gov) | SSV01S01906A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTMAPPING (US Gov) | SSV01S01907A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTINCIDENT (US Gov) | SSV01S04311A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMARTVIDEO (US Gov) | SSV01S05746A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMART PROGRAMMING (FedRAMP) | SWV01S03742A | 1 - 7 years | $166.00 / year | $87.00 / year | 712
SMARTCONNECT (FedRAMP) | SWV01S03743A | 1 - 7 years | $166.00 / year | $87.00 / year | 712
SMARTLOCATE (FedRAMP) | SWV01S03744A | 1 - 7 years | $166.00 / year | $87.00 / year | 712
SMARTMAPPING (FedRAMP) | SWV01S04243A | 1 - 7 years | $166.00 / year | $87.00 / year | 712

#### Application Services (BYOS and/or WiFi)

Description | Nomenclature | Duration | Single App Service | Bundle of 4 App Svcs | APC
SmartProgramming BYOS/WiFi (US Gov) | SSV01S02190A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartConnect BYOS/WiFi (US Gov) | SSV01S02186A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartLocate BYOS/WiFi (US Gov) | SSV01S02188A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartMapping BYOS/WiFi (US Gov) | SSV01S02242A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartIncident BYOS/WIFI (US Gov) | SSV01S04312A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartMessaging BYOS/WiFi (US Gov) | SSV01S02192A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartVideo BYOS/WiFI (US Gov) | SSV01S05748A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartProgramming BYOS/WiFi (FedRAMP) | SWV01S03745A | 1 - 7 years | $111.00 / year | $87.00 / year | 712
SmartConnect BYOS/WiFi (FedRAMP) | SWV01S03746A | 1 - 7 years | $111.00 / year | $87.00 / year | 712
SmartLocate BYOS/WiFi (FedRAMP) | SWV01S03747A | 1 - 7 years | $111.00 / year | $87.00 / year | 712
SmartMapping BYOS/WiFi (FedRAMP) | SWV01S04244A | 1 - 7 years | $111.00 / year | $87.00 / year | 712

#### Application Services Add-On for Fielded APX NEXT Devices

If a customer wishes to add application services to their existing Service Contract for fielded APX NEXT devices, please engage with your APX NEXT App Service Inside Sales representative found here who will assist with submitting the add-on request.

#### Please refer to the End-to-End ordering guides below to see all components required to enable Application Services.

- SmartConnect
- SmartLocate
- SmartMessaging
- SmartMapping
- SmartIncident
- SmartVideo

If this is the first time SmartConnect or SmartLocate are being deployed on the customer's system, please engage your Pre-Sales team to ensure that all system components required to enable the services are ordered.

### Billing Options

Service Activation Delay

To accommodate the lead time sometimes required for new system deployments and radio configuration, customers may elect to delay the start of the Application Services and Device Managed Services contracts.

Service Activation Delay is available for 30 days after the shipment of radios.

Billing Options

Device purchases are invoiced at the time of shipment.

Service billing options are: Immediate, Annually, Monthly in Arrears (Federal only)

### Software and Provisioning

APX N70™ Out of the Box Provisioning

RadioCentral™ Factory default codeplugs for all APX N70 radios will be made available to you in a secure cloud application. Motorola Solutions will set up a default account for your agency upon initial device purchase and invite you by email to access MyView (https://myview.motorolasolutions.com) to set up user accounts and download the RadioCentral programming application client.

If you already have an existing log-in for Motorola Command Central, you can use the same credentials to access RadioCentral via https://radiocentral.motorolasolutions.com. If this is the 1st time you will receive an email from Motorola how to set up your initial account.

Follow these steps after your RadioCentral account is activated:

1- Log into RadioCentral. Use the CommandCentral credentials to login RadioCentral URL. You will see the factory default codeplugs for your recently purchased APX NEXT radios

2- Install the R35.00.00 or later CPS on the computer you would like to access RadioCentral. CPS will be utilized as template editor during the Edit/Publish flow in RadioCentral.

3- Build new codeplug or reuse a legacy APX codeplug using RadioCentral. You can pick a proper base factory default codeplug to launch CPS editor, and then launch another CPS to open the reference APX legacy codeplug to drag/drop/copy/paste to reuse whatever configurations to build a new codeplug for your NEXT/N70 radios.

4- Schedule a programming job. Apply the radio configuration to your devices.NOTE: To assure proper device deployment please ensure that your organization has received the radios before scheduling specific programming jobs.

5- Remove the radio from the box, insert a battery and turn on the radio.

APX N70 radios are enabled with LTE service and preset with default Wi-Fi SSID, to wirelessly download radio configurations and updates.

a.Upon power up, the radio will scan for the "Customer1" Network SSID access point with WPA/WPA2 security password of "MotorolaSolutions".

b.If "Customer1" is found, the radio will connect to secure hosted RadioCentral database and download any scheduled configuration. NOTE: Wi-Fi must be connected to the open Internet. If using a firewall, open port 443 for radio programming traffic.

c.If "Customer1" access point cannot be found, the radio will attempt to connect to LTE.

d.LTE connections are open to the internet by default, so if the radio is in LTE coverage, it will connect to secure RadioCentral database and download any pending configuration.

e.If neither Wi-Fi nor LTE is found, the radio will continue scanning for a broadband connection.

For security reasons, it is recommended that the first radio configuration update over "Customer1" access point would remove all default SSIDs and replace them with an agency secure network SSID and password.

For assistance, please call 800-MSI-HELP (800-674-4375).

Special Note for United States - State & Local Markets Only
In accordance with FCC mandate, the APX N70 family of radios is restricted to12.5 KHz operation only and does NOT support 25 KHz in the VHF and UHF Bands (excluding T-Band). This applies to customers under Rule Part 90. Customers with FCC waivers can contact their Business Development Representative.

The following LMR features are not supported in APX N70 at this time

H02 | TACTICAL RADIO STW-STUN/KILL
QA09012 | MISSION CRITICAL GEOFENCING
QA00982 | SITE SELECTABLE ALERT FOR P25 TRUNKING
H04 | TACTICAL REKEY WITH MULTIKEY
QA09008 | GROUP SERVICES OPTION IS OBSOLETE FOR APX N70. (The device firmware download is only available through SmartProgramming for APX N70. OTA Alias Updates and LMR Group Texting are included in standard configuration)
Site Lock/Unlock (Toggle) |
Display Color Change on channel change |
Transmit Inhibit |
Tactical Inhibit Stun/Kill for Portable (Encode & Decode) |
Radio Uninhibit Conventional system via USB |
Selectable location formats |
Phone Encode / Decode (Call/Notification) |
LMR Phone Call from Contacts |
Dynamic ID |
Operational Message |
Inactivity timer for overlay |
Responder Alert -Sensor Hub |
Responder Alert Enhanced Data Delivery |
Responder Alert- Local User, Low Batt and Taser Holder |
Responder Alert - Weapon Fired |
Responder Alert - Vest Piercing via Emergency |
Cached Event Tag upon Reconnect |
Radio Lock, Change Password, Secure Auto Log-on |

### Self-Quieting Spurs

7/800 MHz
Radio Alone
768
774.8
775.2
775.6
866.4

### HazLoc Approved Accessories (UL Div 1)

This information is subject to change. For the latest information on accessories approved for HazLoc environments, please refer to the UL manuals and addendums that ship with every HazLoc approved APX N70 radio.

Audio Accessories | Model
AUDIO ACCESSORY-REMOTE SPEAKER MICROPHONE,XVP750 RSM | PMMN4141
AUDIO ACCESSORY-REMOTE SPEAKER MICROPHONE,XVP730 RSM | PMMN4142
RM780 IMPRES WINDPORTING REMOTE SPEAKER MICROPHONE, LARGE (IP68) | PMMN4128
RM760 IMPRES WINDPORTING REMOTE SPEAKER MICROPHONE, LARGE (IP68) | PMMN4140
2-WIRE SWIVEL LOUD AUDIO EARPIECE WITH EARTIP | PMLN8295
BEHIND-THE-HEAD HEADSET | PMLN8085
OVER-THE-HEAD HEADSET | PMLN8086
REPLACEMENT CABLE FOR RSM | PMKN4232
RX ONLY XL CLEAR TUBE EARPIECE, 3.5MM JACK | PMLN8120

Antennas | Model
ANTENNA, WHIP, 762-870 MHZ , 15CM, FERRULE | AN000411A01
ANTENNA, STUBBY, 762-870 MHZ, 10CM, FERRULE | AN000418A01
ANTENNA, WHIP, UHF (380-520MHz), 12 CM, FERRULE | AN000452A01
ANTENNA, WHIP, VHF (136 -174MHZ), 14 CM, FERRULE | AN000414A01

Batteries | Model
BATT IMPRES 2 LIION TIA4950 IP68 3650T | PMNN4818A