Back

##### APX 6000

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Software and Services
- Ship Card

Back

##### APX 6000

### Model

APX™ 6000 P25 Portable Radio
700/800 MHz Band
P25 Phase 2 Single Band Capable Radio

### Updates

DHS Project 25 Compliance Assessment Program (CAP) has defined a "CAP Encryption Requirements compliant radio" as a radio that can be ordered without encryption or one that can be ordered with AES256. << Click to learn more>>

Effective February, 2018, the new standard 7/800 MHz whip antenna on the APX 6000 7/800 MHz model will be PMAF4040 instead of NAF5085. PMAF4040 is has a slightly thinner and more flexible form factor.

Effective March, 2018, PMNN4547 IMPRES 2 LIION 3100 MAH will be available for order on all of the APX 6000 models. This battery is slightly larger and will require a new holster, PMLN7901. This holster is now the standard carry holster for the Models 2.5 and Models 3.5 and will fit all of the current batteries in the portfolio. The legacy holster, PMLN5709 is no longer available.

### Ordering Information

Ordering Guide

#### Features

All APX 6000 P25 Portable Radio models include the following features:

- Dual Microphone

- Integrated GPS*
- Mission-Critical Wireless Bluetooth® 4.0 (LE)*
- Detachable belt clip (Model 1.5 Only) / Carry Holster (Models 2.5 & 3.5)
- Li-ion 2550mAh IMPRES 2 Battery
- Antenna (Dependent on Frequency)
- Intelligent Lighting
- IP68

- Three programmable side buttons
- Orange programmable button
- 16-position mode rotary select switch
- Wi-Fi® 802.11 b/g/n*¹
- Angled on/off volume knob
- Low battery alert tone
- Noise cancellation software
- One top-mounted programmable three-position toggle switch
- Top display: one line of text, one line of icons, zero menu lines (8 characters)
- Advanced Digital Privacy (ADP) hardware/ software encryption ships standard w/ single key
- Emergency Find Me¹

####

APX 6000 P25 Portable Radio Limited Keypad and Full Keypad with Dual Display Model also includes:

- Universal carry holder
- Unified call list
- Front color display: four lines of text, two lines of icon (14 characters)

- Radio profiles
- Full keypad: 4x3 alphanumeric 3 programmable button, four-way navigation, home and data buttons

*Must purchase Software to ENABLE.

¹Features only available on the following models (Ship Acceptance August 6th, 2016): H98KGD9PW5BN, H98KGF9PW6BN, H98KGH9PW7BN

New RFID enabled volume knobs (QA04526) available for portable radios. See RFID Enabled Volume Knob section below for more information. See RFID Solution Partner link below for information on partners that can provide customers with scanner hardware and back end asset management solutions.

All APX 6000 P25 Portable Radios are part of the FLASHport® program and ship standard with a FLASH EE Prom, which allows for feature and system upgrades (contingent upon remaining within the current RF capabilities of the radio)

****NOTE: APX Portable and Mobile Radios ship standard with the Software Key (QA01749). The Hardware Key (QA01648) is available as an alternative option to purchase. The System ID is required to be entered as supplemental data when ordering the Hardware Key (QA01648). It is CRITICAL that the CORRECT SYSTEM ID is entered when placing the order as this will impact the radios’ ability to operate on the intended system. If an incorrect System ID is entered, a FLASHport upgrade will be required in order to fix this error. The Master Key Start-Up Kit (DVN4046) is required to use the Hardware Key (QA01648) or to operate on a third-party trunking system if the customer does not already possess one, or if theirs has expired. Please CLICK HERE for further details regarding the DVN4046 Kit.

ASK (Advanced System Key)

#### General Information

Operating Modes

APX 6000 P25 Portable Radio Models are capable of operating in FOUR different voice communication modes:

1. Normal analog (clear voice)
2. 3.6 kB ASTRO digital (both clear and coded voice)
3. 9.6 kB ASTRO 25 digital (both clear and coded voice)
4. 9.6 kB 12.5kHz two-slot digital TDMA (both clear and coded voice)

TDMA
FDMA (Frequency Division Multiple Access) is a proven technology that is widely used today in radio systems and is part of Project 25 Phase 1 standard. FDMA carries one call per channel. TDMA (Time Division Multiple Access) is part of P25 Phase 2 standard and provides double the voice capacity as 2 calls can share 1 channel. Customers can add more users to their systems without the need of additional frequencies or infrastructure. The APX radios support both P25 Phase 1 and TDMA technologies seamlessly. Using Motorola's unique Dynamic Dual Mode (DDM) capability, the radios dynamically switch between FDMA and TDMA without the user having to change channels. This provides interoperability on demand with existing and future networks.

Please note: TDMA X2 is not supported on the APX6000

#### New to APX6000 Models

Wi-Fi

APX 6000 supports Wi-Fi 802.11 b/g/n with WPA2/WPA (PSK), and WEP security protocols. Wi-Fi can be used with the Radio Management SW in order to do codeplug updates, firmware refreshes, and FLASHport upgrades over a Wireless Network (WLAN). The radio will only connect to available Wi-Fi networks which have been pre-provisioned in the radio codeplug via CPS. The radio can be pre-provisioned with up to 20 SSIDs.
The Wi-Fi feature requires ordering option QA09001. The Wi-Fi feature is also available aftermarket as a FLASHport upgrade if not ordered out of the factory.

Radio Management (RM) is required in order to take advantage of the Wi-Fi capabilities on APX 6000.

Out-of-the-box Wi-Fi Provisioning
If a radio is ordered the Wi-Fi option (QA09001) and the customer wishes to provision the radios out of the box using Wi-Fi, the radio must also be ordered with the Out of the Box Wi-Fi Provisioning option (QA09007).
A radio ordered with the Wi-Fi option and the Out of the Box Provisioning over Wi-Fi option will come with the following default codeplug configuration relative to Wi-Fi:
a. Wi-Fi will be enabled.
b. There will be one pre-configured network with the Network SSID set to “MyNetwork” and security type will be set to “None”.
c. The default state of Wi-Fi will be “on”.
A Wi-Fi router is required for connecting the Wi-Fi capable radio to the Device Programmer. The Wi-Fi router is to be procured by the agency programming the radios and must be provisioned with the Network SSID set to “MyNetwork” (case sensitive) with no password enabled.

For more details regarding the Out of the Box Wi-Fi Provisioning process, please refer to the Out of the Box Wi-Fi Provisioning Leaflet.

Bluetooth 4.0 & Emergency Find Me
With Bluetooth 4.0 wireless technology and our APX™ Mission Critical Wireless portfolio, users can now connect a variety of Bluetooth audio accessories and data devices with their APX™ radio.

Bluetooth 4.0 also enables Emergency Find Me, a feature providing personnel with an added level of security by improving response time in emergencies. Once an emergency is activated on the APX 6000, a Bluetooth beacon signals other Bluetooth-enabled APX radios within range. Based on bluetooth signal strength, nearby APX radios will receive an emergency alert via intelligent lighting and a text message with users Radio ID along with signal strength status (excellent, poor, fair) to determine proximity, and will guide the nearest personnel to the user in distress.

Adaptive Audio Engine
By selecting QA09006, the Adaptive Audio Engine option, the APX 6000 is equipped with a 3-watt speaker, 3 integrated microphones and the Adaptive Audio Engine. This changes the level of noise suppression, microphone gain, windporting and speaker equalization to produce clear and loud audio in any environment. QA09006 must be ordered in order to receive this feature.

IMPRES 2
Effective August 2016, the APX6000 comes standard with Q712AY, PMNN4485 SLIM IMPRES 2 LIION 2550MAH battery. Please see below for additional IMPRES 2 Battery Options available for the APX6000. The benefits of this IMPRES 2 technology requires both IMPRES 2 Batteries & IMPRES 2 Chargers. Please see the Accessories Catalog and Accessories ECAT pages for more information on IMPRES 2 technology.

Please note: QA01837 (NNTN7038), QA02021 (PMNN4403), QA00781 (NNTN7034), H335 (NNTN7037), QA02726 (NNTN7573) and Q393 (NNTN7036) are no longer be available on the APX6000.

RUGGED

The RUGGED option (H499JX) is ordered with APX 6000 Enhanced Model Numbers will now meet MIL-STD 512.X/I, IP68 submersion standards for 2 meters for 4 hours. Effective October, 2016, if H499 is selected, the standard battery is still PMNN4485A. If HAZLOC certification is required, please see the HAZLOC battery options below. The following APX6000 batteries are tested for Delta-T/Rugged standards when H499 is ordered: PMNN4485, PMNN4486, PMNN4487, PMNN4494A, NNTN8930, NNTN8921.

#### FLASHport AFTERMARKET UPGRADES

**PLEASE NOTE: The new APX6000 models will not share the same codeplugs as the previous APX6000 models (H98UCD9PW5AN, H98UCF9PW6AN, H98UCH9PW7AN). Direct cloning will not be available. New features, such as Wi-Fi, Bluetooth 4.0, and the Adaptive Audio Engine will not be available as a FLASHport upgrade on the previous APX6000 models (H98UCD9PW5AN, H98UCF9PW6AN, H98UCH9PW7AN).**

The APX 6000 P25 Portable Radios are part of the FLASHport Program. This means that APX 6000 hardware models can be loaded with different software packages that provide the features and functionalities that our customers require.

System Enhancement Options can be loaded at the time of radio purchase or at a later date through the use of software field upgrades (a USB cable is required for all software upgrades.) The APX 6000 portable can be upgraded electronically in the field with new features in the current system or to new systems operation (contingent upon remaining within the same RF sub-band) by ordering upgrade kits.

A new way to upgrade radios in the field launched in early 2015. The previous method, which makes use of the FLASHport USB dongle, will be supported, but for those looking for a more convenient way, a new online method will be supported in Radio Management (RM). For more information, please select APX 6000/APX 6000XE FLASHport in the pulldown select list above.

#### RADIO MANAGEMENT

Radio Management (RM) is a suite of software applications shipping with the APX Customer Programming Software (CPS) that provides the ability to manage your entire fleet of ASTRO APX radios through one central database.

Radio Management (RM) can help reduce fleet programming time and improve overall radio asset management. Radio Management allows:

- Manage and track radio codeplugs through a central database
- Make changes to a shared codeplug template and push to multiple radios
- Manage and update radios without taking them out of service
- Schedule programming updates to radios ahead of time

Note: Radio Management is available only with Customer Programming Software Release 7.12, version R08.02.00 and later and can only be used with ASTRO® Digital APX radios. For more details regarding Radio Management and the Ordering Process, please refer to the ASTRO Radio Management page.

#### FCC Information

#### H98UCD9PW5BN, H98UCF9PW6BN, H98UCH9PW7BN Model Information

Band/Model | Power Output | Transmitter Certification | Emissions | Applicable Rules
--- | --- | --- | --- | ---
700/800 (764-870MHz) | 700 - 1 to 2.5W 800 - 1 to 3W | AZ489FT7086 | 8K10F1D, 8K10F1E, 8K10F1W, 11K0F3E, 16K0F3E, 20K0F1E, 20K0F1E | 90

The FCC is mandating all Public Safety and Industrial/Business licensees convert existing 25 kHz efficiency operations in the VHF and UHF bands to minimum 12.5 kHz efficiency analog or digital operation, and that going forward they implement no more 25 kHz efficiency systems. To implement this mandate, the FCC developed rules and deadlines that impact both radio users and equipment providers.

APX 6000 Enhanced Two-way Radio Specifications Sheet
Enhancement Level Reference Guide
ASTRO 25 Subscriber At A Glance Brochure

RSA Comprehensive

RSA
Portable Accessories Catalog
PSM User Guide

Radio Applications \ Advanced System Key
Fleet Management Ordering Guide
Fleet Management Program Download Information
RFID Solution Partner Information

Fleet Management software was previously distributed on DVDs shipped out of Elgin. It is now downloadable from motsolutions.com at the link below. Look at the right edge of the page under Resources Spotlight. The first link is the Order Guide which tells you what you need. The second link is a free trial version that they can download and evaluate free for 90 days. The third link is the actual program. You need to purchase a license to use it (explained in the order guide).

Accessories for APX 6000 can now be found in the select list pulldown above.

### Software and Services

RADIO WIDE FEATURES
Maximum Modes
APX 6000 Top Display | 96 | 96 | 96 | 96
APX 6000 Limited Keypad | 1000 | 1000 | 1000 | 1000
APX 6000 Full Keypad | 1000 | 1000 | 1000 | 1000
Analog and Digital Operation | Yes | Yes | Yes | Yes
6.25/12.5/20/25 KHz Programmable Channels | Yes | Yes | Yes | Yes
Secure Capable | No | Yes (Digital Only) | Yes (Digital Only) | Yes (Digital Only)
One Touch Operation | Yes | Yes | Yes | Yes
Real Time Clock | Yes | Yes | Yes | Yes
Surveillance Mode | Yes | Yes | Yes | Yes
Keypad Lock | Yes | Yes | Yes | Yes
Radio Lock | Yes | Yes | Yes | Yes
Smart Battery | Yes | Yes | Yes | Yes
Radio Wide Transmit Inhibit | Yes | Yes | Yes | Yes
Time Out Timer | Yes | Yes | Yes | Yes
FLASHport | Yes | Yes | Yes | Yes
ANALOG CONVENTIONAL FEATURES
Conventional Features are additional radio wide features beyond those specified above.
CSQ/PL/DPL | Yes | Yes | Yes | Yes
Dual Priority Channel Scan | Yes | Yes | Yes | Yes
Adaptive Power Control | No | Yes | Yes | Yes
Repeater/Talkaround Operation | Yes | Yes | Yes | Yes
Scan (Auto, Pre-programmed, Operator Selectable) | Yes | Yes | Yes | Yes
Smart PTT | Yes | Yes | Yes | Yes
Monitor | Yes | Yes | Yes | Yes
DTMF Tone Generation | Yes | Yes | Yes | Yes
DTMF Signaling | Future | Future | Future | Future
Quick-Call Signaling | Yes | Yes | Yes | Yes
DIGITAL CONVENTIONAL SIGNALING FEATURES
These features are APCO Project 25 Conventional Interoperable Features when used in the ASTRO Digital CAI Mode (Q806).
Unaddressed Voice Call (Dispatch Call) | Yes | Yes | Yes | Yes
Talk Group Call | Yes | Yes | Yes | Yes
Group Call Alert™ | Yes | Yes | Yes | Yes
Talk Group Identification (TGID) | Yes | Yes | Yes | Yes
Selective Call (Individual Voice Call) | MDC-1200 Only | Yes | Yes | Yes
Selective Call Decode (Individual Voice Call) | MDC-1200 Only | Yes | Yes | Yes
PTT ID (Individual Identification) | MDC-1200 Only | Yes | Yes | Yes
Call Alert Encode/Decode | MDC-1200 Only | Yes | Yes | Yes
Emergency Alarm w/Channel Revert & Ack. | MDC-1200 Only | Yes | Yes | Yes
Telephone Interconnect | Yes | Yes | Yes | Yes
Manual Phone Number Entry | Dual Display Only | Dual Display Only | Dual Display Only | Dual Display Only
Selective Radio Inhibit | MDC-1200 Only | Yes | Yes | Yes
Radio Check | MDC-1200 Only | Yes | Yes | Yes
Status/Message | MDC-1200 Only | Yes | Yes | Yes
Trunking Type II Only Features
Maximum Number of Trunked Systems-20 | Yes | Yes | Yes | Yes
Talkgroup Calls | Yes | Yes | Yes | Yes
PTT ID | Yes | Yes | Yes | Yes
Call Alert Encode/Decode | Yes | Yes | Yes | Yes
Analog/Digital Dual Mode Scan | No | Yes | Yes | Yes
Failsoft by Talkgroup | Yes | Yes | Yes | Yes
Telephone Interconnect Encode/Decode | Yes | Yes | Yes | Yes
System Wide Call (Receive Only) | Yes | Yes | Yes | Yes
Selective Radio Inhibit | Yes | Yes | Yes | Yes
Priority Monitor Scan | Yes | Yes | Yes | Yes
Dynamic Regrouping | Yes | Yes | Yes | Yes
Status/Message | Yes | Yes | Status Only | Status Only
Private/Enhanced Conversation Encode/Decode | Yes | Yes | Yes | Yes
Remote Monitor/Radio Trace | Yes | Yes | Yes | Yes
Reprogram Request | Yes | Yes | Yes | Yes

Trunking Type II Only Features
Voice on Control | - | - | - | -
SmartZone Automatic Site Registration | Yes | Yes | Yes | Yes
SmartZone RSSI Operation | Yes | Yes | Yes | Yes
SmartZone Preferred Site | Yes | Yes | Yes | Yes
SmartZone Forced Site Search | Yes | Yes | Yes | Yes
SmartZone Site Lock/Unlock | Yes | Yes | Yes | Yes
SmartZone Adjacent Control Channel OSW | Yes | Yes | Yes | Yes
Emergency Alarm Call Receive Indication | Yes | Yes | Yes | Yes

Channel Spacing

There are no maximum frequency separation conditions that must be adhered to on the APX 6000 P25 portable radio. Separation of frequencies can be as wide as the allowable band per radio model with no degradation of any performance specifications. If an incorrect antenna is used, degraded performance may be experienced.

Zoned Operation

This option converts APX 6000 P25 portable radios to Zone Operation radios.

For Top Display radios, a maximum of 16 channels (conventional RX and TX pairs or trunking talkgroups) are accessible in a zone. There is a maximum of six accessible zones (96 channels) when zone selection operation is programmed on the 3 position toggle switch and the Zone Bank feature is programmed on a button. The Zone Bank feature allows the 3 position toggle switch to access zones 1-3 or 4-6.

For the Top Display radio there is a maximum of 6 accessible zones, and 16 accessible channels per zone with the overall maximum of 96 channels. For the Dual Display Radios with Limited keypad or Full Keypad, there is a maximum of 50 zones, 625 channels per zone with the overall maximum of 1000 channels. These radios provide "ZONE" and "CHAN" menus that allows access to zones and channels not accessible via the switches.

*Note: Top Display Radio code plugs can be programmed with the same zone/channel configuration as the Dual Display Radios even though not all of the zones and channels are accessible. This is useful for having a common zone/channel template that can be shared between the different radio models.

Project 25 Encryption

Encryption is available for Project 25 voice (Phase 1 FDMA and Phase 2 TDMA) and data communications. The mode of operation is programmed on a channel-by-channel basis. With the coded/clear switch set to the clear mode, the APX 6000 P25 Portable Radio is capable of transmitting clear analog voice or clear (unencrypted) ASTRO Digital voice, depending on the channel programming. With the coded/clear switch set to the coded mode, the APX 6000 P25 Portable Radio is capable of transmitting encrypted CVSD (analog) voice or encrypted ASTRO Digital encryption voice, depending on the channel programming.

An encryption option is not required for either clear analog operation or clear ASTRO Digital operation. Encryption can be ordered with the APX 6000 P25 Portable Radio either as a factory installed option or separate from the radio for later field installation. APX 6000 P25 Portable Radio functions include selected ASTRO digital signaling and digital speech coding.

When ordering any of the Encryption Algorithms:

- The DES-OFB and AES encryption algorithms offered are compliant with Project 25 standards, neither of which support CVSD (analog) encryption operation. These algorithms require ASTRO Digital CAI (Q806) to operate.
- The ADP, DES-XL, and DVP-XL encryption algorithms can operate in CAI digital mode, but will not be compliant with the APCO Project 25 standard.
- The DES, DES-XL, and DVP-XL encryption algorithms can operate in CVSD (analog) mode.
- If ordering multiple encryption options, the Multikey (H869) option is required for purchase.

Additional encryption algorithms can be ordered later via APX MACE Upgrades:

1. If using a KVL 4000, please click here.
2. If using a KVL 3000 Plus, please click here.

FIPS140-2 Compliance

Encryption Modules equipped with AES are FIPS 140-2 compliant. Details regarding the certification, and copies of the relevant certificates, can be obtained on the NIST website at: http://csrc.nist.gov/groups/STM/cmvp/validation.html.

Further information regarding FIPS 140-2 certification may be found using the following link - FIPS 140-2 Crypto Module Validation Program (CMVP) http://csrc.nist.gov/groups/STM/cmvp/index.html

Hazardous Location

UL
The APX 6000 is certified by Underwriters' Laboratory when properly equipped with alternate battery options QA05574, QA005575, QA06304, or QA06305. When equipped with Motorola Batteries NNTN8930A or NNTN8921A, the APX6000 models are certified as intrinsically safe for use in ANSI/TIA 4950-A and CAN/CSA C22.2 NO. 157-92; Classification Rating Class I, Division 1, Groups C, D; Class II, Division 1, Group E, F, G; Class III, Hazardous (Classified) Locations. ANSI/ISA 12.12.01-2015 and CAN/CSA C22.2 No.213-15; Class I, Division 2, Groups A, B, C, D; T3C. Tamb = -25° C to +60° T3C.

APX Series Hazloc Fact Sheet

ASTRO Text Messaging Service
ASTRO Text Messaging Service will be available on APX 6000 Dual Display Portable radios. Text Messaging Service (TMS) allows subscriber users to send and receive text messages to other subscribers or dispatch operators. Users can select messages and addresses from a predefined list or enter freeform text messages and addresses via the keypad. Text Messaging Service is available on ASTRO P25 Conventional and Trunked IV&D Systems and Subscribers.

Text Message is NOT supported on APX 6000 Top Display (Model 1.5) Portable radio.

Ordering ASTRO Text Messaging for APX 6000 Portable Requires:

- APX 6000 Dual Display

- ASTRO Digital CAI Operation (Q806)

- Conventional Operation (H35)

OR

- APX 6000 Dual Display

- ASTRO Digital CAI Operation (Q806)

- SmartZone Operation (H38)

- ASTRO Project 25 Trunking Software (Q361)

NOTE: There is no specific option to order for the Text Messaging Service on the subscribers as the functionality is included in the Packet Data option. Please order Digital Operation to receive Text Messaging ability as Packet Data is a standard feature on APX Portable and Mobile Radios.

Outdoor Personnel Location Global Positioning Satellite (GPS) Feature

The personnel outdoor location tracking GPS feature enables a dispatcher the ability to locate on-foot patrols and out of the vehicle officers who are involved in life threatening situations. The radio user’s GPS position information is sent over the ASTRO 25 Integrated Voice & Data (IV&D) network and is delivered to the dispatch operator using a third party mapping display application at the dispatch center (Mapping Application is not yet available through Motorola at this time, however an Application Developers Tool Kit is available for 3rd party vendors to use to modify existing applications. See link below for more details.) On the Dual Display model only it is possible to the user to determine their own location (latitude/longitude) through the use of the location menu.

During normal operation the radio battery capacity will be reduced by 10 to 16 percent.

In order to obtain an initial GPS fix position, the radio must be located in an open sky, outdoor environment with no barriers that could affect the signal around you or above you. During this initial fix, the radio should NOT be worn on the body as this may affect the process of acquiring signal and/or add additional time to first fix.

Note Limitations of Use:

GPS works best in an open sky (clear view of the sky with no obstructions) environment. Due to the limitations of the technology, there are certain situations which prevent GPS coverage. These situations include but are not limited to:

- Underground locations (tunnels, subways, etc.)
- Inside of buildings, elevators, parking garages, trains, other covered vehicles, etc.
- Under metal or concrete roof structures
- Urban canyons (between tall buildings or under dense tree coverage)

***GPS Performance may be degraded when the radio is worn against the body and/or against the body within a vehicle.

Due to the limitations mentioned above, GPS should only be utilized as a method to assist the user with location information but not as a means for mission critical communication. Therefore, in any emergency situation, the location should always be verbally reported to the dispatcher.

Ordering GPS for APX 6000 P25 Portable Radios requires:

- APX GPS Activation (QA00782)

#### 700/800 MHz Self-quieting Spurs

700/800 Models (1.5, 2.5, 3.5) | AN Model Frequencies | BN Model Frequencies
--- | --- | ---
700 MHz | 767.95 | 768
800 MHz | 855.95 | 775.20

CPS 3-Year Subscription Update

In addition to the traditional 3 Year DVD CPS software subscription (RVN5224 - List $399), we will offer a download-only 3 Year CPS software subscription (HKVN4289A, - List $299) which will provide access to CPS software through your Motorola Online account. Only one subscription per MOL account is needed. The original price of $375 for RVN5224 will increase to $399 on July 1, 2015.

How to order DVD CPS Subscription (RVN5224) through COF:

1. Sign and return the Software License Agreement

2. Order the software part number (RNN5224)

3. New releases on disk will be automatically sent for a three-year period.

How to order Download-Only CPS Subscription (HKVN4289A) through MOL:

1. Call 1-800-422-4210, option 4 (MOL Support Team) to request an MOL account or to add a CPS subscription to an existing account.

2. Sign and return the Software License Agreement through MOL

3. Order HKVN4289A

4. Provide a valid email address; as the 3 year subscription period ends subscription renewal reminders will be sent to this email address.

CPS downloads are only available on MOL for North America. Please see your regional MOL page for information on receiving CPS in other regions.

### Ship Card

Data Not Available

####