Back

##### APX NEXT XE (4G LTE + 5G)

###### Product Catalog

##### Jump to ...

- APX NEXT™ XE (4G LTE + 5G)
- Configuration
- Application Services
- Billing Options
- Software and Provisioning
- HazLoc Approved Accessories (UL Div 2)
- Update History
- Ship Card

Back

##### APX NEXT XE (4G LTE + 5G)

### APX NEXT™ XE (4G LTE + 5G)

·

·

·

·

·

·

APX NEXT™ XE (4G LTE + 5G) is the next-generation of Motorola Solutions’ latest development in our mission to advance the lifeline for public safety communications. Designed to the military-grade standards for maximum toughness and building on the values of APX XE by delivering new and groundbreaking capabilities

MISSION-CRITICAL DEVICE

APX NEXT™ XE (4G LTE + 5G) is designed to military standards for intrinsic ruggedness. The Gorilla Glass 3 touchscreen, combined with a user interface purpose-built for public safety, works with or without gloves - in heat, rain, or snow. Every interaction is simple, fast, and logical, so you can stay focused on what matters most - your mission and your safety.

MOBILE CONNECTION TO INTELLIGENCE

SmartConnect automatically switches between LMR and LTE to extend radio communication beyond the boundaries of the radio system, so users can concentrate on their mission and not worry about coverage.

SmartLocate let’s dispatchers see where everyone under their care is, so they can stay focused on critical situations.

SmartMapping enhances situational awareness by enabling radio users to see their own location on the radio front display, find an address, drop waypoints, and view the locations other colleagues at a glance, then tap the screen to instantly communicate with them.

SmartIncident is a CAD client that gives frontline responders a clear, consolidated view of assignments, unit status updates, map views and multimedia – right on their radio.

SmartMessaging is a secure and convenient way to share texts, images, videos and voice notes across an extended team.

SmartVideo is designed for SVX users to offload critical video to CommandCentral DEMS via the APX NEXT’s LTE. It also allows for users to livestream into CommandCentral Aware via the LTE in APX NEXT.

STREAMLINED OWNERSHIP EXPERIENCE

Radio Central, the cloud based provisioning system, lets you prepare radios before they even arrive and SmartProgramming allows for radio updates to be delivered over broadband regardless of geographic location.

CustomerHub provides direct access to subscriptions, entitlements, warranties and licenses to administer your fleet, and a range of services help you to manage your operations.

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

- New Application service!! SMARTVIDEO is now available on APX NEXT family with the release SR2025.3.

- To arrange for Short Term APX NEXT Customer Demos (60 Days or Less) or Sales Funded APX NEXT Trial Units for Customers, see instructions at: https://drive.google.com/file/d/1vLcX-EQjEq955NmgWJPv1bm4vK0mVYzr/view

- Core Bundle includes AES + ADP encryption (Q629); however, when selecting Custom Configuration, be aware that, effective October 5th, 2020, all U.S. orders will require an encryption selection. Q667 ADP is now available at $0. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 cost. Please refer to the encryption section for details on AES and other encryption options, including ADP.
- WARNING: Radios shipped with QA05751 are not field-upgradable for encryption, and any changes will require the units to be sent to a Motorola depot.

- Trunking System Key clarification: Software System Key (QA01749) is the default selection for all APX radios. APX NEXT radios ordered with Software Keys (QA01749), can be programmed with either Software keys, Hardware keys, or a combination of Software and Hardware keys. APX NEXT radios ordered with Hardware System Key (QA01648) can only be programmed when all Hardware keys are loaded into RadioCentral. Ensure that you make the correct selection based on the type of System Keys your customer is using, as they cannot be changed in the field after the radios ship.

- Recommended APX NEXT training classes for new customers:
- APX NEXT Overview ($0) Direct Link to class: AST4002
- APX NEXT Radio Central Overview ($0) Direct Link to class: AST0137
- APX NEXT Features & Service ($0) Direct Link to class: AST4012

Standard Features

All ASTRO Digital APX NEXT™ XE models include the following features:

- All-Band Capability (UHF, VHF, 7/800)

- Front Display: 3.6” TFT Transflective, 24-bit Full Color

- User Interface: Capacitive Touch, immune to false actuation from water, snow, dirt, or grease

- Top Color Display: 1 line of icons, 2 lines of text, 14 characters per line

- 16 Position Mode Rotary Select Switch

- Angled On/Off Volume Knob

- 4 Programmable Side Buttons

- Orange Programmable Button

- Top Mounted Programmable 3 Position Toggle Switch

- Wireless Bluetooth® 5.0 (LE) (QA00583)

- 4G LTE - AT&T FirstNet, Verizon, T-Mobile and Bell Mobility Certified

- 5G Standalone (SA) - Verizon and T-Moblie Certified

- Dual SIM Hardware Ready (Physical SIM + eSIM)

- ADP Privacy - Single Key (Q667)

- Radio Packet Data (Q947)

- Software Key (QA01749)

- GPS Software & Hardware (QA00782)

- Enhanced Zone Bank (QA01768)
- Adaptive Audio Engine

- 3 Watt Rated Audio

- High Dynamic Range Microphones

- One Touch/Status Message (H46)

- Radio Trace/Remote Monitor (H43)

- Alias Update over LMR

- Intelligent Noise Reduction (QA010089)

- ViQi Voice Control

- IP68 (2 m, 2 hr)

Standard Radio configuration includes the following:

- IMPRES 2 Battery 4400 mAh IP68 UL DIV 2 (NNTN9217)*

- All-Band Flexible Antenna (AN000297A01)

- Plastic Carry Holster (PMLN8935A) with 2.5" Belt Clip (NTN8266)

- Side Connector Dust Cover (HW001924A01)

*NOTE: APX NEXT / APX NEXT XE batteries are only compatible with NNTN9199 Single Unit Charger and NNTN9115 6-Slot Multi Unit Charger.

APX NEXT XE radios provide customers with a new ownership experience that allows radio configurations to be set up in a cloud hosted RadioCentral programming tool, even before the radios have physically arrived. On first power up, the APX NEXT XE radios will automatically connnect over WiFi or LTE to the RadioCentral cloud database and download the preset codeplug configuration.

Default radio codeplugs are loaded into the customer's specific cloud database called Provisioning Agency, before the radios ship from the Motorola Solutions factory. A Provisioning Agency will automatically be set up for every customer the first time they purchase APX NEXT XE radios.

When an APX NEXT XE radio is first ordered, the email address of the administrator for the Provisioning Agency has to be entered. That person will receive an email from Motorola Solutions inviting him/her to access the RadioCentral portal and set up other users with access to the Provisioning Agency, so they can program radios going forward.

Information that you will need to place an order:

- Name and Email address of the customer's Technical Contact

- Provisioning Agency name (if the customer has multiple)

- Specify End User Type of who will be the users of the radios for FirstNet Service Eligibility verification (US customers only).
Available categories are: Police Protection; Fire Protection; Ambulance or Other (describe in free-form text)

- System ID for the system on which the APX NEXT XE radios will be deployed. If not known, use "FFFF"

If this is the first time you are quoting APX NEXT or APX NEXT XE to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX NEXT / APX NEXT XE radios and enable the customer system to support the required application services.

#### To ensure accuracy of APX NEXT XE configuration, please create Quotes and Request Orders in CPQ (access through https://motorolasolutions.my.salesforce.com).

### Configuration

#### 1: Base Radio $13,169.42 List $7,243.18 Disc $6,243.18 w/Trade

Description | Full Description | Nomenclature | APC | Price
PORTABLE RADIO APX NEXT; ALL-BAND MODEL 4.5 |  | H55TGT9PW8BN | 0437 | inc.
ADD: SMARTZONE OPERATION |  | H38DA | 0437 | inc.
ADD: P25 9600 BAUD TRUNKING |  | Q361CD | 0437 | inc.
ADD: ASTRO DIGITAL CAI OPERATION |  | Q806CH | 0437 | inc.
ADD: TDMA OPERATION |  | QA00580BA | 0437 | inc.
ADD: VIQI VC RADIO OPERATION |  | QA09028AA | 0437 | inc.
ADD: ENHANCED DATA |  | QA03399AK | 0437 | inc.
ADD: DVRS PSU ACTIVATION |  | QA00631AL | 0437 | inc.
ADD: PROGRAMMING OVER P25 (OTAP) |  | G996 | 655 | inc.
ADD: HW KEY SUPPLEMENTAL DATA |  | QA01648AA | 0655 | inc.
ADD: CPS ENABLEMENT. |  | QA08853AA | 0437 | inc.
ADD: WIFI CAPABILITY |  | QA09001AM | 0437 | inc.
ADD: OUT OF THE BOX WIFI PROVISIONING |  | QA09007 | 0437 | inc.
ADD: APX NEXT XE M4.5 RUGGED RADIO | - | QA02006AE | 0437 | $824.00
ALT: APX NEXT XE HOUSING GREEN | - | QA01427AK | 0437 | $30.00
ADD: CPS ENABLEMENT. |  | QA08853AA | 0621 | inc.

#### Delete Frequency Bands (Optional)

The "Delete Frequency Bands" option is exclusive to the APX NEXT (4G LTE + 5G) - H55TGT9PW8BN Model.

NOTE: 2 bands may be deleted to make a single band APXNext

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE VHF BAND | Deletes VHF Band | QA05508AB | 0437 | ($800.00)
DEL: DELETE UHF BAND | Deletes UHF (both R1 & R2) Band | QA05509AB | 0437 | ($800.00)

System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 Trunking (Q361) | QA01767 | 655 | $118.00

Algorithm Types (Required)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

Description | Full Description | Nomenclature | APC | Price
CHIFFRAGE AES | Requires digital operation. P25 CAP Compliant option. Includes ADP. | Q629 | 655 | $523.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | Q667BB | 0430 | $0.00

Multikey Types (Optional)

Description | Full Description | Nomenclature | APC | Price
ENH: MULTIKEY | Required when purchasing more than one encryption algorithm or encryption key? "Requires MultiKey". | H869 | 655 | $363.00
MULTICLE OTAR ASTRO P25 | Includes Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. | Q498 | 655 | $814.00
ADD: MULTI SYSTEM OTAR | Requires Q498 ASTRO 25 OTAR W/ MULTIKEY | QA07680AA | 0655 | $177.00

####

#### Antenna (Optional)

APX NEXT XE ships standard with the All-Band Flexible antenna (AN000297A01). You may select an alternate antenna from the list below only if you deleted both VHF and UHF bands.

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE STANDARD ANTENNA | - | H112MC | 0437 | $0.00
ALT: STUBBY 7-800MHZ 6CM ANTENNA | - | QA07710AA | 0437 | $0.00
ALT: 7/800 MHZ WHIP ANTENNA (762-870MHZ) | Whip Antenna 7/800 MHz (762-870MHz) 16 cm | QA08243AA | 0142 | $0.00

#### Battery Selection (Optional)

APX NEXT XE ships standard with the LI-ION IMPRES 2 IP68 4400 mAh UL DIV 2 battery (NNTN9217). You may select an alternate battery from the list below.

NOTE: APX NEXT XE batteries are only compatible with NNTN9199 Single Unit Charger and NNTN9115 6-Slot Multi Unit Charger.

Description | Full Description | Nomenclature | APC | Price
ALT: BATTERY LI-ION IMPRES 2 IP68 5500T UL DIV 2 XE | PMNN4896A UL2054 DIV 2 IMPRES 2, LiIon, IP68, 5550 mAh Battery | QA10128AB | 0437 | $181.26

#### Carry Accessory (Optional)

APX NEXT XE ships standard with the PLASTIC HOLSTER (PMLN8935) with 2.5" BELT CLIP (NTN8266) You may select an alternate carry solution from the list below.

Description | Full Description | Nomenclature | APC | Price
ALT: PLASTIC CARRY HOLSTER WITH 3 INCH CLIP | Consists of: PMLN8935A APX NEXT XE PLASTIC HOLSTER and PMLN7965B 3" BELT CLIP | Q698AG | 0437 | $0.00
DEL: DELETE BELT CLIP/BASIC CARRY XE | This option deletes the APX NEXT XE carry holder, PMLN8208, and belt clip. | H301DJ | 0437 | ($10.00)

#### Packaging Selection (Optional)

APX NEXT XE ships standard in Bulk (10 radios per box). Select H842 if you wish to have radios packaged in Individual boxes.

Description | Full Description | Nomenclature | APC | Price
ADD: SINGLE UNIT PACKING | - | H842BT | 0437 | $0.00

#### Factory Configuration (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: TEST RESULTS / RATED AUDIO PRINTOUT | - | H799BH | 0437 | $12.00

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
RadioManagement (On-Prem) | See “How to Order” section in the below Ordering Guide. | N/A | N/A | N/A

#### Device Management Services (DMS)

Includes hardware repair, tech support, firmware updates and MyView access, with the option to add Accidental Damage. Can select 3, 5 or 7 years of coverage (7 year bundle is 10% cheaper annually). The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
APX NEXT DMS Essential | Provides HW repair, tech support, firmware updates and MyView | LSV01S03446A | 723 | $76.94
APX NEXT DMS Essential with Accidental Damage | Provides accidental damage and HW repair, tech support, firmware updates and MyView | LSV01S03447A | 723 | $150.31

### Application Services

If this is the first time you are quoting APX NEXT or APX NEXT XE to a customer or you are quoting a new application service to the customer, consult your Pre-Sales Engineer to assess the need for SI Services to program APX NEXT / APX NEXT XE radios and enable the customer system to support the required application services.

BYOS (Bring Your Own SIM) is an optional new offering where the customer can order APX NEXT or APX N70 without MSI managed LTE service. The limitation is that the customer has to procure their own LTE service from AT&T FirstNet, Verizon (w/ Priority & Preemption), or Bell Canada.

ViQi Virtual Partner and SmartIncident are not available in Canada.

SmartIncident requires SmartLocate and SmartMapping Application Services to be ordered as well.

Refer to the End-to-End ordering guide below for more details.

Description | Nomenclature | Duration | Single App Service | Bundle of 4+ App Svcs | APC
SMART PROGRAMMING (US Gov) | SSV01S01407A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTCONNECT (US Gov) | SSV01S01406A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTLOCATE (US Gov) | SSV01S01476A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTMESSAGING (US Gov) | SSV01S01906A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTMAPPING (US Gov) | SSV01S01907A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTINCIDENT (US Gov) | SSV01S04311A | 1 - 5 years | $144.00 / year | $75.00 / year | 712
SMARTVIDEO (US Gov) | SSV01S05746A | 1 - 7 years | $144.00 / year | $75.00 / year | 712
SMART PROGRAMMING (FedRAMP) | SWV01S03742A | 1 - 5 years | $166.00 / year | $87.00 / year | 712
SMARTCONNECT (FedRAMP) | SWV01S03743A | 1 - 5 years | $166.00 / year | $87.00 / year | 712
SMARTLOCATE (FedRAMP) | SWV01S03744A | 1 - 5 years | $166.00 / year | $87.00 / year | 712
SMARTMAPPING (FedRAMP) | SWV01S04243A | 1 - 5 years | $166.00 / year | $87.00 / year | 712

#### Application Services (BYOS and/or WiFi)

Description | Nomenclature | Duration | Single App Service | Bundle of 4+ App Svcs | APC
SmartProgramming BYOS/WiFi (US Gov) | SSV01S02190A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartConnect BYOS/WiFi (US Gov) | SSV01S02186A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartLocate BYOS/WiFi (US Gov) | SSV01S02188A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartMapping BYOS/WiFi (US Gov) | SSV01S02242A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartIncident BYOS/WIFI (US Gov) | SSV01S04312A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartMessaging BYOS/WiFi (US Gov) | SSV01S02192A | 1 - 5 years | $96.00 / year | $75.00 / year | 712
SmartVideo BYOS/WiFI (US Gov) | SSV01S05748A | 1 - 7 years | $96.00 / year | $75.00 / year | 712
SmartProgramming BYOS/WiFi (FedRAMP) | SWV01S03745A | 1 - 5 years | $111.00 / year | $87.00 / year | 712
SmartConnect BYOS/WiFi (FedRAMP) | SWV01S03746A | 1 - 5 years | $111.00 / year | $87.00 / year | 712
SmartLocate BYOS/WiFi (FedRAMP) | SWV01S03747A | 1 - 5 years | $111.00 / year | $87.00 / year | 712
SmartMapping BYOS/WiFi (FedRAMP) | SWV01S04244A | 1 - 5 years | $111.00 / year | $87.00 / year | 712

#### Application Services Add-On for Fielded APX NEXT Devices

If a customer wishes to add application services to their existing Service Contract for fielded APX NEXT devices, please engage with your APX NEXT App Service Inside Sales representative found here who will assist with submitting the add-on request.

#### Please refer to the End-to-End ordering guides below to see all components required to enable Application Services.

- SmartConnect
- SmartLocate
- SmartMessaging
- SmartMapping
- SmartIncident
- SmartVideo

### Billing Options

Service Activation Delay

To accomodate the lead time sometimes required for new system deployments and radio configuration, customers may elect to delay the start of the Application Services and Device Managed Services contracts.

Service Activation Delay is available for 30 days after the shipment of radios.

Billing Options

Device purchases are invoiced at the time of shipment.

Service billing options are: Immediate, Annually, Monthly in Arrears (Federal only)

Special Note for United States - State & Local Markets Only
In accordance with FCC mandate, the APX NEXT XE is restricted to12.5 KHz operation only and does NOT support 25 KHz in the VHF and UHF Bands (excluding T-Band). This applies to customers under Rule Part 90. Customers with FCC waivers can contact their Business Development Representative.

The following LMR features are not supported in APX NEXT XE at this time

H02 | TACTICAL RADIO STW-STUN/KILL
QA09012 | MISSION CRITICAL GEOFENCING
QA00982 | SITE SELECTABLE ALERT FOR P25 TRUNKING
QA09008 | GROUP SERVICES OPTION IS OBSOLETE FOR APX. (The device firmware download is only available through SmartProgramming for APX NEXT. OTA Alias Updates and LMR Group Texting are included in standard configuration)
Display Color Change on channel change |
Transmit Inhibit |
Tactical Inhibit Stun/Kill for Portable (Encode & Decode) |
Phone Encode / Decode (Call/Notification) |
LMR Phone Call from Contacts |
Dynamic ID |
Operational Message |
Inactivity timer for overlay |
Responder Alert -Sensor Hub |
Responder Alert Enhanced Data Delivery |
Responder Alert- Local User, Low Batt and Taser Holder |
Responder Alert - Weapon Fired |
Responder Alert - Vest Piercing via Emergency |
Cached Event Tag upon Reconnect |
Radio Lock, Change Password, Secure Auto Log-on |

### Self-Quieting Spurs

7/800 Mhz | 7/800 Mhz | VHF | VHF | UHF | UHF
Radio Alone | Radio + XVE500 RSM | Radio Alone | Radio + XVE500 RSM | Radio Alone | Radio + XVE500 RSM
- | - | - | 138.5375 | 410.4000 | 403.2000
- |  |  | 142.8250 | 411.2125 | 410.4000
- |  |  | 142.8750 | 428.5250 | 415.5500
- |  |  | 153.6000 | 428.5500 | 415.6000
- |  |  | 160.1125 | 445.8625 | 422.4000
- |  |  | 172.8000 | 456.0000 | 441.6000
- |  |  |  | 460.8000 | 445.8625
- |  |  |  | 463.1500 | 467.4875
- |  |  |  | 467.4875 | 467.5375
- |  |  |  | 471.8250 | 467.5875
- |  |  |  | 480.0000 | 476.1625
- |  |  |  | 489.1375 | 480.0000
- |  |  |  | 501.6000 | 493.4750
- |  |  |  | 506.4250 | 501.6000
- |  |  |  | 506.4750 | 510.8125
- |  |  |  | 518.4000 | 518.4000
- |  |  |  |  | 519.4375

### HazLoc Approved Accessories (UL Div 2)

This information is subject to change. For the latest information on accessories approved for HazLoc environments, please refer to the UL manuals and addendums that ship with every HazLoc approved APX NEXT XE radio.

#### Audio Accessories

Description | Full Description | Nomenclature | APC | Price
XVE500 DIV 1 REMOTE SPEAKER MIC, HIGH IMPACT GREEN WITHOUT KNOB, UL | - | PMMN4152A | 372 | $707.00
XVE500 DIV 1 REMOTE SPEAKER MIC, BLACK WITHOUT KNOB, UL | - | PMMN4152ABLK | 372 | $756.00
XVE500 DIV 1 REMOTE SPEAKER MIC, HIGH IMPACT GREEN WITH KNOB, UL | - | PMMN4154A | 372 | $748.00
XVE500 DIV 1 REMOTE SPEAKER MIC, BLACK WITH KNOB, UL | - | PMMN4154ABLK | 372 | $800.00

Antennas | Model
ANTENNA STUBBY (760-870 MHZ) 65mm | AN000296A01
ANTENNA STUBBY UHF1 (380-470 MHZ) 90mm | AN000369B01
ANTENNA STUBBY UHF2 (450-527 MHZ) 90mm | AN000369B02
ANTENNA WHIP ALLBAND 200mm | AN000297A01
ANTENNA WHIP (762-870MHZ) WHIP 160mm | AN000392A01
ANTENNA WHIP UHF (380-520MHZ) 140mm | AN000393A01

Batteries | Model
BATT, IMPRES GEN2, LIION, IP68, 4400T, UL2054 Div 2 | NNTN9217A
BATT, IMPRESS GEN2 LIION, 1P68 5550T, UL2054 Div 2 | PMNN4896A

###