Back

##### APX 6000Li Family

###### Product Catalog

##### Jump to ...

- Models
- Updates
- Configuration
- Software and Services
- Ship Card

Back

##### APX 6000Li Family

### Models

·

·

·

·

·

·

·

APX™ 6000Li P25 Portable Radio P25 Phase 2 Single Band Capable Radio

### Updates

#### Announcements

Effective March 5th, 2020: All U.S. orders will book as P25 CAP Compliant by internally generating the P25 “clear” non-encryption option QA05751 (Disable Encryption) if no other encryption is selected. ADP will no longer ship standard. It will now be an orderable option (G193 for mobiles, Q667 for portables). Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.

### Ordering Information

#### Standard Features

All ASTRO Digital APX 6000Li models include the following features:

- GPS Software & Hardware (QA00782)

- Mission Critical Wireless Bluetooth® 4.0 (LE) (QA00583)

- ADP Privacy - Single Key

- Radio Packet Data (Q947)

- Software Key (QA01749)

- 3 Programmable Side Buttons
- Orange Programmable Button
- 16 Position Mode Rotary Select Switch
- Angled On/Off Volume Knob
- 1 Top Mounted Programmable 3 Position Toggle Switch

- Top Display: 1 line of text, 1 line of icons, 0 menu lines
- Dual Microphone

- Detachable Belt Clip (Model 1.5) / Carry Holder (Models 2.5 & 3.5)

- IMPRES 2 Battery (PMNN4485)

- IP 68 (2m, 2hr)

- Single-Band Antenna (dependent on model/frequency selected)

- Models 2.5 & 3.5:

- Unified Call List
- Front Color Display: 4 Lines of Text, 2 Lines of Icons
- Radio Profiles
- 3 Programmable Buttons
- 4-Way Navigation
- Home & Data Buttons

- Model 3.5: 4 X 3 Alpha-Numeric Keypad

#### APX 6000Li Limitations

- No Infrastructure OTAR Capability

- No Delta T (H499)

- No Color Housing (Yellow/H64 or Green/QA01427)

- No Multiple Encryption Algorithms (not including ADP) such as AES and DES

- No 3600/9600 Interoperability Option

- No Enhanced Level 2 Option Available

- No WiFi (QA09001) Option Available

- No Audio Adaptive Engine (QA09006) Option Available

### Configuration

#### Models

1: Base Radio $7,415.42 List $4,078.48 Disc $2,828.48 w/Trade

Description | Full Description | Nomenclature | APC | Price
APX6000 700/800 MODEL 3.5 PORTABLE | - | H98UCH9PW7BN | 481 |
ADD: 9600 TRUNKING OR 3600 DIGITAL TRUNKING |  | QA02756 | 755 |
ADD: TDMA OPERATION |  | QA00580 | 481 |
ADD: PROGRAMMING OVER P25 (OTAP) |  | G996AU | 0481 |
ADD: ENHANCED DATA APX |  | QA03399 | 656 |
ADD: DVRS PSU ACTIVATION |  | QA00631 | 655 |
ENH: RADIO TRACE/ REMOTE MONITOR |  | H43 | 481 |
ADD: GROUP SERVICES |  | QA09008 | 655 |
ADD: HW KEY SUPPLEMENTAL DATA |  | QA01648AA | 0655 |

RFID Enabled Volume Knob (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: RFID KNOB | Compatible with APX6000, APX7000 & APX8000. Portable radio volume knob with embedded RFID tag making it easier to track assets. When option is ordered, RFID Volume knob will come in the box with the portable radio and other ordered accessories but RFID knob will not be assembled to the radio. AFTERMARKET purchase through Parts department for fielded radios NNTN8646 (APX6000/APX7000/APX8000) and NNTN8647 (APX6000XE/APX7000XE/APX8000XE). See RFID Solution Partner link for information on partners that can provide customers with scanner hardware and back end asset management solutions. | QA04526 | 655 | $30.00

#### System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: P25 LINK LAYER AUTHENTICATION | Requires P25 Trunking (Q361) | QA01767 | 481 | $118.00
ENH: ONE TOUCH/STATUS MSG | Compatible on models 1.5, 2.5 and 3.5. | H46 | 481 | $83.00
ADD: FRONT PANEL PROGRAMMING & CLONING | Compatible with Model 3.5 Radios only. Requires FPP HW dongle (NNTN7526A)to be purchased. | Q53 | 481 | $165.00
ADD: FRONT PANEL PROGRAMMING & CLONING (FEDERAL) | Compatible with Model 3.5 Radios only. | Q52 | 481 | $165.00
ADD: MISSION CRITICAL GEOFENCING | Requires GPS (QA00782). | QA09012 | 426 | $177.00
ADD: EXTREME 1-SIDED NOISE REDUCTION | Compatible with all APX6000 Radios. Comes standard on APX6000XE. | QA01833AH | 0481 | $30.00

Algorithm Types (one must be selected)
AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM.

Description | Full Description | Nomenclature | APC | Price
ENH: AES ENCRYPTION AND ADP | Requires digital operation. P25 CAP Compliant option. Includes ADP. | Q629 | 481 | $523.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | Q667BB | 0430 | $0.00

Multikey Types (Optional)

Description | Full Description | Nomenclature | APC | Price
ENH: MULTIKEY | Required when using more than one encryption algorithm or encryption key | H869 | 481 | $363.00

Antenna (Optional)

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE STANDARD ANTENNA | For APX6000/Li/XE, deletes standard antenna. PMAF4040 (7/800), NAR6593 (VHF) or PMAE4065 (UHF). | H112 | 481 | ($10.00)
ALT: 1/4- WAVE 7/800 GPS STUBBY (NAR6595A | 7/800 Models Only | H122 | 481 | $28.00

#### Battery (Optional- Can Only Select One)

HAZLOC Approved

Description | Full Description | Nomenclature | APC | Price
ALT: BATT IMPRES 2 LIION TIA4950 IP68 3100T STD | This option will delete the standard battery and replace it with LIION IMPRES 3100MAH (PMNN4547). | QA07577 | 481 | $167.00
ALT: LI-ION IMPRES 2 4500 MAH UL/CSA (NNTN8921A) | This option will delete the standard battery and replace it with LIION IMPRES 4500MAH (NNTN8921). | QA05575 | 655 | $165.00

Not Compatible if HAZLOC Certification is Required.

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE STANDARD BATTERY | Deletes the standard SLIM IMPRES 2 LIION 2550MAH battery for the APX6000/Li AN/BN Models, or the standard LIION IMPRES 2 LIION 2650MAH battery for the APX6000XE AN/BN Models. | H207 | 481 | ($30.00)
ALT: LI-ION IMPRES 2 IP68 3400 MAH | This option will delete the standard battery and replace it with IMPRES 2 LIION 3400MAH(PMNN4486). Compatible with all APX6000/XE/Li & SRX2200 AN & BN model numbers. Compatible with the APX7000XE. | QA05570 | 562 | $124.00
ALT: LI-ION IMPRES 2 IP68 4850 MAH | This option will delete the standard battery and replace it with IMPRESS 2 LIION 4850MAH (PMNN4487). | QA05571 | 655 | $143.00
ALT: LI-ION IMPRES 2 IP68 5100MAH | This option will delete the standard battery and replace it with IMPRESS 2 LIION 5100MAH (PMNN4494). | QA05573 | 655 | $167.00

Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: APX DATA CABLE | PMKN4012B- Used to program the radio with Customer Programming Software and Tuner Software. PMKN4013C - Used to program and service the radio with Customer Programming Software and Tuner Software. Compatible on ALL APX Portable Radios | Q157 | 655 | $89.00

Belt Clips (Optional-Can Only Select One)

Description | Full Description | Nomenclature | APC | Price
ALT: BASIC CARRY HOLDER (PMLN7901) | This carry holder equipped with a 2.5 in. belt clip ships standard with the Dual Display models. It is an alternative to the Belt Clip that ships standard with the Top Display model. | QA00779 | 481 | $34.00
ADD: BELT CLIP 3.0" (HLN6875) | Replaces the standard 2.5 in. belt clip that ships with the Model 1.5 radio with a 3 in.. Model 1.5 radios in 700/800 and VHF will ship standard with the 2.5 in. belt clip, and UHF radios will ship with the 3 in. belt clip. | QA01222 | 481 | $14.00

Packaging (Optional)

#### Service Options (Must Select One)

Description | Full Description | Nomenclature | APC | Price
ADD: 3Y ESSENTIAL SERVICE | Provides 3 years of hardware coverage beginning at time of purchase. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | H885BK | 185 | $133.00
ADD: 3Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 3 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00022AB | 185 | $272.00
ADD: 5Y ESSENTIAL SERVICE | Provides 5 years of hardware coverage beginning at time of shipment. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | Q887 | 185 | $222.00
ADD: 5Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 5 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00025AG | 185 | $454.00
ADD: 7Y ESSENTIAL SERVICE HTP | - | HA00690 | 185 | $386.00
ADD: 7Y ESSENTIAL W ACC DMG HTP | - | HA00691 | 185 | $729.00

Documentation (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: DATA LINK MANAGER APP CD- PORTABLES | Option provides the NVN5424 Data CD. Please order this option if you would like the Data CD, and are unable to obtain it through other sources such as MOL. | QA00205 | 655 | $0.00

### Software and Services

Bluetooth 4.0 & Emergency Find Me

With Bluetooth 4.0 wireless technology and our APX™ Mission Critical Wireless portfolio, users can now connect a variety of Bluetooth audio accessories and data devices with their APX™ radio.

Bluetooth 4.0 also enables Emergency Find Me, a feature providing personnel with an added level of security by improving response time in emergencies. Once an emergency is activated on the APX 6000, a Bluetooth beacon signals other Bluetooth-enabled APX radios within range. Based on bluetooth signal strength, nearby APX radios will receive an emergency alert via intelligent lighting and a text message with users Radio ID along with signal strength status (excellent, poor, fair) to determine proximity, and will guide the nearest personnel to the user in distress.

#### Self-Quieting Spurs

7/800 Frequencies | VHF Frequencies | UHF R1 Frequencies | UHF R2 Frequencies
768 | 136.8 | 384 | 456
775.2 | 144 | 396.8 | 480
866.4 | 153.6 | 403.2 | 493.545

###