Back

##### APX 6500Li

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Software and Services
- Update History

Back

##### APX 6500Li

### Model

ASTRO® Digital APX 6500Li Mobile Subscriber
700/800 MHz (10 – 35 Watts)
VHF - 136 -174 (10-50 Watts)
UHFR1 - 380-470 (10-40 Watts)
UHF R2 450-520 (10-45 Watts)

Secure and Trunked Radio Systems

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

- CLICK HERE to see the Latest Lead Time Estimates

####

Effective October 11th, 2021: APX Mobile One Touch Feature will be enhanced and integrated with DEK’s Status Message functionalities. Users will benefit from the ability to program and assign alias Status Messages on the APX Control Head display. One Touch Feature G683 pricing will increase from $75 to $125.

Effective October 5th, 2020: All U.S. orders will require an encryption selection. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. G193/Q667 ADP only is also available at $0. Please see encryption section for AES and other encryption options that come with ADP. Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.

Effective June 19th, 2020: The O5 control head (option G442 and kit H1904) have been canceled and replaced by the E5 GA01670 and H1930

Special Note for United States - State & Local Markets:

In accordance with FCC mandate, the U1/U2 Mid Power and U1/7-800 band combinations for this product are restricted to not allow programming for 25 KHz operation. These frequencies are restricted to 12.5 KHz operation only.

### Ordering Information

#### Please Read All Option Descriptions Before Making Your Selection

Required Selections:

1) Main Model

2) Mounting

3) Control Head Selection

4) RF Antenna

5) Operation Mode

6) Feature Antenna(s)

7) Encryption

8) Remote Mount Cables (if remote mount is selected)

9) Microphone

10) Speaker

11) Service

Please note, the APX 6500Li does not support Motorcycle Configuration.

#### Additional Ordering Information for Service Options

ViQi Virtual Partner End to End Ordering Guide

### Configuration

#### 1. Main Model (Must Select One)

Special Note for United States - State & Local Markets: In accordance with FCC mandate, the U1/U2 Mid Power and U1/7-800 band combinations for this product are restricted to not allow programming for 25 KHz operation. These frequencies are restricted to 12.5 KHz operation only.

#### 2. Mounting (Must Select One)

If a remote mount cable other than 5 meters (17ft) is desired for G67, please reference the "Remote Mount Cables" section.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DASH MOUNT | Required for Control Station Operation. | G66 | 656 | $138.00

#### Control Station Operation (Optional)

O2 & E5 Control Heads Only. Must select one.

Requires Dash Mount (G66)

Some microphones are not compatible with Control Station Operation. Please read descriptions carefully.

Although the Power Supply is optional, it is needed for a full Control Station solution.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: CONTROL STATION POWER SUPPLY | Corresponding kit: HPN4007 | G91 | 656 | $296.00

#### 3A Control Head Software (Required)

#### 3B Control Head Options (Must select one)

O2 Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD:IMPACT GREEN COLOR HOUSING (O2) | When ordered in conjunction with GA00804 you will get a green colored O2 housing. | G201 | 656 | $28.00
ADD: SCHOOL SERCURITY ENHANCEMENT PACKAGE | Education O2 Emergency Push Button | GA01056 | 514 | $55.00

E5 Control Head Option

No Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX NO O2/O7 CH NEEDED MTCL | Requires remote mounting option (G67 or G655) | G88 | 656 | $0.00

#### 4. RF Antenna (Required)

No Antenna Requested

7/800 Antennas

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANT 3DB LOW-PROFILE 762-870 | Corresponding kit: HAF4013 | G174 | 656 | $47.00
ADD: ANT 1/4 WAVE 762-870 MHZ | Corresponding kit: HAF4016 | G335 | 656 | $15.00
ADD: ANT 3DB ELEVATED FEED 762-870 | Corresponding kit: HAF4014. | G175 | 656 | $83.00
ALT: ANT 3DB GAIN 762-870MHZ | Corresponding kit: HAF4017. | W484 | 656 | $42.00

VHF Antennas

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 3BD ANT 136-174MHZ | Corresponding kit: HAD4022A. | G301 | 656 | $64.00
ADD: 1/4 WAVE WHIP ROOF TOP 136-144 | Corresponding kit: HAD4006 | G296 | 656 | $15.00
ADD: 1/4 WAVE ROOF TOP 144-150.8 | Corresponding kit: HAD4007 | G297 | 656 | $15.00
ADD: 1/4 WAVE ROOF TOP 150.8-162 | Corresponding kit: HAD4008 | G299 | 656 | $21.00
ADD:1/4 WAVE ROOF TOP ANT VHF | Corresponding kit: HAD4009 | G300 | 656 | $15.00
1/4 WAVE BROADBAND ANT 146-174 | Corresponding kit: HAD4017 | G629 | 656 | $70.00
ADD:VHF ANT WIDEBAND 136-174 MHZ | Corresponding kit: HAD4021 | G792 | 656 | $83.00
ALT: 1/4 WV BDBD ANT 136-162 MHZ | Corresponding kit: HAD4016 | W652 | 656 | $53.00

UHF R1 Antennas

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANT 3.5DB 380-420 MHZ MAXRAD | Corresponding kit: HAE6010. | G427 | 656 | $61.00
ADD: ANT 5.0DB 380-420 MHZ MAXRAD | Corresponding kit: HAE6011 | G429 | 656 | $68.00
ADD: ANT 5.0DB 445-470 MHZ | Corresponding kit: RAE4014ARB. | G430 | 656 | $121.00
ADD: ANT 1/4 WAVE WHIP 380-420 MHZ | Corresponding kit: HAE6012. **DESIGN MODIFICATIONS ARE BEING MADE TO THIS ANTENNA. THE NEW DESIGN INCLUDES TITANIUM BLACK PLATING, TEARDROP TOP, AND GOLD BUTTON PLATING.** | G425 | 656 | $28.00
ADD: ANT 1/4 WAVE WHIP 450-470 MHZ | TEMPORARY: Not compatible with U2-7/800 Bandsplit. Corresponding kit: HAE4003. | G426 | 656 | $28.00
ADD: ANT 3.5DB 450-470 MHZ | Corresponding kit: HAE4011 | G428 | 656 | $55.00
ADD: ANT WIDEBAND 380-470 MHZ MAXRA | Corresponding kit: HAE6013. | G431 | 656 | $64.00
ADD: ANT 2DB WIDEBAND 380-520 MHZ | TEMPORARY: Not compatible with U2-7/800 Bandsplit. Corresponding kit: HAE6031 | GA00505 | 656 | $55.00

UHF R2 Antennas

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANT 5.0DB 445-470 MHZ | Corresponding kit: RAE4014ARB. | G430 | 656 | $121.00
ADD: ANT 1/4 WAVE WHIP 450-470 MHZ | TEMPORARY: Not compatible with U2-7/800 Bandsplit. Corresponding kit: HAE4003. | G426 | 656 | $28.00
ADD: ANT 3.5DB 450-470 MHZ | Corresponding kit: HAE4011 | G428 | 656 | $55.00
ADD: ASSEMBLY,ANTENNA ASSEMBLY,ADD: 5DB GAIN ANT 494-512 MHZ | Corresponding kit: RAE4016ARB. | G486 | 656 | $64.00
ADD: ANT 1/4 WAVE 470-512 MHZ | Corresponding kit: HAE4004. | G490 | 656 | $15.00
ADD: ANT 3 DB ROOF TOP 470-495 MHZ | Corresponding kit: HAE4012 | G493 | 656 | $36.00
ADD: ANT 3 DB ROOF TOP 494-512 MHZ | Corresponding kit: HAE4013 | G494 | 656 | $36.00
ADD: ANT LOW PROFILE 450-512 MHZ | Corresponding kit: HAE6016 | G510 | 656 | $55.00
ADD: ANT 2DB WIDEBAND 380-520 MHZ | TEMPORARY: Not compatible with U2-7/800 Bandsplit. Corresponding kit: HAE6031 | GA00505 | 656 | $55.00
ADD: ANT ROOF TOP 5 dB 470-494 MHz | Corresponding kit: RAE4015ARM | GA00652 | 656 | $90.00

#### 5: Operation Mode (Must Select One)

Trunking mode requires either a Software Key (QA01749 comes standard unless QA01648 is selected), or a Hardware Key (QA01648).

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
SOFTWARE LICENSE ENH: 3600 OR 9600 TRUNKING BAUD SINGLE SYSTEM | Provides for Digital and P25 Trunking. | QA02756AB | 0426 | $1,727.00
ENH: LI ANALOG 3600 TRUNKING | Provides for Analog Trunking | Q443 | 755 | $1,210.00
ADD: ANALOG CONVENTIONAL | Provides for Analog Conventional | QA02829 | 471 | $440.00
SOFTWARE LICENSE ENH: SOFTWARE P25 CONVENTIONAL | Provides for Digital Conventional. | Q811BR | 0426 | $650.00

#### System Enhancement Options (Optional)

The following options are optional and will provide additional capabilities, if required.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DIGITAL TONE SIGNALING | Requires Digital Operation. | GA09000 | 656 | $165.00
ADD: DVRS MSU ACTIVATION | Incompatible with Data Modem Tethering. Requires Remote Mount and P25 Digital Trunking. | GA00631 | 656 | $275.00
ADD: DVRS PSU ACTIVATION | Requires P25 Digital Trunking. If you are connecting your radio directly to a DVR then order GA00631. | QA00631 | 655 | $110.00
ADD: ENHANCED DATA APX | Requires P25 9600 Trunking | QA03399 | 656 | $165.00
ADD: GROUP SERVICES | Offers Conventional Alias updates, Trunking Alias updates and Trunking Group Messaging. This option requires Digital for Conventional only capabilities and P25 Trunking for any Trunking only capabilities. You can now also do Over the Air Firmware Updates with this feature. | GA09008 | 656 | $165.00
ADD: MISSION CRITICAL GEOFENCING | Requires Digital, IV&D, and GPS. | GA09012 | 471 | $165.00
ADD: MULITCAST VOTING SCAN | Requires Digital Operation. | G387 | 656 | $220.00
ADD: APX MOBILE RADIO AUTHENTICAT | Requires P25 9600 Trunking | GA01767 | 527 | $110.00
ADD: MOBILE PERSONAL ACCOUNTABILITY SW | Requires Digital Operation | G445 | 571 | $150.00
ENH: OVER THE AIR PROVISIONING | Requires P25 Digital Trunking. To do in field POP25 programming must use Advanced System Key (DVN4046A). | G996 | 656 | $110.00
ENH: ENH: RADIO TRACE | Requires W20, W22, W872, G892, or GA00221. Some older revisions are not compatible. | G170 | 656 | $83.00
ADD: SITE SELECTABLE ALERT FOR P25 TRUNKING | Requires P25 9600 Trunking | GA00982 | 656 | $165.00
ADD: TDMA OPERATION APX | Requires P25 Digital Trunking | GA00580 | 656 | $495.00

#### 6. Feature Antennas (Must select one)

Although GPS comes standard, an antenna is required for the full solution.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: GPS ANTENNA GLASS MT | Corresponding kit: PMAN4001 | GA00270 | 656 | $36.00
ADD: GPS ANTENNA | Corresponding kit: HAG4000 | GA00226 | 656 | $83.00

#### Advanced System Key (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: HW KEY SUPPLEMENTAL DATA | The SOFTWARE KEY is the default Advance System Key option that ships standard on all APX products. You cannot order software key QA01749. The HARDWARE KEY QA01648 can be ordered instead. Be sure to enter the CORRECT SYSTEM OWNER ID in the supplemental data. If an INCORRECT ID is entered, a FLASHport order is required to fix the error. Order HARDWARE KEY (QA01648) if required to operate/program on a trunking system. Not compatible with conventional. | QA01648AA | 0655 | $6.00

#### 7. Encryption Algorithms (Must select one)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

The APX 6500Li does not support multiple hardware encryption types.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: AES ENCRYPTION APX AND ADP | Requires digital operation. P25 CAP Compliant option. Includes ADP. | G843 | 656 | $523.00
ADD: DES/DES-XL/DES-OFB ENCRYPTION AND ADP | Multikey is required for use of more than one key. Non-P25 CAP Compliant option. Includes ADP. | G625 | 656 | $659.00
ADD: DVP-XL ENCRYPTION AND ADP | Includes ADP. Non-P25 CAP Compliant option. | W797 | 656 | $536.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP Compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | G193 | 430 | $0.00
ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below. QA05751 is CAP a COM compliant option. | QA05751AA | 0655 | $0.00

#### Multikey

All multikey options require an encryption algorithm selection.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: MULTIPLE KEY ENCRYPTION OPERATION | Required when using more than one encryption algorithm or encryption key. | W969 | 656 | $363.00

#### 8. Remote Mount Cables (17 FT STD)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD:CBL REMOTE MOUNT 10 FEET | Corresponding kit: HKN6170 | G618 | 656 | $11.00
ADD: REMOTE MOUNT CBL 30 FEET | Corresponding kit: HKN6168 | G610 | 656 | $28.00
ADD: REMOTE MOUNT CBL 50 FEET | Corresponding kit: HKN6167 | G609 | 656 | $39.00
ADD:CBL REMOTE MOUNT 75 FEET | Corresponding kit: HKN6166A | G607 | 656 | $50.00
ADD:REMOTE MOUNT CBL 115 FEET | Corresponding kit: HKN6165 | G879 | 656 | $61.00
ADD: REMOTE MOUNT CABLE 128 FT | Actual length 128 ft. Corresponding kit: HKN6164 | G582 | 656 | $72.00

#### Data/Programming Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: USB DATA INTFC CABLE-DASH | 6 FT USB W/IGNITION SENSE Corresponding kit: HKN6163B. Can be used to program APX Mobile Radios. | G308 | 656 | $55.00
ADD:USB DATA INTFC CABLE-TRK | 16.5 FT USB W/IGNITION SENSE Corresponding kit: HKN6172B. Can be used to program APX Mobile Radios. | G309 | 656 | $55.00
ADD: RS232 DATA INTFC CBL DASH | 6 FT RS232 DATA CABLE Corresponding kit: HKN6160A. | G303 | 656 | $55.00
ADD: RS232 DATA INTFC CBL TRK | 20 FT RS232 DATA CABLE Corresponding kit: HKN6161A. | G304 | 656 | $55.00

#### Cable Accessories (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: EXTERNAL ALARM RELAY AND CABLE | For either horns or lights, not both. | W116 | 656 | $83.00
ADD: KEY LOCK MOUNT APX | Requires Remote Mount | W81 | 471 | $36.00
ADD: GCAI EXTENSION CABLE 2 FT | Requires GCAI style Mic. Corresponding Kit PMKN4093A. | GA00589 | 656 | $33.00
ADD:REMOTE MOUNT VIP CBL APX | Park/Kill, Gunlock, 'Horn Ring/Horn Transfer' or Horn/Lights Park/Kill and Horn 'Ring/Horn Transfer' only available with Motorola Siren. Corresponding Kit: HKN6196B | G322 | 656 | $39.00
ADD: UNIVERSAL RELAY CONTROLLER | Requires URC-Transceiver Cable | GA00259 | 656 | $275.00
ADD: CABLE URC TO TRANSCEIVER | Requires Universal Relay Controller | GA00260 | 656 | $17.00

#### 9: Microphones (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: HAND MIC,GCAI WATER RESISTANT | Not compatible with control station operation. Corresponding kit HMN1089A | G892 | 656 | $79.00
ADD: MODEL III GCAI KEYPAD HANDSET | Not compatible with Control Station. Corresponding kit: HMN4097A | GA00221 | 656 | $325.00
ADD: KEYPAD MIC GCAI | Corresponding kit: HMN4079 | W20 | 471 | $198.00
ADD:GATEWAY RSM AND WIRELESS RSM WITH VEHICLE CHARGER | Includes 12V Vehicle Charger Corresponding kit: RLN6551 | GA01354AA | 656 | $550.00
ADD:GATEWAY RSM AND WIRELESS RSM | Corresponding kit: RLN6552 | GA01439 | 656 | $431.00
ADD: CONTROL STATION DESK GCAI MIC | Not compatible with Remote Mount. Requires Control Station, DEK, and Dash Mount. Corresponding Kit: RMN5070 | W382 | 656 | $186.00
ADD:GATEWAY RSM | Corresponding kit: PMMN4097 | GA01438 | 656 | $138.00
ADD: STD PALM MICROPHONE APX | Corresponding kit: HMN1090 | W22 | 471 | $79.00
ADD: VISOR MIC REMOTE MOUNT | Requires PTT Option. Incompatible with Control Station. Corresponding Kit Number: RMN5054 | W872 | 656 | $33.00
ADD: GOOSENECK PTT | Requires Visor Mic. Kit Number: HMN1087A | G233 | 656 | $62.00
ADD: PTT FOOTSWITCH | Requires Visor Mic. Kit Number: GLN7278 | G235 | 656 | $56.00

#### Emergency (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: EMERGENCY ID EXT. FOOTSWITCH | Corresponding kit: HLN5113. | W470 | 656 | $62.00
ADD: EXTERNAL EMERGENCY PUSHBUTTON | Corresponding kit: HLN5131 | W688 | 656 | $62.00

#### Direct Mode Entry & Status/Message

Require Remote Mount configuration.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 8 MODE DIRECT ENTRY | Corresponding kit: H1835 | W599 | 656 | $198.00
ADD: 16 MODE DIRECT ENTRY | Corresponding kit: H1836 | W614 | 656 | $396.00
ADD: 24 MODE DIRECT ENTRY | Corresponding kit: H1837 | W615 | 656 | $594.00
ADD: STATUS/MESSAGE 8 | Corresponding kit: H1838 | W355 | 656 | $523.00
ADD: STATUS/MESSAGE 16 | Corresponding kit: H1839A | W374 | 656 | $715.00
ADD: DEK FOR WHELEN SIREN | Corresponding kit: H1883A | GA00814 | 656 | $116.00

#### 10: Speakers (Must Select One)

Speakers are not compatible with Control Station Operation.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SPKR 15W WATER RESISTANT | Corresponding kit: HSN4040 | G831 | 656 | $66.00
ADD: SPKR 7.5W WATER RESISANT | Corresponding kit: HSN4038 | G832 | 656 | $67.00
ADD: AUXILIARY SPKR 7.5 WATT | Corresponding kit: HSN4031 | B18 | 656 | $66.00
ADD: AUXILARY COVERT SPKR 10W APX | Corresponding kit: HSN4042 | GA01203 | 656 | $66.00
ADD: AUXILARY SPKR 13W (3.2OHM) | Corresponding kit: HSN4032 | W432 | 656 | $79.00
ADD: NO SPEAKER NEEDED | Required for Control Station | G142 | 656 | $0.00

#### Auxiliary Wildcard

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: AUXILIARY SWITCH PANEL | Remote Mount Required. Corresponding kit: HLN1196. | W591 | 656 | $182.00

#### Amplifier

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: RF PREAMP | Option applies only to VHF & UHF radios. | W12 | 471 | $73.00

#### Documentation (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX MOBILE USER GUIDE | User Guide CD. PDFs of User Guides can be found on the page. | G657 | 656 | $28.00

#### RFID (Optional)

#### 11: Service (Must Select One)

SIREN AND LIGHTS INTERFACE MODULE
(Allows for control of most light and siren systems via radio control head. Not required for Motorola Siren.)

MOTOROLA SIREN

(This siren can be connected directly to the mobile radio)

Siren and Lights Interface Module not required for this siren.

NOTE: THE NEW SIREN IS COMPATIBLE WITH APX AND XTL REMOTE MOUNT MOBILES WITH "O" SERIES CONTROL HEADS ONLY. THIS SIREN IS NOT COMPATIBLE WITH ANY "W" SERIES CONTROL HEADS.

THE SIREN BASE MODEL TT2592, CABLE TT05900 AND THE SIREN MOUNTING HARDWARE TT0507 MUST ALWAYS BE ORDERED (THIS SIREN TT2592 IS ORDERED AS A SEPARATE LINE ITEM THEN THE RADIO MODEL).

DEK OPTIONS ARE AVAILABLE AS OPTIONS TO THE SUBSCRIBER AS SHOWN BELOW.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
WHELEN/MOTOROLA SIREN | Siren AMP- box only spare part: DDN1542 If you need the siren speaker as well, use DDN1784A | TT2592 | 256 | $679.00
ADD: SIREN TO RADIO CABLE (21-PIN D | Spare parts part number: DDN1833 | TT05900AA | 256 | $87.00

Bull Horns for Sirens and Public Address

Control Station Tray and Power Supply

Customer Programming Software

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
CABLE CH, PROGRAMMING,USB | HKN6184C - Used to program the radio with Customer Programming Software and Tuner Software. Compatible with APX mobile radios. | HKN6184C | 261 | $57.25

Programming and Data Cables
(Please see CPS PART NUMBER GUIDE for cable descriptions)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
CABLE KIT 20' DATA | RS232 Data Interface Cable - REMOTE | HKN6161 | 500 | $50.00
CABLE CH, PROGRAMMING,USB | HKN6184C - Used to program the radio with Customer Programming Software and Tuner Software. Compatible with APX mobile radios. | HKN6184C | 261 | $57.25

####

### Software and Services

- CLICK HERE to see the Latest Lead Time Estimates

- CLICK HERE to see the Latest Lead Time Estimates

### Update History

Starting January 1 2015.The SOFTWARE KEY (QA01749) is the default Advance System Key, it ships by default on all APX products; The HARDWARE KEY can be ordered instead by using QA01648. The DVN4046 Master Key Starter Kit is required for the Hard Key or to operate on a thrid-party Trunking system. The CORRECT System Owner ID will be required upon ordering the Hard Key or DVN Kit. Details can be found on the Advanced System Keys-ASK for RSD Subscriber ECAT page Be sure to enter the CORRECT SYSTEM OWNER ID when supplemental data is required. If an INCORRECT ID is entered, a FLASHport order is required to fix the error.