Back

##### APX 6500 Mobile Radio

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Software and Services
- Ship Card
- Update History

Back

##### APX 6500 Mobile Radio

### Model

ASTRO® Digital APX 6500 Mobile Subscriber
700/800 MHz (10 – 35 Watts)
VHF - 136 -174 (10 - 50 Watts)
UHFR1 - 380-470 (10 - 40 Watts)
UHF R2 450-520 (10 - 45 Watts)

Secure and Trunked Radio Systems

### Updates

####

- CLICK HERE to see the Latest Lead Time Estimates

Effective June 15th, 2022: APX 6500 U2 AN stopped shipments, its last order date was May 15th, 2022. The enhanced BN version has been available since April, 2022.

Effective October 11th, 2021: APX Mobile One Touch Feature was enhanced and integrated with DEK’s Status Message functionalities. Users benefit from the ability to program and assign alias Status Messages on the APX Control Head display. One Touch Feature G683 pricing increased from $75 to $125. .

Effective October 5th, 2020: All U.S. orders have required an encryption selection. QA05751 “Clear Radio No ADP” became an orderable option with a $0 dollar cost. G193/Q667 ADP only is also available at $0. Please see encryption section for AES and other encryption options that come with ADP. Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.

Effective Aug 1st, 2020: The O5 control head (option G442 and kit H1904) was canceled and replaced by the E5 (GA01670 and H1930)

Effective August 26, 2019: Multi-System OTAR (GA01620) is available. Users who frequently move from one secure system to another will benefit from the ease and speed that radio keys are shared and updated. Our Multi-System Over-the-Air Rekeying (Multi-System OTAR) feature supports over-the-air-rekeying with up to 19 different secure systems, key sharing across profiles and seamless migration of fielded radios. The customer must order OTAR W/ MULTIKEY as a prerequisite for MS-OTAR.

Effective July 31, 2018: The APX 6500 High Power Models were cancelled. The replacement model is the APX 8500 HP Model (M37TXS9PW1AN)

Special Note for United States - State & Local Markets:

In accordance with FCC mandate, the U1/U2 Mid Power and U1/7-800 band combinations for this product are restricted to not allow programming for 25 KHz operation. These frequencies are restricted to 12.5 KHz operation only.

### Ordering Information

#### Please Read All Option Descriptions Before Making Your Selection

Required Selections:

1) Main Model

2) Mounting

3) Control Head Selection

4) RF Antenna

5) Operation Mode

6) Feature Antenna(s)

7) Encryption

8) Remote Mount Cables (if remote mount is selected)

9) Microphone

10) Speaker

11) Service

Please note, the APX 6500 does not support Motorcycle Configuration.

#### Additional Ordering Information for Service Options

ViQi Virtual Partner End to End Ordering Guide

### Configuration

####

#### 1. Main Model (Must Select One)

Special Note for United States - State & Local Markets: In accordance with FCC mandate, the U1/U2 Mid Power and U1/7-800 band combinations for this product are restricted to not allow programming for 25 KHz operation. These frequencies are restricted to 12.5 KHz operation only.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
APX6500 UHF R2 MID POWER | - | M25SSS9PW1 N | 527 | $2,896.00

#### 2. Mounting (Must Select One)

If a remote mount cable other than 5 meters (17ft) is desired for G67, please reference the "Remote Mount Cables" section.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DASH MOUNT | Required for Control Station Operation. O3 Dash mount is identical to remote mount minus the 17? extension cable PMLN4958A | G66 | 656 | $148.00
ADD: REMOTE MOUNT MID POWER | G67 is required for Motorcycle Configuration. G67 FOR Motorcycle Remote Mount is $400 DUP. | G67 | 656 | $350.00

#### Control Station Operation (Optional)

O2, E5 & O7 Control Heads Only. Must select one.

Requires Dash Mount (G66)

Some microphones are not compatible with Control Station Operation. Please read descriptions carefully.

Although the Power Supply is optional, it is needed for a full Control Station solution.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: CONTROL STATION OPERATION | Requires a O2, O5, E5, or O7 Control Head. Requires Dash Mount (G66) Some microphones are not compatible with Control Station Operation. Please read descriptions carefully. | W665 | 656 | $82.00
ADD: CONTROL STATION POWER SUPPLY | Although the Power Supply is optional, it is needed for a full Control Station solution. Corresponding kit: HPN4007 | G91 | 656 | $317.00

#### 3A Control Head Software (Required)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX CONTROL HEAD SOFTWARE | - | G444 | 656 | $0.00

#### 3B Control Head Options (Must select one)

O2 Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX O2 CH (GREY) | - | GA00804 | 656 | $579.00
ADD:IMPACT GREEN COLOR HOUSING (O2) | When ordered in conjunction with GA00804 you will get a green colored O2 housing. | G201 | 656 | $30.00
ADD: SCHOOL SERCURITY ENHANCEMENT PACKAGE | Education O2 Emergency Push Button | GA01056 | 514 | $55.00

O3 Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX O3 HANDHELD CH | Requires No Microphone (G90). If Lights & Siren Keypad and Software is required, order GA00806. | G72 | 656 | $1,114.00
ADD:CH SIREN & LIGHTS KEYPAD | Available on O3 (G72) and O7 (GA00805) Control Heads. | GA00806 | 656 | $59.00

E5 Control Head Option

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX E5 CONTROL HEAD | - | GA01670 | 681 | $767.00

O7 Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX O7 CONTROL HEAD. | If Lights & Siren Keypad and Software is required, order GA00806. | GA00805 | 656 | $744.00
ADD:CH SIREN & LIGHTS KEYPAD | Available on O3 (G72) and O7 (GA00805) Control Heads. | GA00806 | 656 | $59.00

No Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: NO O3 CONTROL HEAD | If you plan to use this model with an O3 Control Head but already have a control head and don't require it, select GA00001. Requires remote mount (G67). | GA00001 | 656 | $0.00
ADD: APX NO O2/O7 CH NEEDED MTCL | If you plan to use this model with an O2/O5/E5/O7 Control Head but already have a control head and don't require it, select G88. Requires remote mount option (G67). | G88 | 656 | $0.00

#### Dual Control Head (Optional)

The APX 6500 mobile can support up to two control heads on a single transceiver. This allows control of a single APX 6500 transceiver from two different control head locations.

Dual Control Head requires Remote Mount.

When ordering the dual control head option, only one type of control head can be selected.

Only available with O2, E5, O7 Control Heads.

The Dual Control Head Option requires an equal number of microphones, speakers, and CAN cables.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX DUAL-CONTRL HD HARDWARE | Requires either O2/O5/E5/O7 Control Head. Requires a remote mount configuration. Requires a selection of 2 for microphones, speakers and CAN cables. | GA00092 | 656 | $627.00

#### 4. RF Antenna (Required)

No Antenna Requested

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: NO RF ANTENNA NEEDED | - | G89 | 656 | $0.00

7/800 Antennas

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANT 3DB LOW-PROFILE 762-870 | Corresponding kit: HAF4013 | G174 | 656 | $50.00
ADD: ANT 3DB ELEVATED FEED 762-870 | Corresponding kit: HAF4014. | G175 | 656 | $89.00
ADD: ANT 1/4 WAVE 762-870 MHZ | Corresponding kit: HAF4016 | G335 | 656 | $16.00
ALT: ANT 3DB GAIN 762-870MHZ | Corresponding kit: HAF4017 | W484 | 656 | $45.00

VHF Antennas

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 3BD ANT 136-174MHZ | Corresponding kit: HAD4022A. | G301 | 656 | $68.00
ADD: 1/4 WAVE WHIP ROOF TOP 136-144 | Corresponding kit: HAD4006 | G296 | 656 | $16.00
ADD: 1/4 WAVE ROOF TOP 144-150.8 | Corresponding kit: HAD4007 | G297 | 656 | $16.00
ADD: 1/4 WAVE ROOF TOP 150.8-162 | Corresponding kit: HAD4008 | G299 | 656 | $22.00
ADD:1/4 WAVE ROOF TOP ANT VHF | Corresponding kit: HAD4009 | G300 | 656 | $16.00
1/4 WAVE BROADBAND ANT 146-174 | Corresponding kit: HAD4017 | G629 | 656 | $75.00
ADD:VHF ANT WIDEBAND 136-174 MHZ | Corresponding kit: HAD4021. | G792 | 656 | $89.00
ALT: 1/4 WV BDBD ANT 136-162 MHZ | Corresponding kit: HAD4016 | W652 | 656 | $57.00

UHF R1 Antennas

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANT 3.5DB 380-420 MHZ MAXRAD | Corresponding kit: HAE6010 | G427 | 656 | $65.00
ADD: ANT 5.0DB 380-420 MHZ MAXRAD | Corresponding kit: HAE6011 | G429 | 656 | $73.00
ADD: ANT 5.0DB 445-470 MHZ | Corresponding kit: RAE4014ARB | G430 | 656 | $121.00
ADD: ANT 1/4 WAVE WHIP 380-420 MHZ | Corresponding kit: HAE6012 | G425 | 656 | $30.00
ADD: ANT 1/4 WAVE WHIP 450-470 MHZ | Corresponding kit: HAE4003. | G426 | 656 | $30.00
ADD: ANT 3.5DB 450-470 MHZ | Corresponding kit: HAE4011 | G428 | 656 | $59.00
ADD: ANT WIDEBAND 380-470 MHZ MAXRA | Corresponding kit: HAE6013 | G431 | 656 | $64.00
ADD: ANT 2DB WIDEBAND 380-520 MHZ | Corresponding kit: HAE6031 | GA00505 | 656 | $59.00

UHF R2

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANT 5.0DB 445-470 MHZ | Corresponding kit: RAE4014ARB | G430 | 656 | $121.00
ADD: ANT 1/4 WAVE WHIP 450-470 MHZ | Corresponding kit: HAE4003. | G426 | 656 | $30.00
ADD: ANT 3.5DB 450-470 MHZ | Corresponding kit: HAE4011 | G428 | 656 | $59.00
ADD: ASSEMBLY,ANTENNA ASSEMBLY,ADD: 5DB GAIN ANT 494-512 MHZ | Corresponding kit: RAE4016ARB | G486 | 656 | $68.00
ADD: ANT 1/4 WAVE 470-512 MHZ | Corresponding kit: HAE4004 | G490 | 656 | $16.00
ADD: ANT 3 DB ROOF TOP 470-495 MHZ | Corresponding kit: HAE4012 | G493 | 656 | $39.00
ADD: ANT 3 DB ROOF TOP 494-512 MHZ | Corresponding kit: HAE4013 | G494 | 656 | $39.00
ADD: ANT LOW PROFILE 450-512 MHZ | Corresponding kit: HAE6016 | G510 | 656 | $59.00
ADD: ANT 2DB WIDEBAND 380-520 MHZ | Corresponding kit: HAE6031 | GA00505 | 656 | $59.00
ADD: ANT ROOF TOP 5 dB 470-494 MHz | Corresponding kit: RAE4015ARM | GA00652 | 656 | $96.00

#### Dual Radio Operation Options

The APX Dual Radio Feature offers the capability to control TWO (2) APX8500, APX7500, APX6500, or APX6500Li mobile radios from ONE (1) O7, or E5 control head. APX Dual Radio allows for mixing and matching of radios across tiers (i.e. APX 8500 with APX 6500) and power levels (High Power with Mid Power).

Each radio in an APX Dual Radio system must be ordered independently.

The mobiles in a dual radio solution can be single or dual band. Both radios can be on the same or different frequency bands.

One radio must be ordered with the Primary Radio option (GA01113) and the other with the Secondary Radio option (GA01117). This will include both the SW and HW required for dual radio operation.

Although each radio must be ordered as either a Primary or Secondary radio, each radio can be configured to work as a Primary, Secondary, or a Standalone radio.

Only one speaker can be connected to the control head and it will play audio from the primary radio. A 30 ft. speaker extension cable is included on the secondary radio to connect the second speaker directly to the secondary radio. If a longer cable is needed, a 131 ft. version can be purchased from AAD (part # HKN6251)

The Dual Radio feature is incompatible with the multi-control head options.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: DUAL RADIO OPERATION (PRIMARY RADIO) | The Primary radio must be ordered with an O7 or E5 CH. APX Dual Radio is not compatible with any other control head. The primary radio includes a short dual radio CAN cable (HKN6245) to connect both radios together. If the stack mount trunnion is ordered, a right-angle version of this cable (HKN6249) will ship instead to facilitate stack-mounted installations. If a different length is desired, the standard remote mount control head cables can also be used to connect both together. | GA01113 | 656 | $715.00
ENH: DUAL RADIO OPERATION (SECONDARY RADIO) | The secondary radio must be ordered with no control head (G88). | GA01117 | 656 | $715.00

#### Dual Radio Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DUAL RADIO STACKABLE MP TRUNNION | Comprised of HLN7045A and HKN6249A | GA01115 | 656 | $350.00

#### 5: Operation Mode (Must Select One)

5A: Digital Trunking (SN/SZ P25 Phase I Interop)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SMARTZONE OPERATION APX6500 | Not compatible with G48. | G51 | 527 | $1,412.00
ADD: ASTRO DIGITAL CAI OPERATION | Not compatible with G241. | G806 | 656 | $607.00
ENH: P25 TRUNKING SOFTWARE APX | Required when ordering Smartzone Operation (G51) & Digital Operation (G806). Smartzone Omnilink (G173) is included with this option. | G361 | 656 | $330.00

5B: Digital Trunking (SN/SZ)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SMARTZONE OPERATION APX6500 | Not compatible with G48. | G51 | 527 | $1,412.00
ADD: ASTRO DIGITAL CAI OPERATION | Not compatible with G241. | G806 | 656 | $607.00
ADD: SMARTZONE OMNILINK | Automatic Zoning Across Zones, Zone Registration, Trespass Protection, Over the Air Site Alias, 32 Preferred Sites, FastStart and AllStart Call Setup. | G173 | 656 | $235.00

5C: Digital Conventional (P25)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ASTRO DIGITAL CAI OPERATION | Not compatible with G241. | G806 | 656 | $607.00
ENH: CONVENTIONAL OPERATION APX6500 | Not compatible with G51. | G48 | 527 | $550.00

5D: Analog Trunking

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SMARTZONE OPERATION APX6500 | Not compatible with G48. | G51 | 527 | $1,412.00
ENH: SW ASTRO READY (ANALOG) | Not compatible with G806 or with Encryption Algorithm W969, W793, W797, G625, G298, G851, or G843 when combined with a Trunking Software Option. | G241 | 656 | $0.00

5E: Analog Conventional

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: CONVENTIONAL OPERATION APX6500 | Not compatible with G51. | G48 | 527 | $550.00
ENH: SW ASTRO READY (ANALOG) | Not compatible with G806 or with Encryption Algorithm W969, W793, W797, G625, G298, G851, or G843 when combined with a Trunking Software Option. | G241 | 656 | $0.00

#### System Enhancement Options (Optional)

The following options are optional and will provide additional capabilities, if required.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DIGITAL TONE SIGNALING | Requires Digital Operation (G806). | GA09000 | 656 | $177.00
ADD: DVRS MSU ACTIVATION | Incompatible with Data Modem Tethering. Requires Remote Mount (G67). | GA00631 | 656 | $294.00
ADD: DVRS PSU ACTIVATION | Enables DVRS Enhanced PSU functionality on APX Mobile Radios. Requires Digital Operation. QA00631 is to be ordered for radios that are not connected directly to a DVR. If you are connecting your radio directly to a DVR then order GA00631. | QA00631 | 655 | $118.00
ADD: ENHANCED DATA APX | Requires P25 9600 Trunking (G361). | QA03399 | 656 | $177.00
ADD: GROUP SERVICES | Offers Conventional Alias updates, Trunking Alias updates and Trunking Group Messaging. This option requires Digital Operation (G806) for Conventional only capabilities and G361 for any Trunking only capabilities. You can now also do Over the Air Firmware Updates with this feature. | GA09008 | 656 | $177.00
ADD: MISSION CRITICAL GEOFENCING | Requires Digital Operation (G806), IV&D (W947), and GPS (GA00229). | GA09012 | 471 | $177.00
ADD: DATA MODEM TETHERING | For Sierra Wireless MG90 operation, KT000259A01 (aftermarket USB Ethernet HUB Cable Assembly) must be ordered on a separate line. Compatible with DVRS MSU GA00631, requires GA01779 (aftermarket cable KT000247A04) when both GA09011 and GA00631 are ordered. For more details on requirements and connectivity options, please refer to MN003449A01 APX Data Modem Tethering User Guide | GA09011 | 681 | $110.00
ADD: MULITCAST VOTING SCAN | Requires Digital Operation (G806). This feature allows for voting of the Conventional Channels only. | G387 | 656 | $235.00
ADD: APX MOBILE RADIO AUTHENTICAT | Requires P25 9600 Trunking (G361). | GA01767 | 527 | $110.00
ADD: MOBILE PERSONAL ACCOUNTABILITY SW | Requires Digital Operation. | G445 | 571 | $161.00
ENH: OVER THE AIR PROVISIONING | Requires P25 9600 Trunking (G361). There is no Analog Functionality for this feature. To do in field POP25 programming must use Advanced System Key (DVN4046A). | G996 | 656 | $110.00
ADD: SITE SELECTABLE ALERT FOR P25 TRUNKING | Requires P25 9600 Trunking (G361). | GA00982 | 656 | $177.00
ENH: TACTICAL RADIO STW-STUN/KILL | Requires digital (G806), IV&D, and a encryption (not including ADP-only). | H02 | 481 | $89.00
ADD: TDMA OPERATION APX | Requires P25 9600 Trunking (G361). | GA00580 | 656 | $530.00
ENH: ENHANCEMENT LEVEL 2 | Please reference the Enhancement Level Reference Guide for more details. | GA01771 | 527 | $235.00
ADD: PSU CONV SCAN | Requires QA00631 | HA00677AA | 0579 | $0.00

Enhancement Level Reference Guide

#### 6. Feature Antennas (Must select one)

Although GPS comes standard, an antenna is required for the full solution.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: GPS ANTENNA GLASS MT | Corresponding kit: PMAN4001 | GA00270 | 656 | $39.00
ADD: GPS ANTENNA | Corresponding kit: HAG4000 | GA00226 | 656 | $89.00

#### Advanced System Key (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: HW KEY SUPPLEMENTAL DATA | The SOFTWARE KEY is the default Advance System Key option that ships standard on all APX products. You cannot order software key QA01749. The HARDWARE KEY QA01648 can be ordered instead. Be sure to enter the CORRECT SYSTEM OWNER ID in the supplemental data. If an INCORRECT ID is entered, a FLASHport order is required to fix the error. Order HARDWARE KEY (QA01648) if required to operate/program on a trunking system. Not compatible with conventional. | QA01648AA | 0655 | $6.42

#### 7. Encryption Algorithms (Must Select One)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: AES ENCRYPTION APX AND ADP | Requires digital operation. P25 CAP Compliant option. Includes ADP. | G843 | 656 | $560.00
ADD: AES/DES-XL/DES-OFB ENCRYPTION AND ADP | Multikey is required for use of more than one key. AES and DES-OFB Operation require digital operation. P25 CAP Compliant option. Includes ADP. | G851 | 656 | $879.00
ADD: DES/DES-XL/DES-OFB ENCRYPTION AND ADP | Multikey is required for use of more than one key. Non-P25 CAP Compliant option. Includes ADP. | G625 | 656 | $659.00
ADD: DVP-XL ENCRYPTION AND ADP | Includes ADP. Non-P25 CAP Compliant option. | W797 | 656 | $574.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP Compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | G193 | 430 | $0.00
ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below. QA05751 is CAP a COM compliant option. | QA05751AA | 0655 | $0.00

#### Multikey (Optional)

All multikey options require an encryption algorithm selection.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: MULTIPLE KEY ENCRYPTION OPERATION | Required when using more than one encryption algorithm or encryption key. | W969 | 656 | $363.00
ENH: ASTRO 25 OTAR W/ MULTIKEY | Not compatible with ADP-Only. Requires AES. Includes multikey, trunking OTAR, and Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. | G298 | 656 | $814.00
ADD:TACTICAL OTAR APX | Requires digital (G806) and IV&D (W947). | H04 | 656 | $412.00
ADD: MULTI SYSTEM OTAR | Requires ASTRO 25 OTAR W/ MULTIKEY (G298) | GA01620 | 656 | $177.00

#### 8. Remote Mount Cables (17 FT STD)

Multi-control head options delete the 17 FT standard cable and customers are required to order a cable per control head. Multi-control head options delete the 17 FT standard cable and customers are required to order a cable per control head. Only for O5, E5 & O7 Control Heads.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD:CBL REMOTE MOUNT 10 FEET | Corresponding kit: HKN6170 | G618 | 656 | $12.00
ADD: REMOTE MOUNT CBL 17 FEET | Included at no charge with Single Control Head Remote Mount installations and High Power. Corresponding kit: HKN6169 | G628 | 656 | $18.00
ADD: REMOTE MOUNT CBL 30 FEET | Corresponding kit: HKN6168 | G610 | 656 | $30.00
ADD: REMOTE MOUNT CBL 50 FEET | Corresponding kit: HKN6167 | G609 | 656 | $42.00
ADD:CBL REMOTE MOUNT 75 FEET | Corresponding kit: HKN6166A | G607 | 656 | $54.00
ADD:REMOTE MOUNT CBL 115 FEET | Corresponding kit: HKN6165 | G879 | 656 | $65.00
ADD: REMOTE MOUNT CABLE 128 FT | For dual control head configurations, the total cable length may not be greater that 131 ft (40 meters). Therefore, this cable should not be used with a dual control head configuration. Corresponding kit: HKN6164 (actual cable length is 128 ft) | G582 | 656 | $77.00

#### Data/Programming Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: USB DATA INTFC CABLE-DASH | 6 FT USB W/IGNITION SENSE Corresponding kit: HKN6163B. Can be used to program APX Mobile Radios. | G308 | 656 | $59.00
ADD:USB DATA INTFC CABLE-TRK | 16.5 FT USB W/IGNITION SENSE Corresponding kit: HKN6172B. Can be used to program APX Mobile Radios. | G309 | 656 | $59.00
ADD: RS232 DATA INTFC CBL DASH | 6 FT RS232 DATA CABLE Corresponding kit: HKN6160A. | G303 | 656 | $59.00
ADD: RS232 DATA INTFC CBL TRK | 20 FT RS232 DATA CABLE Corresponding kit: HKN6161A. | G304 | 656 | $59.00

#### Cable Accessories (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: EXTERNAL ALARM RELAY AND CABLE | For either HORN or LIGHTS. NOT both | W116 | 656 | $89.00
ADD:BUZZER 110MA APX | Corresponding Kit: HLN6953 | B116 | 656 | $59.00
ADD: GCAI EXTENSION CABLE 2 FT | For use with 07, O9 Control Heads and GCAI style Mic. KIT #PMKN4093A. | GA00589 | 656 | $35.00
ADD:REMOTE MOUNT VIP CBL APX | Park/Kill, Gunlock, 'Horn Ring/Horn Transfer' or Horn/Lights Park/Kill and Horn 'Ring/Horn Transfer' only available with Motorola Siren. Gunlock supported on O9 Control Head Only. CORRESPONDING KIT: (HKN6196B) | G322 | 656 | $42.00
ADD: UNIVERSAL RELAY CONTROLLER | Required to Control Vehicle Lights with the O3, 07 and O9 Control Heads.Requires URC Cable GA00260. | GA00259 | 656 | $294.00
ADD: CABLE URC TO TRANSCEIVER | Connects Universal Relay Controller to APX Transciver via a RJ45 and CGAI connection. | GA00260 | 656 | $18.00
ADD: KEY LOCK MOUNT APX | Remote Mount Mid Power Only. | W81 | 471 | $39.00

#### 9: Microphones (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: HAND MIC,GCAI WATER RESISTANT | Corresponding kit HMN1089A | G892 | 656 | $85.00
ADD: MODEL III GCAI KEYPAD HANDSET | Corresponding kit: HMN4097A | GA00221 | 656 | $348.00
ADD: NO MICROPHONE NEEDED | Select this option when ordering O3 Handheld Control Head (G72). If ordering with Motorcycle G138 the DB 25 connector on harness needs to be sealed to prevent corrosion. | G90 | 656 | $0.00
ADD: KEYPAD MIC GCAI | Corresponding kit: HMN4079 | W20 | 471 | $212.00
ADD:GATEWAY RSM AND WIRELESS RSM WITH VEHICLE CHARGER | Includes 12V Vehicle Charger Corresponding kit: RLN6551 | GA01354AA | 656 | $589.00
ADD:GATEWAY RSM AND WIRELESS RSM | Corresponding kit: RLN6552 | GA01439 | 656 | $461.00
ADD: CONTROL STATION DESK GCAI MIC | Dash Mount Required Corresponding Kit: RMN5070 | W382 | 656 | $199.00
ADD: STD PALM MICROPHONE APX | Corresponding kit: HMN1090 | W22 | 471 | $85.00
ADD:GATEWAY RSM | Corresponding kit: PMMN4097 | GA01438 | 656 | $148.00
ADD: VISOR MIC REMOTE MOUNT | Requires G90 No Microphone Needed & G235 Footswith PTT. Kit Number: RMN5054_ | W872 | 656 | $35.00
ADD: GOOSENECK PTT | Requires W872 Visor Mic. Kit Number: HMN1087A | G233 | 656 | $66.00
ADD: PTT FOOTSWITCH | Requires W872 Visor Mic. Kit Number: GLN7278_ | G235 | 656 | $60.00
ADD: HANDSET WITHOUT KEYPAD | Corresponding kit: HMN4098 | QA08865 | 656 | $202.00

#### Emergency

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: EMERGENCY ID EXT. FOOTSWITCH | Corresponding kit: HLN5113. | W470 | 656 | $66.00
ADD: EXTERNAL EMERGENCY PUSHBUTTON | Corresponding kit: HLN5131 | W688 | 656 | $66.00

#### Direct Mode Entry & Status/Message (Optional)

DEKs are incompatible with the O3 Control Head (except for DEK for Whelen Siren - GA00814). They require Remote Mount Configuration.

Please note, 24 modes are the maximum number of modes available. Although a combination of Direct Mode Entry boxes and Status/Message boxes can be used, the maximum available entries is 24.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 8 MODE DIRECT ENTRY | Corresponding Kit: H1835 | W599 | 656 | $212.00
ADD: 16 MODE DIRECT ENTRY | Corresponding Kit: H1836A | W614 | 656 | $424.00
ADD: 24 MODE DIRECT ENTRY | Corresponding Kit: H1837A | W615 | 656 | $636.00
ADD: STATUS/MESSAGE 8 | Corresponding Kit: H1838A | W355 | 656 | $560.00
ADD: STATUS/MESSAGE 16 | Corresponding Kit: H1839A | W374 | 656 | $765.00
ADD: DEK FOR WHELEN SIREN | Corresponding kit: H1883 | GA00814 | 656 | $124.00
ADD: DEK FOR WHELEN SIREN W/ O3 CH ONLY | Requires O3 CH. Corresponding kit: H1882A. | GA00812 | 656 | $124.00

#### 10: Speakers (Must Select One)

Not compatible with Control Station Operation. Control Station Operation requires No Speaker Needed (G142).

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SPKR 15W WATER RESISTANT | Corresponding kit: HSN4040 | G831 | 656 | $71.00
ADD: SPKR 7.5W WATER RESISANT | Corresponding Kit: HSN4038 | G832 | 656 | $72.00
ADD: AUXILIARY SPKR 7.5 WATT | Corresponding kit: HSN4031 | B18 | 656 | $71.00
ADD: AUXILARY COVERT SPKR 10W APX | Corresponding Kit: HSN4042 | GA01203 | 656 | $71.00
ADD: AUXILARY SPKR 13W (3.2OHM) | Corresponding kit: HSN4032 | W432 | 656 | $85.00
ADD: NO SPEAKER NEEDED | Required for Control Station Operation (W665) | G142 | 656 | $0.00

#### Auxiliary WILDCARD (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: AUXILIARY SWITCH PANEL | Corresponding kit: HLN1196. Remote Mount Required. NOT compatible with O3 control head or motorcycle. | W591 | 656 | $195.00

#### Amplifier (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: RF PREAMP | Option applies only to VHF & UHF radios. | W12 | 471 | $78.00

#### Documentation (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: PRINTED TEST RESULTS APEX | - | G799 | 656 | $12.00
ADD: APX MOBILE USER GUIDE | - | G657 | 656 | $30.00

#### RFID (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: RFID LABEL | - | GA00268 | 656 | $30.00

#### 11: Service Option (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 3Y ESSENTIAL SERVICE | - | G78 | 185 | $288.00
ADD: 5Y ESSENTIAL SERVICE | - | GA00318 | 185 | $480.00
ADD: 3Y ESSENTIAL ACCIDENTAL DAMAGE | - | GA00249AE | 185 | $402.00
ADD: 5Y ESSENTIAL ACCIDENTAL DAMAGE | - | GA00255AF | 185 | $670.00
ADD: 7Y ESSENTIAL SERVICE HTM | - | HA00694 | 185 | $605.00
ADD: 7Y ESSENTIAL W ACC DMG HTM | - | HA00695 | 185 | $844.00

ASTRO Advanced Messaging Solution (AMS)

The ASTRO 25 Advanced Messaging Solutions is the latest messaging platform from Motorola Solutions and will replace ASTRO Text Messaging Service (TMS). As a complete end-to-end solution it leverages the core assets of ASTRO 25 IV&D/CID networks, ASTRO 25 radios, Integrated Command Center applications and Unified Network Services. The application allows responders to send/receive messages and run database queries from ASTRO 25 data enabled portable radios, extending real time information access to the field so dispatchers and first responders can be more efficient and achieve safer outcomes.

Provides functional parity with TMS and leverages the PremierOne messaging services platform, offering multiple configurations to enhance and extend core messaging functionality that can include queries and dispatch notifications. Based upon the configuration chosen, ASTRO 25 Advanced Messaging Solution extends Computer Aided Dispatch (CAD) information beyond the vehicle to select ASTRO 25 Portable radios.

Many Public Safety agencies have experienced the benefits of messaging and sharing important information to/from the communication center (dispatch) and vehicles equipped with MDT's. With ASTRO 25 Advanced Messaging Solution we are extending that capability to responders when Outside the Vehicle.

ASTRO Advanced Messaging Solution will be available on APX 7000 Dual Display Portable radios. Advanced Messaging is NOT supported on APX 7000 Top Display Portable radios.

Ordering ASTRO Advanced Messaging Solution for APX Mobiles Require: (Note: some control heads are not available on all main models)

- O9, O7, O5, E5, O3 or O2 Control Heads
- With O2, E5 or O5 Control Heads Require Keypad Mic (W20)
- ASTRO Digital CAI Operation (G806)
- P25 Conventional (G48)
- Packet Data Interface (W947)

OR

- O9, O7, O5, E5, O3 or O2 Control Heads
- With O2, E5 or O5 Control Heads Require Keypad Mic (W20)
- ASTRO Digital CAI Operation (G806)
- SmartZone Operation (G51)
- ASTRO Project 25 Trunking Software (G361)
- Packet Data Interface (W947)

NOTE: There is no specific option to order for the Advanced Messaging Solution on the subscribers as the functionality is included in the Packet Data option. Also, the text messaging functionality carries a per-radio charge on the server side of $50 (one time license fee to access messaging services) per radio. When adding query the fee is $125 per radio. For additional ordering guidelines of the AMS feature which includes the server and radio license fees, please visit - ASTRO25 Advanced Messaging

Control Station Tray and Power Supply

Customer Programming Software

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
CABLE CH, PROGRAMMING,USB | HKN6184C - Used to program the radio with Customer Programming Software and Tuner Software. Compatible with APX mobile radios. | HKN6184C | 261 | $243.00

Programming and Data Cables
(Please see CPS PART NUMBER GUIDE for cable descriptions)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
CABLE KIT 20' DATA | RS232 Data Interface Cable - REMOTE | HKN6161 | 500 | $50.00
CABLE CH, PROGRAMMING,USB | HKN6184C - Used to program the radio with Customer Programming Software and Tuner Software. Compatible with APX mobile radios. | HKN6184C | 261 | $243.00

DEK/VIP

#### Siren & Interface Module

Please visit the SLIM Product Page

#### In-Vehicle Router Based Solutions

Please visit the In-Vehicle Router Based Solutions Product Page. It includes the catalog pages for Sierra Wireless' MG90, the MP70 and the RV55.

### Software and Services

### Ship Card

- CLICK HERE to see the Latest Lead Time Estimates

- CLICK HERE to see the Latest Lead Time Estimates

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
ALARMCONT | MWR | DDN1775B | COMPUTER PERIPHERAL,SLIM POWER HARNESS | 818 | 2
ALARMCONT | MWR | DDN1776B | CABLE, HARNESS,SLIM POWER HARNESS | 818 | 2
DATATERM | FSA | H1838 | 8 STATUS MESSAGE DEK KIT | 656 | 3
APX_PORTABLE | US1 | HA00677AA | ADD: PSU CONV SCAN | 0579 |
PARTS | CDP | HAD4006 | ANTENNE MOB. 136-144MHZ, 1/4 D'ONDE | 554 | 8
PARTS | CDP | HAD4006 | ANTENNE MOB. 136-144MHZ, 1/4 D'ONDE | 554 | 8
PARTS | CDP | HAD4007 | ANTENNE MOB. 144-152MHZ, 1/4 D'ONDE | 554 | 5
PARTS | CDP | HAD4007 | ANTENNE MOB. 144-152MHZ, 1/4 D'ONDE | 554 | 5
PARTS | CDP | HAD4007 | ANTENNE MOB. 144-152MHZ, 1/4 D'ONDE | 554 | 5
PARTS | CDP | HAD4008 | ANTENNE MOB. 152-162MHZ, 1/4 D'ONDE | 554 | 12
PARTS | CDP | HAD4008 | ANTENNE MOB. 152-162MHZ, 1/4 D'ONDE | 554 | 12
PARTS | CDP | HAD4008 | ANTENNE MOB. 152-162MHZ, 1/4 D'ONDE | 554 | 12
PARTS | CDP | HAD4009 | ANTENNE MOB. 162-174MHZ, 1/4 D'ONDE | 554 | 2
PARTS | CDP | HAD4009 | ANTENNE MOB. 162-174MHZ, 1/4 D'ONDE | 554 | 2
PARTS | PDC | HAD4009 | ANTENNE MOB. 162-174MHZ, 1/4 D'ONDE | 554 | 28
PARTS | VAN | HAD4009 | ANTENNE MOB. 162-174MHZ, 1/4 D'ONDE | 554 | 28
PARTS | CDP | HAD4017A | ANT ROOF MT WB VHF 146/174 | 554 | 9
PARTS | CDP | HAD4017A | ANT ROOF MT WB VHF 146/174 | 554 | 9
PARTS | CDP | HAD4017A | ANT ROOF MT WB VHF 146/174 | 554 | 9
FIXEDSTN | CDP | HAD4022A | ANTENNA 132-174 3DB GAIN | 554 | 204
FIXEDSTN | CDP | HAD4022A | ANTENNA 132-174 3DB GAIN | 554 | 204
FIXEDSTN | CDP | HAD4022A | ANTENNA 132-174 3DB GAIN | 554 | 204
PARTS | CDP | HAF4013 | ANTENNA (762-870 MHZ) 3DB LOW-PROFILE | 554 | 3
PARTS | CDP | HAF4013 | ANTENNA (762-870 MHZ) 3DB LOW-PROFILE | 554 | 3
PARTS | CDP | HAF4013 | ANTENNA (762-870 MHZ) 3DB LOW-PROFILE | 554 | 3
PARTS | SCB | HAF4014 | ANTENNA (762-870 MHZ) 3DB ELEVATED FEED | 554 | 6
PARTS | SCB | HAF4014 | ANTENNA (762-870 MHZ) 3DB ELEVATED FEED | 554 | 6
PARTS | SCB | HAF4016 | ANTENNA (762-870 MHZ) 1/4 WAVE | 554 | 7
PARTS | SCB | HAF4016 | ANTENNA (762-870 MHZ) 1/4 WAVE | 554 | 7
PARTS | SCB | HAF4016 | ANTENNA (762-870 MHZ) 1/4 WAVE | 554 | 7
PARTS | CDP | HAF4017 | ANTENNA (762-870 MHZ) 3DB GAIN COLLINEAR | 554 | 3
PARTS | CDP | HAF4017 | ANTENNA (762-870 MHZ) 3DB GAIN COLLINEAR | 554 | 3
PARTS | CDP | HAF4017 | ANTENNA (762-870 MHZ) 3DB GAIN COLLINEAR | 554 | 3
PARTS | CDP | HAF4017 | ANTENNA (762-870 MHZ) 3DB GAIN COLLINEAR | 554 | 16
PARTS | PGF | HKN4191 | POWER CABLE, 10 FT. (LOW/MID POWER) 30 & 35 WATT | 706 | 105
PARTS | PGF | HKN4191 | POWER CABLE, 10 FT. (LOW/MID POWER) 30 & 35 WATT | 706 | 105
PARTS | PGF | HKN4191 | POWER CABLE, 10 FT. (LOW/MID POWER) 30 & 35 WATT | 706 | 105
PARTS | PGF | HKN4191 | POWER CABLE, 10 FT. (LOW/MID POWER) 30 & 35 WATT | 706 | 105
PARTS | PGF | HKN4191 | POWER CABLE, 10 FT. (LOW/MID POWER) 30 & 35 WATT | 706 | 105
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
PARTS | CDP | HKN6110 | CABLE, POWER, 100W | 362 | 13
PARTS | CDP | HKN6158 | AUDIO CABLE ADAPTER | 706 | 66
PARTS | CDP | HKN6159 | ADAPTER CABLE DATA | 706 | 13
MOBILES | PGF | HKN6161 | CABLE KIT 20' DATA | 500 | 119
MOBILES | FSA | HKN6161 | CABLE KIT 20' DATA | 500 | 4
PARTS | CDP | HKN6164 | CABLE,REMOTE MOUNT,131 FT | 362 | 5
PARTS | CDP | HKN6165 | CABLE, REMOTE MOUNT, 115 FT | 362 | 4
PARTS | CDP | HKN6165 | CABLE, REMOTE MOUNT, 115 FT | 362 | 4
PARTS | CDP | HKN6166 | CABLE, REMOTE MOUNT, 75 FT | 362 | 6
PARTS | CDP | HKN6167B | CABLE, REMOTE MOUNT, 15M | 362 | 9
PARTS | CDP | HKN6167B | CABLE, REMOTE MOUNT, 15M | 362 | 3
PARTS | PGF | HKN6169B | CABLE, REMOTE MOUNT, 5M | 362 | 10
PARTS | PGF | HKN6169B | CABLE, REMOTE MOUNT, 5M | 362 | 10
PARTS | CDP | HKN6169B | CABLE, REMOTE MOUNT, 5M | 362 | 6
PARTS | PDC | HKN6169B | CABLE, REMOTE MOUNT, 5M | 362 | 4
PARTS | VAN | HKN6170 | CABLE, REMOTE MOUNT, 10 FT | 362 | 19
PARTS | PDC | HKN6184C | CABLE CH, PROGRAMMING,USB | 261 | 2
PARTS | PDC | HKN6184C | CABLE CH, PROGRAMMING,USB | 261 | 2
PARTS | PDC | HKN6184C | CABLE CH, PROGRAMMING,USB | 261 | 2
PARTS | CDP | HKN6184C | CABLE CH, PROGRAMMING,USB | 261 | 2
PARTS | PDC | HKN6184C | CABLE CH, PROGRAMMING,USB | 261 | 532
PARTS | CDP | HKN6239A | KIT, ADK1.1 CABLE WITH GCAI & DB25 CONNECTORS INCL. 1-WIRE | 986 | 5
MOBILES | FSA | HLN1196 | WILDCARD | 362 | 145
MOBILES | FSA | HLN1196 | WILDCARD | 362 | 145
PARTS | CDP | HLN1457 | HANDSET/HANGUP (HANGUP CUP) | 706 | 69
PARTS | CDP | HLN5113 | EMERGENCY FOOT SWITCH | 706 | 14
PARTS | CDP | HLN5113 | EMERGENCY FOOT SWITCH | 706 | 14
PARTS | CDP | HLN5113 | EMERGENCY FOOT SWITCH | 706 | 14
PARTS | RNS | HLN6042 | MOBILE DESK TRAY | 706 | 17
PARTS | RNS | HLN6042 | MOBILE DESK TRAY | 706 | 17
PARTS | RNS | HLN6042 | MOBILE DESK TRAY | 706 | 17
PARTS | RNS | HLN6042 | MOBILE DESK TRAY | 706 | 17
PARTS | PGF | HMN4079D | XTL5000 KEYPAD MICROPHONE | 706 | 1
PARTS | CDP | HMN4097A | MODEL III KEYPAD TELEPH HANDSET KIT | 706 | 3
PARTS | CDP | HMN4097A | MODEL III KEYPAD TELEPH HANDSET KIT | 706 | 3
PARTS | CDP | HMN4097A | MODEL III KEYPAD TELEPH HANDSET KIT | 706 | 6
PARTS | PDC | HSN4032B | MCS EXT SPKR 13W | 706 | 3
PARTS | PDC | HSN4032B | MCS EXT SPKR 13W | 706 | 3
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | CDP | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 10
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 38
PARTS | PGF | HSN4039 | EXTERNAL 13W WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 19
PARTS | PDC | HSN4039 | EXTERNAL 13W WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 11
PORTABLES | VAN | HSN4040A | EXTERNAL WATER RESISTANT SPEAKER 15 WATTS | 706 | 3
PARTS | PGF | HSN6003B | MCYCLE WP SPEAKER | 500 | 18
PARTS | FSA | HSN6003B | MCYCLE WP SPEAKER | 500 | 16
MOBILES | FSA | M25KSS9PW1 N | APX6500 VHF MID POWER | 527 | 14
MOBILES | FSA | M25QSS9PW1 N | APX6500 UHF R1 MID POWER | 527 | 18
MOBILES | FSA | M25SSS9PW1 N | APX6500 UHF R2 MID POWER | 527 | 129
MOBILES | FSA | M25URS9PW1 N | APX6500 7/800 MHZ MID POWER MOBILE | 527 | 10
PARTS | CDP | PMKN4033A | CABLE, MOBILE MIC EXTENSION, 10FT | 706 | 5
PARTS | CDP | PMKN4033A | CABLE, MOBILE MIC EXTENSION, 10FT | 706 | 5
PARTS | CDP | PMKN4033A | CABLE, MOBILE MIC EXTENSION, 10FT | 706 | 11
PARTS | PDC | PMLN4958B | O3 CAN 17' EXTENSION CABLE | 362 | 8
PARTS | PDC | PMLN4958B | O3 CAN 17' EXTENSION CABLE | 362 | 8
PARTS | CDP | PMLN4958B | O3 CAN 17' EXTENSION CABLE | 362 | 41
APX_PORTABLE | US1 | QA01648AA | ADD: HW KEY SUPPLEMENTAL DATA | 0655 |
APX_PORTABLE | US1 | QA05751AA | ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | 0655 |
PARTS | PGF | RAD4002ARB | ANTENNA VHF 1/4 WAVE | 554 | 70
PARTS | CDP | RAD4002ARB | ANTENNA VHF 1/4 WAVE | 554 | 15
PARTS | CDP | RAD4004ARB | ANTENNA VHF 1/4 WAVE | 554 | 3
PARTS | CDP | RAD4004ARB | ANTENNA VHF 1/4 WAVE | 554 | 3
PARTS | CDP | RAD4005ARB | ANTENNA VHF 1/4 WAVE | 554 | 5
PORTABLES | PGF | RLN5926A | PUSH BUTTON PTT | 706 | 20
PORTABLES | PGF | RLN5926A | PUSH BUTTON PTT | 706 | 20
PORTABLES | PGF | RLN5926A | PUSH BUTTON PTT | 706 | 20
PARTS | PGF | RMN5070A | AS. SPECTRA & XTL5000 DESKTOP MIC | 706 | 13
PARTS | PGF | RMN5070A | AS. SPECTRA & XTL5000 DESKTOP MIC | 706 | 13
PARTS | CDP | TDN6251 | SPEAKER SIREN, ROUND W/CHROME & BLACK | 706 | 2
PARTS | CDP | TDN6252 | SPEAKER RECTANGULAR WITH CHROME FINISH | 706 | 2
PARTS | CDP | TDN6253 | SPEAKER UNDERHOOD WITH GRAY FINISH | 706 | 4
PARTS | CDP | TDN6254 | SPEAKER ROUND WITH GRAY FINISH | 706 | 2
QUOTEDS | WDE | TT2592 | WHELEN/MOTOROLA SIREN | 256 | 42
ALARMCONT | MWR | TT2723B | SLIM KIT (MODULE+GPIO+PWR+AUDIO) | 818 | 651

### Update History

Starting January 1 2015.The SOFTWARE KEY (QA01749) is the default Advance System Key, it ships by default on all APX products; The HARDWARE KEY can be ordered instead by using QA01648. The DVN4046 Master Key Starter Kit is required for the Hard Key or to operate on a thrid-party Trunking system. The CORRECT System Owner ID will be required upon ordering the Hard Key or DVN Kit. Details can be found on the Advanced System Keys-ASK for RSD Subscriber ECAT page Be sure to enter the CORRECT SYSTEM OWNER ID when supplemental data is required. If an INCORRECT ID is entered, a FLASHport order is required to fix the error.