Back

##### APX 6500 Enhanced

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Software and Services
- Ship Card

Back

##### APX 6500 Enhanced

### Model

·

·

·

·

ASTRO® Digital APX 6500 Enhanced Mobile Subscriber

700/800 MHz
764-776 MHz (3-30 W); 851-870 MHz (3-35 W)

800/900 MHz 806-825 MHz, 851-870 MHz (3-35W); 896-902 MHz, 935-941 MHz (1-30W)

VHF
136-174 (1-50 W)

UHF R1
380-470 MHz (1-40 W)

Self-Quieting Spurs
7/800: None

VHF: 153.6 MHz

UHF R1: 438.681 MHz, 438.706 MHz

UHF R2; 511.805. MHz

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

Beginning September 2023 APX radios can be ordered with the New Feature/Latest release or the Baseline release firmware. The Baseline release is defined as a single major software release (i.e. 202X.1) to ship from the factory for a 1 year duration. The first major release each year will be the Baseline Release. A New Feature Release is defined as the second and third major releases each year (202X.2 and 202X.3) and is required for customers to access new feature content and/or products. New Feature releases contain the current year’s Baseline content as well as content from the previous New Feature release.

IMPORTANT! Radios that are ordered via COF must add the Baseline Release option (QA09113) if the Baseline firmware is desired. If the Baseline option (QA09113) is not added to COF orders, radios will ship with the Latest Release and cannot be rolled back to the Baseline Release. Most quotes and orders should keep the default Baseline Firmware (QA09113) unless a customer desires new functionality only provided in a New Feature release. More information about the Baseline and New Feature Release strategy can be found in MTN-0111-23-NA.

Effective October 11th, 2021: APX Mobile One Touch Feature enhanced and integrated with DEK’s Status Message functionalities. Users benefit from the ability to program and assign alias Status Messages on the APX Control Head display. One Touch Feature G683 pricing increased from $75 to $125.

Effective August 1st 2021: E5 control head pricing increased from $572 to $652.

Effective July 19th 2021 All APX Mobile Orders Booked: The APX Mobile Bluetooth feature available on APX 8500 and Enhanced “BN” APX Mobiles. The E5 Control Head supports COTS Bluetooth and MPP Bluetooth Pairing. The O7, O3 & O2 Control Heads support COTS Bluetooth ONLY. Bluetooth included on all APX Mobile orders and reflected in the Flashcode unless DELETE Bluetooth option (QA05336) is used to remove it. A Wifi/Bluetooth antenna is required to enable the Bluetooth functionality. Flashport upgrades will also be supported. Bluetooth is not supported on the APX Consolette or APX Dual Radio.

Effective October 5th, 2020: All U.S. orders require an encryption selection. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. G193/Q667 ADP only is also available at $0. Please see encryption section for AES and other encryption options that come with ADP. Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.

Effective, June, 2020: New enhanced "BN" models and the E5 Control Head (GA01670) are orderable.

Effective Effective August 1, 2020: The O5 control head (option G442 and kit H1904) has been canceled and replaced by the E5 GA01670 and H1930

Effective August 26, 2019: Multi-System OTAR (GA01620) is available. Users who frequently move from one secure system to another will benefit from the ease and speed that radio keys are shared and updated. Our Multi-System Over-the-Air Rekeying (Multi-System OTAR) feature supports over-the-air-rekeying with up to 19 different secure systems, key sharing across profiles and seamless migration of fielded radios. The customer must order OTAR W/ MULTIKEY as a prerequisite for MS-OTAR.

Retrofit kits and FLASHport for the Enhanced Models are now available. Please choose the correct vintage when ordering an APX kit.

### Ordering Information

#### Please Read All Option Descriptions Before Making Your Selection

Required Selections:

1) Main Model

2) Mounting

3) Control Head Selection

4) RF Antenna

5) Operation Mode

6) Feature Antenna(s)

7) Encryption

8) Remote Mount Cables (if remote mount is selected)

9) Microphone

10) Speaker

11) Service

#### Additional Ordering Information for Service Options

SmartConnect End to End Ordering Guide

### Configuration (NOTE: Base price does not include antennas (Rf and GPS), speaker or mount type selections – must be picked from below)

1: Base Radio $8,181.42 List $4,499.78 Disc $3,249.78 w/Trade

Description | Full Description | Nomenclature | APC | Price
APX6500 ENHANCED 7/800 MHZ |  | M25URS9PW1BN | 527 | inc.
ADD: APX CONTROL HEAD SOFTWARE |  | G444 | 656 | inc.
ADD: ASTRO DIGITAL CAI OPERATION |  | G806 | 656 | inc.
ENH: SMARTZONE OPERATION APX6500 |  | G51 | 527 | inc.
ENH: P25 TRUNKING SOFTWARE APX |  | G361 | 656 | inc.
ADD: ENHANCED DATA APX |  | QA03399 | 656 | inc.
ADD: GROUP SERVICES |  | GA09008 | 656 | inc.
ENH: OVER THE AIR PROVISIONING |  | G996 | 656 | inc.
ENH: ENH: RADIO TRACE |  | G170 | 656 | inc.
ADD: TDMA OPERATION APX |  | GA00580 | 656 | inc.
ADD: HW KEY SUPPLEMENTAL DATA |  | QA01648AA | 0655 | inc.
ADD: APX E5 CONTROL HEAD |  | GA01670 |  | inc.
ADD: KEYPAD MIC GCAI |  | W20 |  | inc.
ADD: SMARTCONNECT |  | GA01630 | 681 | inc.

#### 2. Mounting (Must Select One)

If a remote mount cable other than 5 meters (17ft) is desired for Remote Mount, please reference the "Remote Mount Cables" section.

The O3 dash and remote mount configurations are the same except that the dash mount configurations do not come with the 17ft extension cable, PMLN4958.

Description | Full Description | Nomenclature | APC | Price
ADD: DASH MOUNT | Required for Control Station Operation. | G66 | 656 | $148.00
ADD: REMOTE MOUNT APXM | - | G67 | 527 | $350.00

#### Motorcycle Mounting (Optional)

HMN1079 (Motorcycle Mic) and HSN4031 (Speaker) are mandatory selections with motorcycle configurations. Motorcycle mount requires the O2, E5, or O7 Control Head and Remote Mount (G67). CAN cables are not compatible with motorcycle. This option includes a weatherized harness. Incompatible with DVRS MSU operation (GA00631) and 800/900 MHz model (M25VRS9PW1CN).

Description | Full Description | Nomenclature | APC | Price
ADD: APX MOTORCYCLE CH SFWR | Requires G67 (Remote Mount) | G138 | 656 | $0.00
ADD: NO CH MOTORCYCLE APXM | - | G67DV | 527 | $471.00
ADD: O2 MOTORCYCLE APXM | - | G67DW | 527 | $471.00
ADD: E5 MOTORCYCLE APXM | - | G67DY | 656 | $471.00
ADD: O7 MOTORCYCLE APXM | - | G67DZ | 527 | $471.00

#### Trunnion Screws (Optional)

The APX 6500 Enhanced model will ship with HLN6861 to accommodate a smaller, lighter form factor. If it is required to use the previous APX 6500 model trunnion, HLN7002, order GA01693, which provides KT000053A01, screws that will fit the previous trunnion.

Description | Full Description | Nomenclature | APC | Price
ADD : LEGACY TRUNNION SCREW KIT | Corresponding kit: KT000053A01 | GA01693 | 471 | $12.00

#### Control Station Operation (Optional)

O2, E5, & O7 Control Heads Only. Must select one.

Requires Dash Mount (G66)

Some microphones are not compatible with Control Station Operation. Please read descriptions carefully.

Although optional, the Power Supply is needed for full Control Station operation.

Power Supply HPN4007 (used in Control Station configuration for AN Models) is not approved for use on Enhanced Models. Please use KT000254A02 (G91).

#### 3B Control Head Options (Select if included E5 head is not desired)

Description | Full Description | Nomenclature | APC | Price
REMOVE 05 HEAD |  |  |  | $(767.00)

O2 Control Head Options

Description | Full Description | Nomenclature | APC | Price
ADD:IMPACT GREEN COLOR HOUSING (O2) | When ordered in conjunction with GA00804 you will get a green colored O2 housing. | G201 | 656 | $30.00
ADD: SCHOOL SERCURITY ENHANCEMENT PACKAGE | Education O2 Emergency Push Button | GA01056 | 514 | $55.00
ADD: APX O2 CH (GREY) | - | GA00804 | 656 | $579.00

O3 Control Head Options

Description | Full Description | Nomenclature | APC | Price
ADD: APX O3 HANDHELD CH | Requires No Microphone (G90). If Lights & Siren Keypad and Software is required, order GA00806. | G72 | 656 | $1,114.00
ADD:CH SIREN & LIGHTS KEYPAD | Available on O3 (G72) and O7 (GA00805) Control Heads. | GA00806 | 656 | $59.00

E5 Control Head Option

Description | Full Description | Nomenclature | APC | Price
ADD: APX E5 CONTROL HEAD | - | GA01670 | 681 | $767.00

O7 Control Head Options

Description | Full Description | Nomenclature | APC | Price
ADD: APX O7 CONTROL HEAD. | If Lights & Siren Keypad and Software is required, order GA00806. | GA00805 | 656 | $744.00
ADD:CH SIREN & LIGHTS KEYPAD | Available on O3 (G72) and O7 (GA00805) Control Heads. | GA00806 | 656 | $59.00

No Control Head Options

Description | Full Description | Nomenclature | APC | Price
ADD: APX MOBILE NO CONTROL HEAD | If you already have a control head and don't require it, select G88. Requires remote mount option (G67). | G88 | 681 | $0.00
REMOVE 05 HEAD |  |  |  | $(767.00)

#### Dual Control Head (Optional)

The APX 6500 mobile can support up to two control heads on a single transceiver. This allows control of a single APX 6500 transceiver from two different control head locations.

Dual Control Head requires Remote Mount.

When ordering the dual control head option, only one type of control head can be selected.

Only available with O2, E5, and O7 Control Heads.

The Dual Control Head Option requires an equal number of microphones, speakers, and CAN cables.

Please note: Audio Pod was discontinued in 2022 and the ability to perform speaker toggling between dual control heads is no longer an available option.

#### 4. RF Antenna (Required)

No Antenna Requested

Description | Full Description | Nomenclature | APC | Price
ADD: NO RF ANTENNA NEEDED | - | G89 | 656 | $0.00

7/800 Antennas

Description | Full Description | Nomenclature | APC | Price
ADD: ANT 3DB LOW-PROFILE 762-870 | Corresponding kit: HAF4013 | G174 | 656 | $50.00
ADD: ANT 1/4 WAVE 762-870 MHZ | Corresponding kit: HAF4016 | G335 | 656 | $16.00
ADD: ANT 3DB ELEVATED FEED 762-870 | Corresponding kit: HAF4014. | G175 | 656 | $89.00
ALT: ANT 3DB GAIN 762-870MHZ | Corresponding kit: HAF4017 | W484 | 656 | $45.00

#### Dual Radio Operation Options

The APX Dual Radio Feature offers the capability to control TWO (2) APX 8500, APX 7500 or APX 6500 mobile radios from ONE (1) O7 control head or E5 control head. APX Dual Radio allows for mixing and matching of radios across tiers (i.e. APX 8500 with APX 6500) and power levels (High Power with Mid Power).

Each radio in an APX Dual Radio system must be ordered independently.

The mobiles in a dual radio solution can be single or dual band. Both radios can be on the same or different frequency bands.

One radio must be ordered with the Primary Radio option (GA01113) and the other with the Secondary Radio option (GA01117). This will include both the SW and HW required for dual radio operation.

Although each radio must be ordered as either a Primary or Secondary radio, each radio can be configured to work as a Primary, Secondary, or a stand alone radio.

Only one speaker can be connected to the control head and it will play audio from the primary radio. A 30 ft. speaker extension cable is included on the secondary radio to connect the second speaker directly to the secondary radio. If a longer cable is needed, a 128 ft. version can be purchased from AAD (part # HKN6251)

The Dual Radio feature is incompatible with the multi-control head options.

Description | Full Description | Nomenclature | APC | Price
ENH: DUAL RADIO OPERATION (PRIMARY RADIO) | The Primary radio must be ordered with an O7 CH, or E5 CH. APX Dual Radio is not compatible with any other control head. The primary radio includes a short dual radio CAN cable (HKN6245) to connect both radios together. If the stack mount trunnion is ordered, a right-angle version of this cable (HKN6249) will ship instead to facilitate stack-mounted installations. If a different length is desired, the standard remote mount control head cables can also be used to connect both together. | GA01113 | 656 | $715.00
ENH: DUAL RADIO OPERATION (SECONDARY RADIO) | The secondary radio must be ordered with no control head (G88). | GA01117 | 656 | $715.00

#### Dual Radio Options

The Dual Radio trunnion is new to accommodate the smaller form factor of the Enhanced APX 6500. HLN7045A, offered on APX 6500 AN models, is not compatible with the Enhanced APX 6500. HLN7045B is compatible will all Enhanced APX 6500 and APX 8500 models.

Description | Full Description | Nomenclature | APC | Price
ADD: DUAL RADIO STACKABLE MP TRUNNION KIT | Corresponding kit: HLN7045B | GA01115 | 527 | $350.00

#### System Enhancement Options (Optional)

The following options are optional and will provide additional capabilities, if required.

Description | Full Description | Nomenclature | APC | Price
ADD: DVRS MSU ACTIVATION | Allows mobile to host A DVR, Requires Remote mount G67. Additional hardware may be needed to operate properly with a DVR Requires depot to change a mobile from a MSU to PSU. Compatible with GA09011 Data Modem Tethering. Require GA01779 (aftermarket cable KT000247A04) when both GA09011 and GA00631 are ordered. | GA00631 | 656 | $294.00
ADD: APX MOBILE RADIO AUTHENTICAT | Requires P25 9600 Trunking (G361). | GA01767 | 527 | $110.00
ADD: WI-FI CAPABILITY | Compatible with Enhanced (BN) models only. Requires a Wi-Fi antenna. Supports codeplug updates, firmware refreshes, and FLASHport upgrades over pre-provisioned wireless networks. Requires Radio Management SW (ordered separately). Must order Out of the Box Wi-Fi Provisioning option (GA09007) if provisioning the radios out of the box using Wi-Fi is desired. | GA09001 | 681 | $353.00
ADD: OUT OF THE BOX WI-FI PROVISIONING | Requires GA09001 (Wi-Fi) | GA09007 | 681 | $0.00

#### 6. Feature Antennas (Must select one)

Note: The Enhanced APX 6500 model has QMA connections for both the WiFi and GPS antenna ports. The RF antenna connection is the same mini-UHF connection as the previous models. Please order CB000091A04/GA01576 to receive an SMA to QMA adaptor cable.

Must select from either Multi-function(Bluetooth/WiFi/GNSS) section or Single function GPS section and Single Function Wi-Fi section (if GA09001 is ordered). Bluetooth requires a WiFi antenna to function.

Even though GPS comes standard, a GPS antenna, Digital and IV&D are required to implement the full solution.

Multifunction Antennas (Must Select One if Multifunction is Selected)

Requires Wi-Fi (GA09001)

Description | Full Description | Nomenclature | APC | Price
ADD: WIFI/GNSS FLEXIBLE CABLE LMR195 | Corresponding kit: AN000163A01. AN000163A05 has flexible BT/WiFi cable (PFP-195) but has 1-1.5 dB lower gain compared to AN000163A01 that has stiffer PFP-240 cable. | GA00250 | 681 | $110.00
ADD: WIFI/GNSS FLEXIBLE CABLE LMR195 | Corresponding kit: AN000163A02 Requires Motorcycle (G138) | GA00250 | 681 | $118.00
ADD: GNSS/BT-WIFI THRU MNT ANT, 17FT FLEXIBLE PFP-100A/195, QMA | Corresponding kit: AN000163A05. AN000163A01 has stiffer BT/Wi-Fi cable (PFP-240) but it has 1-1.5 dB better gain compared to AN000163A05 that has flexible PFP-195 cable. | GA00250AC | 681 | $130.00

GPS Antennas (Must select one)

Description | Full Description | Nomenclature | APC | Price
ADD: COVERT GNSS GLASSMOUNT LMR100 | Corresponding kit: PMAN4109 | GA01580AA | 681 | $82.00
ADD: GPS/GNSS MAG MOUNT ANTENNA | Corresponding kits: CB000091A04, & PMAN4010 | GA01305 | 656 | $71.00
ADD: GPS ANTENNA | Requires GA01576. Corresponding kit: HAG4000 | GA00226 | 656 | $89.00
ADD: GPS ANTENNA MTCL | Corresponding kit: HAG4001. Requires Motorcycle (G138). | GA00269 | 656 | $89.00

GPS Antenna Adaptor

Description | Full Description | Nomenclature | APC | Price
ADD: SMA TO QMA ADAPTER | Requires GA01305, or GA00226. Corresponding kit: CB000091A04. Corresponding kit: CB000091A04 | GA01576 | 986 | $22.00

Wi-Fi/BT Antennas (Must select one if single function Wi-Fi/BT is requested)

Description | Full Description | Nomenclature | APC | Price
ADD: COVERT WIFI GLASSMOUNT 2.4/5 GHZ | Corresponding kit: PMAN5101 Requires Wi-Fi (GA09001). | GA01579AB | 681 | $77.00

#### 7. Encryption Algorithms (Required Selection)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

Description | Full Description | Nomenclature | APC | Price
ADD: AES ENCRYPTION APX AND ADP | Requires digital operation. P25 CAP Compliant option. Includes ADP. | G843 | 656 | $560.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP Compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | G193 | 430 | $0.00

#### Multikey (Optional)

All multikey options require an encryption algorithm selection.

Description | Full Description | Nomenclature | APC | Price
ADD: MULTIPLE KEY ENCRYPTION OPERATION | Required when using more than one encryption algorithm or encryption key. | W969 | 656 | $363.00
ADD: MULTI SYSTEM OTAR | Requires ASTRO 25 OTAR W/ MULTIKEY (G298) | GA01620 | 656 | $177.00
ENH: ASTRO 25 OTAR W/ MULTIKEY | Not compatible with ADP-Only. Requires AES. Includes multikey, trunking OTAR, and Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. Requires AES. | G298 | 656 | $814.00

#### 8. Remote Mount Cables (17 FT STD)

Multi-control head options delete the 17 FT standard cable and customers are required to order a cable per control head. Only for O5, E5 & O7 Control Heads.

Description | Full Description | Nomenclature | APC | Price
ADD:CBL REMOTE MOUNT 10 FEET | Corresponding kit: HKN6170 | G618 | 656 | $12.00
ADD: REMOTE MOUNT CBL 17 FEET | Included at no charge with Single Control Head Remote Mount installations and High Power. Corresponding kit: HKN6169 | G628 | 656 | $18.00
ADD: REMOTE MOUNT CBL 30 FEET | Corresponding kit: HKN6168 | G610 | 656 | $30.00
ADD: REMOTE MOUNT CBL 50 FEET | Corresponding kit: HKN6167 | G609 | 656 | $42.00
ADD:CBL REMOTE MOUNT 75 FEET | Corresponding kit: HKN6166A | G607 | 656 | $54.00
ADD:REMOTE MOUNT CBL 115 FEET | Corresponding kit: HKN6165 | G879 | 656 | $65.00
ADD: REMOTE MOUNT CABLE 128 FT | For dual control head configurations, the total cable length may not be greater that 131 ft (40 meters). Therefore, this cable should not be used with a dual control head configuration. Corresponding kit: HKN6164 (actual cable length is 128 ft) | G582 | 656 | $77.00

#### Data/Programming Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: USB DATA INTFC CABLE-DASH | 6 FT USB W/IGNITION SENSE Corresponding kit: HKN6163B. Can be used to program APX Mobile Radios. | G308 | 656 | $59.00
ADD:USB DATA INTFC CABLE-TRK | 16.5 FT USB W/IGNITION SENSE Corresponding kit: HKN6172B. Can be used to program APX Mobile Radios. | G309 | 656 | $59.00
ADD: RS232 DATA INTFC CBL DASH | 6 FT RS232 DATA CABLE Corresponding kit: HKN6160A. | G303 | 656 | $59.00
ADD: RS232 DATA INTFC CBL TRK | 20 FT RS232 DATA CABLE Corresponding kit: HKN6161A. | G304 | 656 | $59.00

#### Cable Accessories (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: EXTERNAL ALARM RELAY AND CABLE | For either HORN or LIGHTS. NOT both | W116 | 656 | $89.00
ADD:BUZZER 110MA APX | Corresponding Kit: HLN6953 | B116 | 656 | $59.00
ADD: GCAI EXTENSION CABLE 2 FT | For use with 07, O9 Control Heads and GCAI style Mic. KIT #PMKN4093A. | GA00589 | 656 | $35.00
ADD:REMOTE MOUNT VIP CBL APX | Park/Kill, Gunlock, 'Horn Ring/Horn Transfer' or Horn/Lights Park/Kill and Horn 'Ring/Horn Transfer' only available with Motorola Siren. Gunlock supported on O9 Control Head Only. CORRESPONDING KIT: (HKN6196B) | G322 | 656 | $42.00
ADD: UNIVERSAL RELAY CONTROLLER | Required to Control Vehicle Lights with the O3, 07 and O9 Control Heads.Requires URC Cable GA00260. | GA00259 | 656 | $294.00
ADD: CABLE URC TO TRANSCEIVER | Connects Universal Relay Controller to APX Transciver via a RJ45 and CGAI connection. | GA00260 | 656 | $18.00
ADD: KEY LOCK MOUNT APX | Remote Mount Mid Power Only. | W81 | 471 | $39.00

#### 9: Microphones (optional)

Description | Full Description | Nomenclature | APC | Price
REMOVE STD KEYPAD MIC PRICING IN BASE RADIO | IF SELECTING FROM BELOW |  |  | $(212.00)
ENH: HAND MIC,GCAI WATER RESISTANT | Corresponding kit HMN1089A | G892 | 656 | $85.00
ADD: MODEL III GCAI KEYPAD HANDSET | Corresponding kit: HMN4097A | GA00221 | 656 | $348.00
ADD:GATEWAY RSM AND WIRELESS RSM WITH VEHICLE CHARGER | Includes 12V Vehicle Charger Corresponding kit: RLN6551 | GA01354AA | 656 | $589.00
ADD:GATEWAY RSM AND WIRELESS RSM | Corresponding kit: RLN6552 | GA01439 | 656 | $461.00
ADD: CONTROL STATION DESK GCAI MIC | Dash Mount Required Corresponding Kit: RMN5070 | W382 | 656 | $199.00
ADD: STD PALM MICROPHONE APX | Corresponding kit: HMN1090 | W22 | 471 | $85.00
ADD:GATEWAY RSM | Corresponding kit: PMMN4097 | GA01438 | 656 | $148.00
ADD: VISOR MIC REMOTE MOUNT | Requires G90 No Microphone Needed & G235 Footswith PTT. Kit Number: RMN5054_ | W872 | 656 | $35.00
ADD: GOOSENECK PTT | Requires W872 Visor Mic. Kit Number: HMN1087A | G233 | 656 | $66.00
ADD: PTT FOOTSWITCH | Requires W872 Visor Mic. Kit Number: GLN7278_ | G235 | 656 | $60.00
ADD: STD PALM MICROPHONE APEX | Corresponding kit: HMN1090. Only microphone compatible with motorcycle operation. | W22 | 656 | $85.00
ADD: NO MICROPHONE NEEDED | Select this option when ordering O3 Handheld Control Head (G72). If ordering with Motorcycle G138 the DB 25 connector on harness needs to be sealed to prevent corrosion. | G90 | 656 | $0.00
ADD: HANDSET WITHOUT KEYPAD | Corresponding kit: HMN4098 | QA08865 | 656 | $202.00

#### Emergency

Description | Full Description | Nomenclature | APC | Price
ADD: EMERGENCY ID EXT. FOOTSWITCH | Corresponding kit: HLN5113. | W470 | 656 | $66.00
ADD: EXTERNAL EMERGENCY PUSHBUTTON | Corresponding kit: HLN5131 | W688 | 656 | $66.00

#### Direct Mode Entry & Status/Message (Optional)

DEKs are incompatible with the O3 Control Head (except for DEK for Whelen Siren - GA00814). They require Remote Mount Configuration.

Please note, 24 modes are the maximum number of modes available. Although a combination of Direct Mode Entry boxes and Status/Message boxes can be used, the maximum available entries is 24.

Description | Full Description | Nomenclature | APC | Price
ADD: 8 MODE DIRECT ENTRY | Corresponding Kit: H1835 | W599 | 656 | $212.00
ADD: 16 MODE DIRECT ENTRY | Corresponding Kit: H1836A | W614 | 656 | $424.00
ADD: 24 MODE DIRECT ENTRY | Corresponding Kit: H1837A | W615 | 656 | $636.00
ADD: STATUS/MESSAGE 8 | Corresponding Kit: H1838A | W355 | 656 | $560.00
ADD: STATUS/MESSAGE 16 | Corresponding Kit: H1839A | W374 | 656 | $765.00
ADD: DEK FOR WHELEN SIREN | Corresponding kit: H1883 | GA00814 | 656 | $124.00
ADD: DEK FOR WHELEN SIREN W/ O3 CH ONLY | Requires O3 CH. Corresponding kit: H1882A. | GA00812 | 656 | $124.00

#### 10: Speakers (Must Select One)

Not compatible with Control Station Operation. Control Station Operation requires No Speaker Needed (G142).

Description | Full Description | Nomenclature | APC | Price
ADD: SPKR 15W WATER RESISTANT | Corresponding kit: HSN4040 | G831 | 656 | $71.00
ADD: SPKR 7.5W WATER RESISANT | Corresponding Kit: HSN4038 | G832 | 656 | $72.00
ADD: AUXILIARY SPKR 7.5 WATT | Corresponding kit: HSN4031 | B18 | 656 | $71.00
ADD: AUXILARY COVERT SPKR 10W APX | Corresponding Kit: HSN4042 | GA01203 | 656 | $71.00
ADD: AUXILARY SPKR 13W (3.2OHM) | Corresponding kit: HSN4032 | W432 | 656 | $85.00
ADD: NO SPEAKER NEEDED | Required for Control Station Operation (W665) | G142 | 656 | $0.00
ADD: AUXILIARY SPEAKER MOTORCYCLE | Corresponding kit: HSN6003. Must select for motorcycle operation. | B18 | 656 | $71.00

#### Auxiliary WILDCARD (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: AUXILIARY SWITCH PANEL | Corresponding kit: HLN1196. Remote Mount Required. Incompatible with O3 control head or motorcycle. | W591 | 656 | $195.00

#### Motorcycle Enclosure

Required if Motorcycle Configuration requested.

Description | Full Description | Nomenclature | APC | Price
ADD: WEATHER PROOF HOUSING ENCLOSURE BLACK | Kit number: HLN7022B | W15 | 656 | $1,412.00
ADD: NO MTRCYCLE ENCL NEEDED APX | - | W620 | 656 | $0.00

#### Documentation (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: PRINTED TEST RESULTS APEX | - | G799 | 656 | $12.00
ADD: APX MOBILE USER GUIDE | - | G657 | 656 | $30.00

#### RFID (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: RFID LABEL | - | GA00268 | 656 | $30.00

#### Programming Solutions

#### 11: Service Option (Must Select One)

Effective June 13, 2020: The Essential Service option for both the U.S. and Canada will receive a 5% price increase.

Description | Full Description | Nomenclature | APC | Price
ADD: 3Y ESSENTIAL SERVICE | Provides 3 years of hardware coverage beginning at time of purchase. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | G78 | 185 | $288.00
ADD: 3Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 3 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with user of the Motorola designated delivery service.. Motorola will pay for outbound shipping via Motorola's normal shipping methods. Not discounts are allowed on this option. | GA00249AE | 185 | $402.00
ADD: 5Y ESSENTIAL SERVICE | Provides 5 years of hardware coverage beginning at time of purchase. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | GA00318 | 185 | $480.00
ADD: 5Y ESSENTIAL ACCIDENTAL DAMAGE | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 5 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | GA00255AF | 185 | $670.00
ADD: 7Y ESSENTIAL SERVICE HTM | Provides 7 years of hardware coverage beginning at time of shipment. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00694 | 185 | $605.00
ADD: 7Y ESSENTIAL W ACC DMG HTM | Provides for extended hardware repair coverage and chemical, liquid, and other physical damage on your Motorola portable and mobile subscriber radios. Comprehensive coverage starts from the first day the radio is put into use and last for 7 YEARS. Repairs will be made only at the designated Motorola repair depot. Local services are not included. Motorola will pay the inbound shipping charges only with use of the Motorola designated delivery service. Motorola will pay for outbound shipping via Motorola's normal shipping methods. No discounts are allowed on this option. | HA00695 | 185 | $844.00

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
RadioManagement (On-Prem) | See “How to Order” section in the Ordering Guide below. | N/A | N/A | N/A

Programming and Data Cables
(Please see CPS PART NUMBER GUIDE for cable descriptions)

Description | Full Description | Nomenclature | APC | Price
CABLE KIT 20' DATA | RS232 Data Interface Cable - REMOTE | HKN6161 | 500 | $50.00
CABLE CH, PROGRAMMING,USB | HKN6184C - Used to program the radio with Customer Programming Software and Tuner Software. Compatible with APX mobile radios. | HKN6184C | 261 | $243.00

#### Accessories

The accessories available are not limited to this list. Please refer to the Accessory Catalog for additional info.

Description | Full Description | Nomenclature | APC | Price
WM800 WIRELESS RSM WITH BATTERY | - | PMMN4158B | 372 | $602.00

#### Siren & Interface Module

Please visit the SLIM Product Page

#### In-Vehicle Router Based Solutions

Please visit the In-Vehicle Router Based Solutions Product Page. It includes the catalog pages for Sierra Wireless' MG90, the MP70 and the RV55.