Back

##### MCD 5000 Deskset System

###### Product Catalog

##### Jump to ...

- Model
- Ordering Information
- Configuration
- Ship Card

Back

##### MCD 5000 Deskset System

### Model

MCD 5000 DESKSET SYSTEM

### Ordering Information

#### General Information

ANNOUNCING FOUR CHANNEL FUNCTIONALITY
As of November 23, 2020, all Desksets/RGU's will be built standard with the Four Channel Feature (R2.4). This will allow a deskset user to connect to and monitor up to four radios at one time. The current and prior versions of the MCD 5000 Deskset only supported the connection of one radio. If a customer would like to upgrade deployed units with the Four Channel feature, they will need to purchase the Four Channel License/Software. See step 8 below for ordering instructions
Release 2.4 also allows the support of the APX Consolette E5 configuration.

MCD 5000 DESKSET SYSTEM OVERVIEW:

The MCD 5000 Deskset System is the Motorola Solution's next generation radio dispatch deskset platform that utilizes VoIP technology. The MCD 5000 Deskset can be deployed on existing customer's IP network or on a stand-alone IP network. The MCD 5000 Deskset is part of the MCD 5000 Deskset System that provides radio dispatch capability when connected to a two-way radio device. MCD 5000 Desksets can be placed anywhere on the IP network. Each MCD 5000 Deskset can connect up to four radio devices at a time. The MCD 5000 Deskset may connect directly to a radio or connect up to four radios over IP network via the MCD 5000 Radio Gateway Units (RGU).

The MCD 5000 Deskset can be used where MC3000, MC1000 and MC2000 desksets have been used in the past. In addition, it can be used with the APX Consolette and/or a MOTOTRBO XPR5550e.

The MCD 5000 Deskset can connect to the following radios:

- ASTRO XTL5000 Consolette (W9): ASTRO Spectra Consolette, ASTRO Spectra Plus Consolette
- CDM1550 Series Radios: CDM 1550, CDM 1550 LS, CDM 1550 LS+ - See Note Below
- MCS 2000 Model III Control Station - See Note Below
- APX Consolette (via IP)- 05 and E5 Control Head. (E5 CH New in R02.04.00)
- 2-Wire or 4-Wire Tone Remote Control (TRC) devices
- 4-Wire E&M devices
- Dimetra-TETRA Mobile Radios (MTM5400 & MTM800E)
- MOTOTRBO XPR5550e Control Station (NEW in R02.03.00)

Note: The CDM1550 Series Radios and MCS 2000 Model III Control Station will not be supported starting in release 2.3.4 (Nov 18, 2019 release). If the customer still wants to use these radios, they can downgrade the Deskset and RGU to any release prior to 2.3.4.

MCD 5000 DESKSET SYSTEM Current Shipping Release R02.04.00 (Dec. 2020):

Changes, New Features and Enhancements with MCD 5000 Deskset System in R02.04.00:

- Four Channel Support – connections of 1-4 radios
- Added Support for APX All-Band Consolette with E5 CH
- Defect Fixes/Enhancements

WHERE TO GO TO LEARN MORE ABOUT THE MCD 5000 DESKSET SYSTEM:

- System Planner: is available on the MCD 5000 Deskset System Google Site
- Manuals: The various manuals for the MCD 5000 Deskset can be downloaded from the ASTRO Dispatch Documentation Site

#### MCD 5000 Deskset System Components

The MCD 5000 Deskset System consists of the following components:

- MCD 5000 DESKSET - IP-based deskset that provides dispatch capability when connected to a radio. Each MCD 5000 Deskset can connect to and monitor up to four radio channels at a time.

- DESKSET AUDIO ACCESSORIES (optional) – each MCD 5000 Deskset is capable of supporting one Desktop Paddle Microphone or one Headset Jackbox in addition to a Push-To-Talk (PTT) Foot Switch.

- MCD 5000 RADIO GATEWAY UNIT (RGU) – is used to connect radios to the MCD 5000 Deskset System. Each MCD 5000 RGU can interface up to 4 radios to the MCD 5000 Deskset System IP network. A MCD 5000 Deskset user can create a talkpath over the IP network to a radio resource connected to the MCD 5000 RGU. The MCD 5000 Deskset can connect to and monitor up to four radio channels at a time.

- IP NETWORK –can be deployable on customer's existing WAN/LAN IP Network or on a dedicated IP network for the deskset system.

- TWO-WAY RADIO DEVICES – are used with the MCD 5000 Deskset to provide access to the customer’s land mobile radio (LMR) system.
  - ASTRO XTL5000 Consolette (W9): ASTRO Spectra Consolette, ASTRO Spectra Plus Consolette
  - CDM1550 Series Radios: CDM 1550, CDM 1550 LS, CDM 1550 LS+ - See Note Below
  - MCS 2000 Model III Control Station - See Note Below
  - APX Consolette (via IP) - O5 and E5 Control Head (E5 CH New in R02.04.00)
  - Direct Connection to 2 or 4 wire Tone Remote Control (TRC) devices
  - 4W-E&M Radios
  - Dimetra TETRA Mobile Radios (MTM5400 & MTM800E)
  - MOTOTRBO XPR5550e Control Station (New in R02.03.00)

Note: The CDM1550 Series Radios and MCS 2000 Model III Control Station will not be supported starting in release 2.3.4 (Nov 18, 2019 release). If the customer still wants to use these radios, they can downgrade the Deskset and RGU to any release prior to 2.3.4.

- CONFIGURATION TOOL (CT) APPLICATION – used to configure all parameters and settings on the MCD 5000 Deskset and MCD 5000 RGU. The CT Application can be located remotely anywhere on the IP network or locally using Ethernet connection. The CT Client PC runs on Microsoft Windows® 7 (64-bit) or Windows 10 Pro (64-bit) or Windows 10 loT Enterprise LTSB 2015/2016 (64-bit) O

#### Features

The MCD 5000 Deskset provides a comprehensive feature set as listed below.

DESKSET CONNECTIONS:

- IP connection to Motorola radios
- Serial (local) connection to Motorola radios
- TRC (Tone Remote Control) connection to LMR radios

DESKSET FEATURES:

- Emulates the buttons and display of the connected radio, for applicable radios
- Perform all the functions of the radio control head, for applicable radios
- Advanced Signaling capabilities such as Push-To-Talk IDs, Emergency, Call Alerts
- Ability to access different radio system types using the deskset - connect up to four radios on the network and change connection when desired
- Programmable security access to certain radio channel - ability to control permissions for individual deskset user to access each radio on the network
- Anywhere access - security PIN solution to allow employees to switch between desksets, customer sites and offices.
- Remote or Local Configuration Management

DESKSET CONTROLS:

- Large LCD Display with Menu Selection and Soft Keys
- Push-To-Talk (PTT), Base Intercom, Channel Selection, Monitor Radio Channel
- Supervisory Mode
- Parallel Deskset Communications and Status Updates
- Inbound Emergency Alarm Acknowledge and Clear
- Generate Outbound Emergency Alarm, for applicable radios
- 3x4 Keypad
- Volume Controls

DESKSET AUDIO INPUTS:

- Front Panel Push-To-Talk (PTT)- (comes standard with deskset)
- Handset with PTT- (comes standard with deskset)
- Supports one PTT Footswitch- (optional)
- Supports one Headset Jackbox OR one Desktop Paddle Microphone- (optional)
- Supports one Local Logging Port - (optional)

DESKSET MOUNTING OPTIONS:

- Desktop Mount via Adjustable Deskset Footstand (comes standard with deskset)
- Wall Mount (optional)

MCD 5000 DESKSET SYSTEM OS HARDENING CDs AVAILABLE :

MCD 5000 Deskset System does offer Windows PC Operating System Hardening CD Kits for Motorola supplied PCs.
Element hardening must be applied to every box in the MCD 5000 System.

The table below summarizes the OS Hardening CD that is available to purchase for Motorola supplied PCs ONLY based on the different MCD 5000 Deskset System types:

- MCD 5000 Deskset System (available for CT PC)

IA COMPLIANT SYSTEM | MCD 5000 DESKSET SYSTEM APPLICATION | MOTOROLA SUPPLIED PC | OS HARDENING CD PART #'s
MCD 5000 Deskset System (IA Non Compliant) | HKVN4861A ACT Application | TT3903 Z2 Mini Workstation Windows 10 loT Enterprise LTSB 2016 (64-bit) Non-Returnable | FVN5956 (Full OS Hardening)

IMPORTANT NOTE:

- The IA OS Hardening CD (FVN5956) for the MCD 5000 Deskset System is ONLY compliant with Motorola supplied PCs.
- For the CT Application, (HKVN4861A or HKVN4862A) the compliant Motorola Supplied PC's are: TT2538 (Z420-Win 7), TT2833 (Z440-Win 7), TT3106 (Z440-Win 10), TT3225 (Z2 Mini-Win 10), TT3492 (Z2 Mini G4-Win 10) and TT3903 (Z2 Mini G5-Win 10)

#### Ordering Requirements

This section will lead you through the necessary ordering steps required to order the MCD 5000 Deskset System.

NOTE: For EMEA, orders are entered in OMAR. In the "Product" field, enter "IPDESKSET" and click GO to get to the MCD 5000 Product.

STEP 1: ORDER THE MCD 5000 DESKSET

MCD 5000 Deskset is a desktop console that provides digital control to a variety of Motorola radios. The MCD 5000 Deskset may connect directly to a radio or it may connect up to four radios over an IP network via the MCD 5000 Radio Gateway Units (RGU). Through the digital control link the MCD 5000 Deskset emulates the control head of the radios allowing the deskset to perform all the functions that can be performed using the radio control head.

Below are the ordering instructions:

1. Order the MCD 5000 Deskset Hardware (F2380) - Required

NOTE: Starting in R2.5 (March 17, 2021) the Deskset is no longer shipping with a CD that contains the manuals. We moved the manuals to an online process which requires the customer to order a separate model for access to this information. It is important that you remember to add this new model... see step 2.

2. Order the MCD 5000 Documentation (HKVN4865A). Required but at zero cost. The customer will need to provide an e-mail to allow the user to access the on-line documentation via the Flexera Download tool.

3. Order a MCD 5000 Deskset Power Supply for each MCD 5000 Deskset - Required

- FHN7469A - Assy, P/S, MCD 5000 Deskset/RGU Power Supply with USA Power Cord (NA Plug)
- FHN7485A - Assy, Kit, FRU: MCD 5000 Deskset/RGU Power Supply with out Power Cord (For EU & UK order plug below)
- 3004209T01 - Power Cord (EU Plug)
- 3004209T02 - Plug, British Standard (UK Plug)

4. Order an ETHERNET CABLE for each MCD 5000 Deskset to connect to LAN Switch - Required. Available through MSI or may be customer provided.
Ethernet Cable 10' with Red and Black (FKN8695)

5. Dependent on Deskset Configuration - Order appropriate RADIO INTERFACE CABLE to connect radio to deskset directly if not using a MCD 5000 RGU.

If system configuration is "Single Deskset" connected to "Single Radio"--- then order the appropriate RADIO INTERFACE CABLE to connect radio to deskset directly:

- FKN8690 - Cable - MCD 5000 to ASTRO Consolette W9 Direct Connect
- FKN8689 - Cable - MCD 5000 to CDM 1550 Series Direct Connect - See Note Below
- FKN8688 - Cable - MCD 5000 to MCS 2000 III Direct Connect - See Note Below
- FKN8691 - Cable - MCD 5000 to MC3000 DJB for ASTRO Consolette W9
- FKN8693 - Cable - MCD 5000 to MC3000 DJB for CDM 1550 Series
- FKN8692 - Cable - MCD 5000 to MC3000 DJB for MCS 2000 III
- FKN0012 - Cable - MCD 5000 to MOTOTRBO XPR5550e Control Station
- FKN2003 - Cable - MCD 5000 to MTM5400 TETRA Mobile Direct Connect
- FKN2004 - Cable - MCD 5000 to MTM800E TETRA Mobile Direct Connect
- Standard Ethernet Cable is needed for connecting the MCD 5000 Deskset or RGU to the APX Consolette

Note: The CDM1550 Series Radios and MCS 2000 Model III Control Station will not be supported starting in release 2.3.4 (Nov 18, 2019 release). If the customer still wants to use these radios, they can downgrade the Deskset and RGU to any release prior to 2.3.4.

STEP 2: ORDER MCD 5000 DESKSET NATIVE LANGUAGE SUPPORT - OPTIONAL

The MCD 5000 Deskset provides the Software enforced licensing option for Native Language support feature.
The MCD 5000 Deskset ships standard with English on the display.
IF a 2nd/Native language (German, French or Japanese) is desired/required on the MCD 5000 deskset display,
THEN complete this Step otherwise skip to Step 3 below.
Below are the ordering instructions IF 2nd/Native Language Support is desired/required:
1. Order the HKVN4858A MCD 5000 Licensing. Quantiy is equal to the number of desksets being upgraded.
2. Enter E-mal address to receive SW License and access.

STEP 3: ORDER MCD 5000 DESKSET ACCESSORIES - OPTIONAL

The MCD 5000 Deskset ships standard with a built-in condenser microphone, an internal front panel speaker, and a K-style handset with a Push-To-Talk (PTT) button.

In addition, the following OPTIONAL MCD 5000 Deskset accessories are also available for ordering:

- MCD 5000 Deskset Wall Mount Kit (FHN7394) - Max of 1 per deskset
- PTT Footswitch (BLN6732B) - Max of 1 per desket
- Desktop Paddle Microphone (RMN5068) OR MCD 5000 Headset Jackbox (FHN7470) - Max of 1 per deskset
- Local Logging Cable (FKN8696) to connect a generic analog voice logger to deskset - Max of 1 per deskset
- VIP Cable (FKN8697) - Max of 1 per deskset

NOTE: The Desktop Paddle Microphone and Headset cannot be used simultaneously since they use the same connector on the MCD 5000 Deskset.

Below are the ordering instructions:

1. Order a MCD 5000 Deskset Wall Mount Kit (FHN7394) for each MCD 5000 Deskset - Optional

2. Order a PTT Footswitch (BLN6732B) for each MCD 5000 Deskset - Optional
NOTE: Each MCD 5000 Deskset can support up one PTT footswitch. The PTT footswitch provides two foot pedals in a rugged, metal housing with a 7 foot cable. One pedal is used for the general transmit feature while the other pedal is used for the monitor feature.

3. Order a Desktop Paddle Microphone (RMN5068) for each MCD 5000 Deskset - Optional
NOTE: Desktop Paddle Microphone and Headset cannot be used simultaneously since they use the same connector on the MCD 5000 Deskset.

4. Order a Headset for each MCD 5000 Deskset - Optional

A headset may be used with the MCD 5000 Deskset to allow the deskset user to listen to receive audio and to talk on the radio channel. The MCD 5000 Deskset supports one headset per deskset. The headset must be connected to a MCD 5000 Deskset Headset Jackbox (FHN7470).

A headset consist of two parts, a base and a top.

The Headset Base consists of an amplifier unit with volume control, an optional PTT switch, a connector for connecting to the headset jack, a clip for attaching the amplifier to the user's clothing and either a 15 or 25 foot cable for connecting to the jack.

The Headset Top consists of an earpiece, a microphone, a cable for connecting to the bottom section and a clip for attaching the cable to the user's clothing.

To use a headset with the MCD 5000 Deskset the following MUST be ordered per deskset:

- Order MCD 5000 Headset Jackbox Hardware (FHN7470)
- Order Headset Base - choice of two headset bases (RLN6098 - Headset Base with PTT switch, 15' CBL) OR (RLN6099A - Headset Base with PTT Switch, 25' CBL)
- Order Headset Top - several to choose from - see below:
  RMN5150A - Over-the-Head Monaural Headset Top with Noise Canceling Microphone
  RMN5151A - Over-the-Head Binaural Headset Top with Noise Canceling Microphone

5. Order a MCD 5000 Logger Cable (FKN8696) for each MCD 5000 Deskset - Optional
NOTE: The MCD 5000 Deskset contains a local 4W-E&M logging output with the ability to connect a generic external voice logger directly to the MCD 5000 Deskset.

6. Order a MCD 5000 VIP Cable (FKN8697) for each MCD 5000 Deskset - Optional

STEP 4: ORDER MCD 5000 RADIO GATEWAY UNITS (RGUs)

MCD 5000 RGU is used to connect radios to the MCD 5000 Deskset System. Each MCD 5000 RGU can interface up to 4 radios to the MCD 5000 Deskset System IP network. A MCD 5000 Deskset user can create a talkpath over the IP network to a radio resource connected to the MCD 5000 RGU. The MCD 5000 Deskset can connect to and monitor up to four radios at a time.

NOTE: The original model of the RGU- F7979A was cancelled in August of 2018. It was replaced by model F7879B (R2.3). The new model has refreshed hardware components but it's connectivity and functionality is identical to the original model.

The customer can integrate the F7879B model with an existing MCD 5000 Deskset System that uses RGU model F7979A. However, if the System is not currently using release R2.3 or higher, they will need to upgrade their system. The Software can be found at the following location: http://motonline.mot-solutions.com At Path = “Resource Center > Software > 2-Way > Dispatch Console > MCD 5000 Deskset System”.

Below are the ordering instructions:

1. Order the MCD 5000 RGU Hardware (F7879B) - Required

2. Order a MCD 5000 RGU Power Supply for each MCD 5000 RGU - Required

- FHN7469A - ASSY, P/S, MCD 5000 Deskset/RGU Power Supply with USA Power Cord (NA Plug)
- FHN7485A - ASSY, KIT, FRU: MCD 5000 Deskset/RGU Power Supply with out Power Cord (For EU & UK order plug below)
- 3004209T01 - Power Cord (EU Plug)
- 3004209T02 - Plug, British Standard (UK Plug)

3. Order an ETHERNET CABLE for each MCD 5000 RGU to connect to LAN Switch - Required (Available thru MSI or may be customer provided)

Ethernet Cable 10' with Red and Black (FKN8695)

4. Order the appropriate RADIO INTERFACE CABLE for each radio connected to each MCD 5000 RGU - Required

NOTE: Each MCD 5000 RGU can connect up to 4 radios.

- Cable - MCD 5000 RGU to ASTRO CONSOLETTE W9 Direct Connect (FKN8690)
- Cable - MCD 5000 RGU to CDM 1550 SERIES Direct Connect (FKN8689) - See Note Below
- Cable - MCD 5000 RGU to MCS 2000 III Direct Connect (FKN8688) - See Note Below
- Standard Ethernet Cable is needed for connecting the MCD 5000 Deskset or RGU to the APX Consolette
- Cable - MCD 5000 Deskset RGU to MTM5400 TETRA Mobile Direct Connect (FKN2003)
- Cable - MCD 5000 Deskset RGU to MTM800E TETRA Mobile Direct Connect (FKN2004)
- Cable - MCD 5000 RGU to MOTOTRBO XPR5550e Control Station (FKN0012)

Note: The CDM1550 Series Radios and MCS 2000 Model III Control Station will not be supported starting in release 2.3.4 (Nov 18, 2019 release). If the customer still wants to use these radios, they can downgrade the Deskset and RGU to any release prior to 2.3.4.

5. Order the appropriate DJB/RADIO INTERFACE CABLE for each radio connected to each MCD 5000 RGU - Required

NOTE: If installing MCD 5000 Desksets in parallel to fielded MC3000 desksets using a Digital Junction Box (DJB) – you must order the appropriate DJB / RADIO INTERFACE CABLES. Each MCD 5000 RGU can connect up to 4 radios.

- Cable - MCD 5000 RGU to MC3000 DJB for ASTRO CONSOLETTE W9 (FKN8691)
- Cable - MCD 5000 RGU to MC3000 DJB for CDM 1550 SERIES (FKN8693)
- Cable - MCD 5000 RGU to MC3000 DJB for MCS 2000 III (FKN8692)

6. Order a RGU RACKMOUNT SHELF (FTN7490) - Optional

NOTE: Each MCD 5000 RGU Rackmount Shelf can fit up to 2 MCD 5000 RGUs (F7879B) per shelf.

STEP 5: ORDER SPARES / FIELD REPLACEMENT UNITS (FRUs) - OPTIONAL

- FHN7290AS - FRU: K-Style Handset (includes coiled cable) for the MCD 5000 Deskset
- FHN7394AS - MCD 5000 Deskset Wall Mount Kit
- FKN8696AS - Cable - MCD 5000 Deskset to Logger
- FHN7470AS - MCD 5000 Headset Jackbox & Cable
- FKN8694AS - Cable - MCD 5000 Deskset to Headset Jackbox
- FHN7469AS - MCD 5000 Deskset / RGU Power Supply with USA Power Cord
- FHN7485AS - MCD 5000 Deskset / RGU Power Supply without Power Cord
- FKN8706AS - FRU: Power Cord for USA - MCD 5000 Deskset / RGU Power Supply
- FKN8695AS - Ethernet Cable 10'
- FKN8704AS - Cable - MCD 5000 RGU Ground Cable
- FKN8690AS - Cable - MCD 5000 RGU to ASTRO Consolette W9 Direct Connect
- FKN8689AS - Cable - MCD 5000 RGU to CDM 1550 Series Direct Connect
- FKN8688A - Cable - MCD 5000 RGU to MCS 2000 III Direct Connect
- FKN8691AS - Cable - MCD 5000 RGU to MC3000 DJB for ASTRO Consolette W9
- FKN8693AS - Cable - MCD 5000 RGU to MC3000 DJB for CDM 1550 Series
- FKN8692AS - Cable - MCD 5000 RGU to MC3000 DJB for MCS 2000 III
- DSF2B56AA - External DVD Drive for the Z2 Mini Workstation
- DSY7B61AA - Vesa Mounting Sleeve for the Z2 Mini Workstation

STEP 6: ORDER FOUR CHANNEL FEATURE UPGRADE - OPTIONAL

The ability to connect up to and monitor four radios at one time was implemented in R2.4 (Dec 2020). Customers with deployed systems that wish to upgrade to this feature, must purchase the Four Channel License/Software.

Below are the ordering instructions for the Four Channel Upgrade.

1. Order the MCD 5000 Licensing model for the type of MCD 5000 system configuration deployed. Enter Qty = number of desksets needing the Four Channel Support feature

Option: HKVN4860A: Four Channel Support

2. Enter Email address to receive the License and access to the FW and Configuration Tool SW needed to complete the upgrade.

### Configuration

#### Models

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
MCD 5000 DESKSET | Provides one MCD 5000 Deskset. An in-line power supply (FHN7469) and an Ethernet cable are NOT included with the MCD 5000 Deskset (F2380) and must be ordered separately. Documentation has been moved to the Flexera Download model and now must be ordered separately at zero cost (HKVN4865A). | F2380 | 202 | $2,275.00
LICENSE,CD, MCD 5000 DOCUMENTATION | Documentation has been moved to the Flexera Download model and now must be ordered separately at zero cost. Contains the following documentation: Deskset Install and Configuration Guide for Systems, System Administration Control Panel Users Guide, Deskset Users Guide and Quick Reference Guide. | HKVN4865 | 202 | $0.00
SM, RADIO GATEWAY UNIT (RGU) | Provides one MCD 5000 Radio Gateway Unit (RGU) and one RGU ground cable (FKN8704). Each RGU (F7879B) is capable of supporting up to 4 radios. A power supply (FHN7469), Ethernet cable and cabling for connecting radios to the RGU are NOT included with the RGU (F7879B) and must be ordered separately. | F7879 | 202 | $2,275.00
TECH GLOBAL EVOLUTION SERIES 19INCH NON TOUCH | 19 Inch Non Touch Display for CT/ACP Workstation | DSTG191B | 708 | $1,118.00
Z2 G9 MINI WORKSTATION NON RETURNABLE | Provides one HP Z2 workstation computer with the Windows 10 Enterprise LTSC 21H2 64 bit operating system. Also includes 1 keyboard, 1 optical mouse, 2 DisplayPort to DVI adapters, 2 DisplayPort to VGA adapters. Does NOT include an internal DVD drive. NOTE THE Z2 WORKSTATION WITH WINDOWS 10 IS NOT RETURNABLE (REALLY!!). | TT4270A | 708 | $2,551.00
HP Z2 MINI G9 VESA MOUNT | VESA compliant mounting sleeve for the HP Z2 Mini Workstation - TT4270A. | DS7Y7Q9U3 | 708 | $80.50

#### Licensing - OPTIONAL

The MCD 5000 Deskset provides software enforced licensing option for Native Language support feature.
The MCD 5000 Deskset ships standard with English on the display.
IF a 2nd/Native language (German, French or Japanese) is desired on the MCD 5000 deskset display,
THEN follow the 2 Steps below otherwise skip this Licensing section.
1. Order the HVKN4858 - MCD 5000 Native Language License. Quantity should be equal to the number of Desksets needing the upgrade.
2. Enter the E-mail address that will receive the license and SW access.

Orders for licenses require an email address to be provided with the order. Motorola emails the License Confirmation and SW access to that email once the order is placed.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
LICENSE,MCD 5000 NATIVE LANGUAGE SUPPORT | Software license that enables the MCD 5000 Deskset to support a native/2nd language (in addition to the English language shipped standard) for the MCD 5000 deskset display. The Qty ordered should be equal to the number of MCD 5000 desksets that need native/2nd language support. | HKVN4858 | 202 | $500.00

#### Accessories

Software Application

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
LICENSE,MCD 5000 DESKSET SYSTEM CONFIG TOOL - SYSTEM W/OUT OMC | Configuration Tool for Four Channel Support - MCD 5000 Deskset System. | HKVN4861 | 202 | $250.00

Direct Radio Interface Cables

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
CABLE - MCD 5000 RGU TO MCS 2000 III DIRECT CONNECT | Provides one cable for connecting a MCS 2000 Model III Control Station to a MCD 5000 RGU (F7879B). Note: This radio type will not be supported starting with release 2.3.4. If the customer wants to use these radios, they can downgrade to a release prior to R2.3.4. | FKN8688 | 202 | $100.00
CABLE - MCD 5000 RGU TO CDM 1550 SERIES DIRECT CONNECT | Provides one cable for connecting a CDM 1550 Series radio to a MCD 5000 RGU (F7879B). Note: This radio type will not be supported starting with release 2.3.4. If the customer wants to use these radios, they can downgrade to a release prior to R2.3.4. | FKN8689 | 147 | $100.00
CABLE - MCD 5000 RGU TO ASTRO CONSOLETTE W9 DIRECT CONNECT | Provides one cable for connecting an ASTRO Consolette W9 to a MCD 5000 RGU (F7879B). | FKN8690 | 202 | $100.00
MCD5000 TO MTM5400 TETRA MOBILE RADIO DIRECT CONNECT | Provides one cable for connecting an MTM5400 Tetra Mobile Radio to a MCD 5000 RGU (F7879B). | FKN2003 | 202 | $100.00
MCD5000 TO MTM800E TETRA MOBILE RADIO DIRECT CONNECT | Provides one cable for connecting an MTM800E Tetra Mobile Radio to a MCD 5000 RGU (F7879B). | FKN2004 | 202 | $100.00
CABLE RGU TO MOTOTRBO | Provides one cable for connecting a Mototrbo XPR5550e Control Station to a MCD 5000 RGU (F7879B). | FKN0012 | 202 | $150.00

Parallel with DJB Radio Interface Cables

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
CABLE - MCD 5000 RGU TO MC3000 DJB FOR ASTRO CONSOLETTE W9 | Provides one cable for connecting a MC3000 DJB with ASTRO Consolette W9 to a MCD 5000 RGU (F7879B). | FKN8691 | 202 | $100.00
CABLE - MCD 5000 RGU TO MC3000 DJB FOR MCS 2000 III | Provides one cable for connecting a MC3000 DJB with MCS 2000 Model III Control Station to a MCD 5000 RGU (F7879B). | FKN8692 | 202 | $100.00
CABLE - MCD 5000 RGU TO MC3000 DJB FOR CDM 1550 SERIES | Provides one cable for connecting a MC3000 DJB with CDM 1550 Series radio to a MCD 5000 RGU (F7879B). | FKN8693 | 202 | $100.00

Ethernet Cable

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ETHERNET CABLE 10' WITH RED & BLACK LABELS | Provides one 10 in. ethernet cable to be used with the MCD 5000 Deskset (F2380) or MCD 5000 RGU (F7879B). Note: This cable is color coded to match the connector colors of the MCD 5000 Deskset and MCD 5000 RGU. | FKN8695 | 202 | $47.00

Power Supply

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
MCD 5000 DESKSET / RGU POWER SUPPLY WITH USA POWER CORD | Provides one in-line power supply unit and a North American AC line power cord that connects directly to the MCD 5000 Deskset (F2380) or MCD 5000 RGU (F7879B) to provide power (110/220 VAC to 12 VDC). Note: This power supply is required for both F2380 and F7879B. | FHN7469 | 202 | $100.00
FRU: MCD 5000 DESKSET / RGU POWER SUPPLY W/OUT POWER CORD | Provides one power supply unit to be used with the MCD 5000 Deskset (F2380) or MCD 5000 RGU (F7879B) to provide power (110/220 VAC to 12 VDC). This part does NOT contain an AC line power cord. Power cord must be ordered separately. | FHN7485 | 202 | $85.00
CORD, POWER | EUROPE POWER CORD - Ordered with FHN7485 | 3004209T01 | 785 | $8.30
PLUG, BRITISH STANDARD | UK POWER CORD - Ordered with FHN7485 | 3004209T02 | 785 | $10.25

Deskset Accessories

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
MCD 5000 DESKSET WALL MOUNT KIT | Provides one wall mount base kit to be used for mounting a MCD 5000 Deskset (F2380) to a wall. | FHN7394 | 202 | $24.00
MCD 5000 DESKSET HEADSET JACK BOX & CABLE | Provides one MCD 5000 Headset Jackbox & cable (FKN8694) that connects to a MCD 5000 Deskset (F2380). The Headset Jackbox provides a connecton for a single headset. Compatible with both 6-wire and 4-wire headsets. A Headset Base and Headset Top are not included with Headset Jackbox and must be ordered separately. | FHN7470 | 202 | $150.00
CABLE - MCD 5000 DESKSET TO LOGGER | Provides one logger cable to connect a generic external analog voice logger directly to the MCD 5000 Deskset (F2380). | FKN8696 | 202 | $40.00
USB EXTERNAL DVD DRIVE | External DVD drive that connects to the computer via USB. May be used with the HP Z2 Mini Workstation - TT4270A. | DSF2B56AA | 708 | $172.00
DESKTOP MIC | Desktop Paddle Microphone | RMN5068A | 706 | $130.00
FOOT, SWITCH TRADITIONAL | PTT Footswitch - Max of 1 per Deskset | BLN6732 | 454 | $135.00
HDST MODULE BASE W/PTT, 15 FT CBL | Headset Base with PTT Switch with 15' cable | RLN6098 | 706 | $227.00
HDST MODULE BASE W/PTT, 25 FT CBL | Headset Base with PTT Switch with 25' cable | RLN6099A | 706 | $261.00
OVER-THE-HEAD, MONAURAL, NOISE-CANCELING HEADSET | Monaural Headset Top with Noise-Cancelling Microphone | RMN5150A | 706 | $161.00
OVER-THE-HEAD, BINAURAL, NOISE-CANCELING HEADSET | Binaural Headset Top with Noise-Cancelling Microphone | RMN5151A | 706 | $168.00

Information Assurance

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
MCD 5000 WINDOWS SUPPLEMENTAL | OS Hardening CD (Full Hardening) for MCD 5000 Deskset System to be ordered with Workstation | FVN5956 | 202 | $50.00
MCAFEE WINDOWS AV CLIENT | This is a standalone installer for Windows operating systems. This should only be ordered for Consoles and MOSCAD products that do not embed the client license. NOTE - MGEGS DO NOT USE MCAFEE SOFTWARE. THEY WILL STAY WITH EXISTING SYMANTEC SOFTWARE IN UNMANAGED MODE. | T7885 | 580 | $182.00

Field Replacement Units

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
FRU: K-STYLE HANDET (INCLUDES COLIED CABLE) FOR MCD 5000 DESKSET | Spare handset for the MCD 5000 Deskset (F2380). | FHN7290 | 202 | $75.00
FRU: CABLE - MCD 5000 DESKSET TO HEADSET JACK BOX | Provides one headset jackbox cable to connect the MCD 5000 Headset Jackbox (FHN7470) to the MCD 5000 Deskset (F2380). Note: The MCD 5000 Headset Jackbox (FHN7470) automatically ships with this cable (FKN8694). | FKN8694 | 202 | $40.00
FRU: CABLE - MCD 5000 DESKSET RGU GROUND CABLE | Spare MCD 5000 RGU ground cable to be used with the MCD 5000 RGU (F7879B). | FKN8704 | 202 | $30.00

#### Upgrade Deployed units to Four Channel Feature

The ability to connect up to and monitor four radios at one time was implemented in R2.4 (Dec 2020). Customers with deployed systems that wish to upgrade to this feature, must purchase the Four Channel License/Software.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
LICENSE,MCD 5000 FOUR CHANNEL SUPPORT W/O OMC | Firmware and Configuration Tool for Four Channel Support - MCD 5000 Deskset System . | HKVN4860 | 202 | $500.00

####

### Ship Card

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
PARTS | VAN | 3004209T01 | CORD, POWER | 785 | 27
PARTS | VAN | 3004209T01 | CORD, POWER | 785 | 27
PARTS | VAN | 3004209T02 | PLUG, BRITISH STANDARD | 785 | 27
PARTS | VAN | 3004209T02 | PLUG, BRITISH STANDARD | 785 | 27
SYSPERIPH | SCB | B1943 | MCD 5000 LICENSING | 202 | 11
PARTS | SSO | BLN6732 | FOOT, SWITCH TRADITIONAL | 454 | 22
PARTS | SSO | BLN6732 | FOOT, SWITCH TRADITIONAL | 454 | 22
PARTS | SSO | BLN6732 | FOOT, SWITCH TRADITIONAL | 454 | 22
QUOTEDS | PCW | DS7Y7Q9U3 | HP Z2 MINI G9 VESA MOUNT | 708 | 4
QUOTEDS | PCW | DSF2B56AA | USB EXTERNAL DVD DRIVE | 708 | 10
QUOTEDS | TIS | DSTG191B | TECH GLOBAL EVOLUTION SERIES 19INCH NON TOUCH | 708 | 80
SYSPERIPH | SCB | F2380 | MCD 5000 DESKSET | 202 | 20
SYSPERIPH | SCB | F2380 | MCD 5000 DESKSET | 202 | 20
FIXEDSTN | SCB | F7879 | SM, RADIO GATEWAY UNIT (RGU) | 202 | 23
SYSPERIPH | SCB | FHN7290 | FRU: K-STYLE HANDET (INCLUDES COLIED CABLE) FOR MCD 5000 DESKSET | 202 | 16
SYSPERIPH | SCB | FHN7394 | MCD 5000 DESKSET WALL MOUNT KIT | 202 | 14
SYSPERIPH | SCB | FHN7469 | MCD 5000 DESKSET / RGU POWER SUPPLY WITH USA POWER CORD | 202 | 16
SYSPERIPH | SCB | FHN7470 | MCD 5000 DESKSET HEADSET JACK BOX & CABLE | 202 | 17
SYSPERIPH | SCB | FHN7485 | FRU: MCD 5000 DESKSET / RGU POWER SUPPLY W/OUT POWER CORD | 202 | 28
SYSPERIPH | SCB | FKN0012 | CABLE RGU TO MOTOTRBO | 202 | 81
SYSPERIPH | SCB | FKN2003 | MCD5000 TO MTM5400 TETRA MOBILE RADIO DIRECT CONNECT | 202 | 15
SYSPERIPH | SCB | FKN2004 | MCD5000 TO MTM800E TETRA MOBILE RADIO DIRECT CONNECT | 202 | 15
SYSPERIPH | SCB | FKN8688 | CABLE - MCD 5000 RGU TO MCS 2000 III DIRECT CONNECT | 202 | 14
SYSPERIPH | SCB | FKN8689 | CABLE - MCD 5000 RGU TO CDM 1550 SERIES DIRECT CONNECT | 147 | 10
SYSPERIPH | SCB | FKN8690 | CABLE - MCD 5000 RGU TO ASTRO CONSOLETTE W9 DIRECT CONNECT | 202 | 20
SYSPERIPH | SCB | FKN8691 | CABLE - MCD 5000 RGU TO MC3000 DJB FOR ASTRO CONSOLETTE W9 | 202 | 113
SYSPERIPH | SCB | FKN8692 | CABLE - MCD 5000 RGU TO MC3000 DJB FOR MCS 2000 III | 202 | 256
SYSPERIPH | SCB | FKN8693 | CABLE - MCD 5000 RGU TO MC3000 DJB FOR CDM 1550 SERIES | 202 | 19
SYSPERIPH | SCB | FKN8694 | FRU: CABLE - MCD 5000 DESKSET TO HEADSET JACK BOX | 202 | 166
SYSPERIPH | CDP | FKN8695 | ETHERNET CABLE 10' WITH RED & BLACK LABELS | 202 | 22
SYSPERIPH | CDP | FKN8695 | ETHERNET CABLE 10' WITH RED & BLACK LABELS | 202 | 22
SYSPERIPH | SCB | FKN8696 | CABLE - MCD 5000 DESKSET TO LOGGER | 202 | 18
SYSPERIPH | CDP | FKN8697 | CABLE - MCD 5000 DESKSET TO VIP (R2.0) | 202 | 6
SYSPERIPH | SCB | FKN8704 | FRU: CABLE - MCD 5000 DESKSET RGU GROUND CABLE | 202 | 166
SYSPERIPH | SCB | FTN7490 | MCD 5000 DESKSET RGU RACK MOUNT PANEL PLUS SCREWS | 112 | 28
SYSPERIPH | SCB | FVN5956 | MCD 5000 WINDOWS SUPPLEMENTAL | 202 | 25
ACCESSORY | CDP | HKVN4858 | LICENSE,MCD 5000 NATIVE LANGUAGE SUPPORT | 202 | 45
ACCESSORY | CDP | HKVN4860 | LICENSE,MCD 5000 FOUR CHANNEL SUPPORT W/O OMC | 202 | 45
ACCESSORY | CDP | HKVN4861 | LICENSE,MCD 5000 DESKSET SYSTEM CONFIG TOOL - SYSTEM W/OUT OMC | 202 | 45
ACCESSORY | CDP | HKVN4865 | LICENSE,CD, MCD 5000 DOCUMENTATION | 202 | 45
PARTS | CDP | RLN6098 | HDST MODULE BASE W/PTT, 15 FT CBL | 706 | 6
PARTS | CDP | RLN6098 | HDST MODULE BASE W/PTT, 15 FT CBL | 706 | 6
PARTS | CDP | RLN6099A | HDST MODULE BASE W/PTT, 25 FT CBL | 706 | 2
PARTS | CDP | RLN6099A | HDST MODULE BASE W/PTT, 25 FT CBL | 706 | 2
PARTS | CDP | RMN5068A | DESKTOP MIC | 706 | 3
FIXEDSTN | CDP | RMN5077B | SUPRAPLUS SINGLE MUFF HEADSET | 706 | 5
FIXEDSTN | CDP | RMN5078B | SUPRAPLUS NC SINGLE MUFF HEADSET | 706 | 8
FIXEDSTN | CDP | RMN5079B | SUPRAPLUS DUAL MUFF HEADSET | 706 | 6
FIXEDSTN | CDP | RMN5080B | SUPRAPLUS NC DUAL MUFF HEADSET | 706 | 2
ACCESSORY | CDP | RMN5150A | OVER-THE-HEAD, MONAURAL, NOISE-CANCELING HEADSET | 706 | 6
ACCESSORY | CDP | RMN5151A | OVER-THE-HEAD, BINAURAL, NOISE-CANCELING HEADSET | 706 | 5
CNTLR | SCB | T7885 | MCAFEE WINDOWS AV CLIENT | 580 | 17