Back

##### Vendetta

###### Product Catalog

##### Jump to ...

- Model
- Ordering Information
- Configuration
- Software & Services

Back

##### Vendetta

### Model

NEN 2500 - VENDETTA

### Ordering Information

#### General Information

YOUR MISSION KNOWS NO BOUNDARIES, YOUR EQUIPMENT SHOULD NOT EITHER

The NEN 2500 - VENDETTA SDR is a highly capable, secure Software Defined Radio (SDR) with built-in power amplifiers, receiver circuitry, and an integrated front end. It is a rapidly deployable dual carrier Base-Transceiver-Station (BTS) which provides the technical agility to process a variety of radio technologies from GSM to LTE with a single, compact piece of hardware.

Purpose-built solution. With its rugged chassis and IP67 certification, the NEN 2500 - VENDETTA SDR sets a new standard in SWaP without compromising performance. NEN 2500 - VENDETTA is ideal for maritime use.

Portable and compact solution. Weighing in at 16.4 lbs without fans and 19.8 lbs with fans, the NEN 2500 - VENDETTA SDR is light anough to be transported and rapidly-deployed at the targeted environment. The NEN 2500 - VENDETTA SDR ideally suited for manned aerial vehicle, marine vehicle, vehicular, and man-portable missions.

#### Features

- Gigabit Ethernet and Wi-Fi for command and control
- Status LEDs
  - Power
  - Ethernet Link
  - Health
  - TX on/off
- RX Antenna (survey/High-Band/Low-Band)
- TX Antenna (survey/High-Band/Low-Band)
- Four port auxiliary RF (generic RX/TX)
- DC Power (+9 to +36 VDC) with remote on/off
- Single Cell Power Consumption 170W (typical)
- Dual Cell Power Consumption <300W (typical), 350W (max)
- eSATA port
- Supported Bands
  - Tunable from 730 MHz thru 2 GHz (amplified); 70 MHz thru 6 GHz (unamplified)
  - 56 MHz instantaneous bandwidth per transceiver
- Freescale i.MX6 Quad-Core processor @1.0 GHz/core
- Xilinx Virtex-7 VX485T-2
- Size (with fans): 18.1”x 10.1”x 2.7” Weight: 19.8lbs
- Size (without fans): 14.9”x 10.1”x 2.7” Weight: 16.4lbs

SUPPORTED APPLICATIONS

- TACTICAL LTE Network
- RDBS

CUSTOM APPLICATIONS AVAILABLE upon request

TARGET ENVIRONMENTS

- MANNED AERIAL VEHICLE
- VEHICULAR
- MARINE VEHICULE
- MAN PORTABLE
- FIXED SITE

#### Ordering Requirements

For ordering information please send an email to: BuyAT@MotorolaSolutions.com.

### Configuration

#### Main Models

Description | Nomenclature | Price
--- | --- | ---
VENDETTA Kit | FDKT00225 | $104,850
VENDETTA TACTICAL LTE Kit | FDKT00262 | $128,000
VENDETTA RDBS Kit | FDKT00230 | $113,300

The NEN 2500 - VENDETTA unit consists of an advanced, state-of-the-art, small-form-factor Software Defined Radio, utilizing modern embedded microprocessor and FPGA technology suitable to handle complex radio applications in the 70-3000 MHz spectrum. Each NEN 2500 - VENDETTA kit provides the user with the following:

(1) NEN 2500 - VENDETTA SDR unit

(1) +9 to +36 VDC power brick with customer power cable

(1) eSATA cable

(1) Custom IP67 10/100/1000 Ethernet cable (RJ45)

(1) GPS Magnetic Mount Antenna

(1) Wi-Fi Magnetic Mount Antenna

Additional components in the NEN 2500 - VENDETTA SDR

(1) Custom Auxiliary RF cable for use with (4) auxiliary RF ports(generic RX/TX)

Additional components in the NEN 2500 - VENDETTA TACTICAL LTE & RDBS

(1) RF to SMA Cable

(3) Wide Band Antennas, 698-2500MHz (survey/RX/TX)

(2) 10' Megaphase RF Cable

(2) 20' Megaphase RF Cable

(4) Adapter, SMA to N Plug

(4) Adapter, SMA to N Jack

(1) Laptop

One (1) CD containing the TACTICAL LTE software or RDBS software

NEN 2500 - VENDETTA TACTICAL LTE Product description: The TACTICAL LTE solution allows for operational use of commercial, cellular,comms protocols by providing a tactical-edge, self-contained,

private, LTE Network with an integrated eNodeB and EPC.

### Software & Services

#### Warranty

LIMITED WARRANTY

Motorola warrants the Product against significant defects in material and workmanship under normal use and service for a period of sixty (60) calendar days from the date of shipment from Motorola. Motorola, at its option, will at no charge, either repair the Product (with new or reconditioned parts), replace it with the same or equivalent Product (using new or reconditioned Product), or refund the purchase price of the Product for significant defects identified during the warranty period provided Motorola is notified of such significant defects no later than 14 calendar days after the expiration of the warranty period according to the terms of this warranty. Repaired or replaced Product is warranted for the balance of the original applicable warranty period. All replaced parts of the Product shall become the property of Motorola.

This warranty sets forth the full extent of Motorola’s responsibilities regarding the Product. Repair, replacement or refund of the purchase price, at Motorola’s option, is the exclusive remedy. THIS WARRANTY IS GIVEN IN LIEU OF ALL OTHER EXPRESS WARRANTIES. MOTOROLA DISCLAIMS ALL OTHER WARRANTIES OR CONDITIONS, EXPRESS OR IMPLIED, INCLUDING THE IMPLIED WARRANTIES OR CONDITIONS OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT SHALL MOTOROLA BE LIABLE FOR DAMAGES IN EXCESS OF THE PURCHASE PRICE OF THE PRODUCT, FOR ANY LOSS OF USE, LOSS OF TIME, INCONVENIENCE, COMMERCIAL LOSS, LOST PROFITS OR LOST SAVINGS OR OTHER INCIDENTAL, SPECIAL, INDIRECT OR CONSEQUENTIAL DAMAGES ARISING OUT OF THE USE OR INABILITY TO USE SUCH PRODUCT, TO THE FULL EXTENT SUCH MAY BE DISCLAIMED BY LAW.