Back

##### APX 8500 Mobile Radio

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Ship Card

Back

##### APX 8500 Mobile Radio

### Model

·

·

·

·

·

·

·

·

ASTRO® Digital APX 8500 Mobile Subscriber
700/800 MHz (1 – 35 Watts)
VHF - 136 -174 (1-50, Watts)
UHF R1 R2- 380-520 (1-45 Watts)

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

Effective July 7, 2025: The CN model of the APX 8500 is available. The CN brings the introduction of 5GHz WiFi and the broadband protection feature for the 7/800MHz band. Along with the introduction of the CN version of the APX 8500 mobile, the intent to cancel for the AN model will be last orders of September 30, 2025 and last ship date of December 31, 2025. Aftermarket support of the AN models will follow the timing of the CN as AN radios will continue to be serviced with CN parts.

Beginning September 2023 APX radios can be ordered with the New Feature/Latest release or the Baseline release firmware. The Baseline release is defined as a single major software release (i.e. 202X.1) to ship from the factory for a 1 year duration. The first major release each year will be the Baseline Release. A New Feature Release is defined as the second and third major releases each year (202X.2 and 202X.3) and is required for customers to access new feature content and/or products. New Feature releases contain the current year’s Baseline content as well as content from the previous New Feature release.

IMPORTANT! Radios that are ordered via COF must add the Baseline Release option (QA09113) if the Baseline firmware is desired. If the Baseline option (QA09113) is not added to COF orders, radios will ship with the Latest Release and cannot be rolled back to the Baseline Release. Most quotes and orders should keep the default Baseline Firmware (QA09113) unless a customer desires new functionality only provided in a New Feature release. More information about the Baseline and New Feature Release strategy can be found in MTN-0111-23-NA.

Effective October 11th, 2021: APX Mobile One Touch Feature will be enhanced and integrated with DEK’s Status Message functionalities. Users will benefit from the ability to program and assign alias Status Messages on the APX Control Head display. One Touch Feature G683 pricing will increase from $75 to $125. The APX 8500 model comes with OneTouch by default.

Effective October 11th, 2021: A new Ethernet faceplate with RJ45 connector will be available on APX 8500 MP. Users will be able to connect the Sierra Wireless MG90 router directly to the APX 8500 MP using an RJ45 Ethernet cable. The Ethernet Faceplate is an orderable option and available at $250. All APX 8500 MP Mobile orders booked after October 11th, 2021 will continue to ship with the current Standard Faceplate at $0 cost unless the ADD Ethernet Faceplate option (GA01787) is selected. Aftermarket Retrofit Kit upgrades will also be supported (HN001998A01). The Ethernet Faceplate only supports APX 8500 MP connected to a Sierra Wireless MG90 router.

Effective August 1st 2021: E5 control head pricing will increase from $572 to $652.

Effective July 19th 2021 All APX Mobile Orders Booked After July 19th 2021: The APX Mobile Bluetooth feature will be available on APX 8500 and Enhanced “BN” APX Mobiles. The E5 Control Head will support COTS Bluetooth and MPP Bluetooth Pairing. The O7, O3 & O2 Control Heads will support COTS Bluetooth ONLY. Bluetooth will be included on all APX Mobile orders and will be reflected in the Flashcode unless DELETE Bluetooth option (QA05336) is used to remove it. A Wifi/Bluetooth antenna will be required to enable the Bluetooth functionality. Flashport upgrades will also be supported. Bluetooth is not supported on the APX Consolette and APX Dual Radio.

Effective October 5th, 2020: All U.S. orders will require an encryption selection. QA05751 “Clear Radio No ADP” has become an orderable option with a $0 dollar cost. G193/Q667 ADP only is also available at $0. Please see encryption section for AES and other encryption options that come with ADP. Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.

Effective Effective August 1, 2020: The O5 control head (option G442 and kit H1904) has been canceled and replaced by the E5 GA01670 and H1930

Effective August 26, 2019: Multi-System OTAR (GA01620) is available. Users who frequently move from one secure system to another will benefit from the ease and speed that radio keys are shared and updated. Our Multi-System Over-the-Air Rekeying (Multi-System OTAR) feature supports over-the-air-rekeying with up to 19 different secure systems, key sharing across profiles and seamless migration of fielded radios. The customer must order OTAR W/ MULTIKEY as a prerequisite for MS-OTAR.

APX 8500 HP/MP ORDERS WITH DVRS MSU ACTIVATION (GA00631)

When GA00631 MSU is selected the all band antenna GA01513 must be purchased separately as AN000131A02.

GA00631 MSU and QA00631 PSU are mutually exclusive and will require depot to change from one to the other.

Please be aware that depending upon the equipment installation and frequency usage, additional equipment may be required to assure optimal performance between the APX™8500 and DVR/VRX1000. More specifically, when using an APX™8500 with an antenna (all band or with a triplexer) that includes the same frequency range as the DVRS / VXR1000, this additional equipment will help to assure the desired performance between these two products. This applies to all sales that combine an APX™8500 with a DVR/VRX1000 as well as any replacements of an existing MSU (Mobile Subscriber Unit) with the APX™8500 where the DVR/VRX1000 may already be deployed.

Please contact sales@futurecom.com for more information. To assist Futurecom sales with assessing a particular configuration, the following information will be needed:

1. MSU band(s) and frequencies if known
2. DVR/VRX1000 frequencies
3. Which MSU band(s) will the DVR/VRX1000 be used with?
4. MSU Antenna type (single band vs all band)?

Supplemental form: http://www.futurecom.com/upl/downloads/catalog/products/supplemental-ordering-form-51a33dfb.pdf

NOTE: Please note the items below has a 2-4 weeks lead time for quantity of 1-10 units. For larger quantities, the lead time is longer.

- H1919A: Single Triplexer Kit:
- DDN2657A: Dual Triplexer Kit:
- DDN2808A: Single Triplexer Kit:
- DDN2658A: Single Triplexer Relay Kit (w/relay):
- DDN2659A: Dual Triplexer Relay Kit:

### Ordering Information

#### Please Read All Option Descriptions Before Making Your Selection

Required Selection:

1) Main Model

2) Mounting (Not required for APX 8500 HP, which is only available in remote mount)

3) Control Head Selection

4) RF Antenna

5) Operation Mode

6) Feature Antenna(s)

7) Encryption

8) Remote Mount Cables (if remote mount is selected)

9) Microphone

10) Speaker

11) Service

#### Additional Ordering Information for Service Options

SmartConnect End to End Ordering Guide

### Configuration (NOTE: Base price does not include antennas (Rf and GPS), speaker or mount type selections – must be picked from below)

1: Base Radio $11,124.42 List $6,118.43 Disc $4,868.43 w/Trade

Description | Full Description | Nomenclature | APC | Price
APX8500 ALL BAND MP MOBILE | - | M37TSS9PW1CN | 681 | inc.
ADD: APX CONTROL HEAD SOFTWARE |  | G444 | 656 | inc.
ADD: ASTRO DIGITAL CAI OPERATION |  | G806 | 656 | inc.
ENH: SMARTZONE OPERATION APX6500 |  | G51 | 527 | inc.
ENH: P25 TRUNKING SOFTWARE APX |  | G361 | 656 | inc.
ADD: ENHANCED DATA APX |  | QA03399 | 656 | inc.
ADD: GROUP SERVICES |  | GA09008 | 656 | inc.
ENH: OVER THE AIR PROVISIONING |  | G996 | 656 | inc.
ENH: ENH: RADIO TRACE |  | G170 | 656 | inc.
ADD: TDMA OPERATION APX |  | GA00580 | 656 | inc.
ENH: TRUNKED ONE TOUCH |  | G683 |  | inc.
ADD: HW KEY SUPPLEMENTAL DATA |  | QA01648AA | 0655 | inc.
ADD: APX E5 CONTROL HEAD |  | GA01670 |  | inc.
ADD: KEYPAD MIC GCAI |  | W20 |  | inc.
ADD: SMARTCONNECT |  | GA01630 | 681 | inc.

####

#### Power Alternative (optional)

Description | Full Description | Nomenclature | APC | Price
REM: APX8500 ALL BAND MP MOBILE | - | M37TSS9PW1CN | 681 | ($6,558.00)
ALT: APX8500 ALL BAND HP MOBILE | - | M37TXS9PW1CN | 681 | $7,728.00

#### Delete Frequency Bands (Optional. Can select a Maximum of Two)

Special Note for United States - State & Local Markets: In accordance with FCC mandate, the U1/U2 Mid Power and U1/7-800 band combinations for this product are restricted to not allow programming for 25 KHz operation. These frequencies are restricted to 12.5 KHz operation only.

Description | Full Description | Nomenclature | APC | Price
DEL: DELETE UHF BAND | Deletes both UHF R1 and UHF R2 frequency bands. | GA05509 | 681 | ($800.00)
DEL: DELETE VHF BAND | - | GA05508 | 681 | ($800.00)

#### 2. Mounting (Must Select Either Dash or Remote Mount for APX 8500 MP)

If a remote mount cable other than 5 meters (17ft) is desired for Remote Mount, please reference the "Remote Mount Cables" section.

The O3 dash and remote mount configurations are the same except that the dash mount configurations do not come with the 17ft extension cable, PMLN4958.

Description | Full Description | Nomenclature | APC | Price
ADD: DASH MOUNT | Not available on APX 8500 HP. Required for Control Station Operation. An O3 Control Head ordered with a Dash Mount Configuration is the same as the O3 Remote Mount configuration, but it does not come with the 17ft extension cable, PMLN4958A. | G66 | 656 | $148.00
ADD: REMOTE MOUNT MID POWER | Not required for selection on APX 8500 HP. G138 is required for Motorcycle Configuration. Motorcycle Remote Mount Option is $440 DUP. | G67 | 656 | $350.00

#### Motorcycle Mounting (Optional)

HMN1079 (Motorcycle Mic) and HSN4031 (Speaker) are mandatory selections with motorcycle configurations. Motorcycle mount requires the O2, E5, or O7 Control Head and Remote Mount (G67). CAN cables are not compatible with motorcycle. This option includes a weatherized harness. Incompatible with DVRS MSU operation (GA00631)

Description | Full Description | Nomenclature | APC | Price
ADD: APX MOTORCYCLE CH SFWR | Requires G67 (Remote Mount) | G138 | 656 | $0.00

#### Control Station Operation (Optional)

Mid Power Model Only

O2, E5 & O7 Control Heads Only. Must select one.

Requires Dash Mount (G66)

Some microphones are not compatible with Control Station Operation. Please read descriptions carefully.

Although the Power Supply is optional, it is needed for a full Control Station solution. The APX 8500 requires a higher capcity power supply KT000254A02.

Description | Full Description | Nomenclature | APC | Price
ADD: CONTROL STATION OPERATION | O3 not supported Requires Dash Mount (G66) HLN6042B | W665 | 656 | $82.00
ADD: CONTROL STATION POWER SUPPLY | Although the Power Supply is optional, it is needed for a full Control Station solution. The APX 8500 requires a higher capacity power supply KT000254A02. | G91 | 656 | $317.00

#### 3B Control Head Options (Select if included E5 head is not desired)

Description | Full Description | Nomenclature | APC | Price
REMOVE 05 HEAD |  |  |  | $(767.00)

####

O2 Control Head Options

Description | Full Description | Nomenclature | APC | Price
ADD: APX O2 CH (GREY) | - | GA00804 | 656 | $579.00
ADD:IMPACT GREEN COLOR HOUSING (O2) | When ordered in conjunction with GA00804 you will get a green colored O2 housing. | G201 | 656 | $30.00
ADD: SCHOOL SERCURITY ENHANCEMENT PACKAGE | Education O2 Emergency Push Button | GA01056 | 514 | $55.00

O3 Control Head Options

Description | Full Description | Nomenclature | APC | Price
ADD: APX O3 HANDHELD CH | Requires No Microphone (G90). If Lights & Siren Keypad and Software is required, order GA00806. | G72 | 656 | $1,114.00
ADD:CH SIREN & LIGHTS KEYPAD | Available on O3 (G72) and O7 (GA00805) Control Heads. | GA00806 | 656 | $59.00

E5 Control Head Option

Description | Full Description | Nomenclature | APC | Price
ADD: APX E5 CONTROL HEAD | - | GA01670 | 681 | $767.00

O7 Control Head Options

Description | Full Description | Nomenclature | APC | Price
ADD: APX O7 CONTROL HEAD. | If Lights & Siren Keypad and Software is required, order GA00806. | GA00805 | 656 | $744.00
ADD:CH SIREN & LIGHTS KEYPAD | Available on O3 (G72) and O7 (GA00805) Control Heads. | GA00806 | 656 | $59.00

No Control Head Options

Description | Full Description | Nomenclature | APC | Price
ADD: NO O3 CONTROL HEAD | If you plan to use this model with an O3 Control Head but already have a control head and don't require it, select GA00001. Requires remote mount (G67). | GA00001 | 656 | $0.00
ADD: APX MOBILE NO CONTROL HEAD | If you plan to use this model with an O2, E5, O5, O7 Control Head but already have a control head and don't require it, select G88. Requires remote mounting option (G67 or W665). | G88 | 681 | $0.00

#### Multi-Control Head Options

The APX 8500 mobile can support up to four control heads on a single transceiver. This allows control of a single APX 8500 transceiver from two different control head locations.

Multi-Control Head options require Remote Mount.

When ordering a multi-control head option, only one type of control head can be selected.

Only available with O2, E5, O7 Control Heads.

Multi-control head options require an equal number of microphones, speakers, and CAN cables.

Multi-control head options are incompatible with the multi-radio options.

Please note: Audio Pod was discontinued in 2022 and the ability to perform speaker toggling between dual control heads is no longer an available option.

Description | Full Description | Nomenclature | APC | Price
ADD: APX DUAL-CONTRL HD HARDWARE | Requires either O2, E5, O7 Control Head. Requires a remote mount configuration. Requires a selection of 2 for microphones, speakers and CAN cables. | GA00092 | 656 | $627.00
ADD: APX QUAD-CONTROL HARDWARE | Requires either O2, E5, O7 Control Head. Requires a remote mount configuration. Requires a selection of 3 for microphones, speakers and CAN cables. | GA00094 | 656 | $1,430.00
ADD: APX TRI-CONTROL HARDWARE | Requires either O2, E5, O7 Control Head. Requires a remote mount configuration. Requires a selection of 3 for microphones, speakers and CAN cables. | GA00093 | 656 | $1,000.00

#### 4. RF Antenna (Required)

The APX 8500 has one QMA style LMR antenna port. Any additional connections will require vehicle multiplexer EQ000103A02 that allows up to 3 QMA antenna connections. We will offer this multiplexer and Adapters through our Parts Division.

Examples are Mini U to QMA CB000091A03, QMA to QMA CB000091A02 and SMA to QMA CB000091A04. Aftermarket Antennas are certified for use on the APX 8500 but do require CB000091A02.

Description | Full Description | Nomenclature | APC | Price
MULTIPLEXER QMA | Order on a separate line. Provides for EQ000103A02 that allows up to 3 QMA antenna connections. | H1919 | 681 | $294.00

#### Must Select One of the Following:

Description | Full Description | Nomenclature | APC | Price
ADD: NO RF ANTENNA NEEDED | - | G89 | 656 | $0.00

All-Band Antenna

Description | Full Description | Nomenclature | APC | Price
ADD: ALL BAND MOBILE ANTENNA (7/8/V/U) | Corresponding kit: AN000131A02. Must be ordered seperately if MSU GA00631 is ordered. Mutilplexer sold seperately as H1919 | GA01513 | 681 | $112.00

#### Motorcycle Antenna Choices

Motorcycle radio orders require an antenna selection for each enabled band (UHF R1 and R2 are considered one band) and comes with multiplexer EQ000103A01.

7/800

Description | Full Description | Nomenclature | APC | Price
ADD: ANT 3DB LOWPRO MCYC 762-870 | Corresponding kit number: AN000197A11 | G174 | 681 | $50.00
ADD: ANT 3DB MCYCLE 762-870MHZ | Corresponding kit number: AN000197A10 | G335 | 681 | $16.00
ADD: NO RF ANTENNA NEEDED | - | G89 | 656 | $0.00

VHF

Description | Full Description | Nomenclature | APC | Price
ADD: ANT MTCL 1/4 WAVE WHIP 136-144 | Corresponding kit number: AN000197A01 + AN000208A01 | GA00510 | 681 | $59.00
ADD: ANT MTCL 1/4 WAVE WHIP 144-150.8 | Corresponding kit number: AN000197A02 + AN000208A01 | GA00511 | 681 | $59.00
ADD: ANT MTCL 1/4 WAVE WHIP 150.8-162 | Corresponding kit number: AN000197A03 + AN000208A01 | GA00512 | 681 | $59.00
ADD: ANT MTCL 1/4 WAVE WHIP 162-174 | Corresponding kit number: AN000197A04 + AN000208A01 | GA00513 | 681 | $59.00

UHF Antennas

Description | Full Description | Nomenclature | APC | Price
ADD: ANT MTCL 1/4 WAVE 380-433MHZ | Corresponding kit number: AN000197A05 + AN000208A03 | G210 | 681 | $34.00
ADD: ANT MTCL 1/4 WAVE WHIP 425-470 | Corresponding kit number: AN000197A06 + AN000208A01 | GA00506 | 681 | $59.00
ADD: ANT MTCL 1/4 WAVE WHIP 450-482 | Corresponding kit number: AN000197A07 + AN000208A01 | GA00507 | 681 | $59.00
ADD: ANT MTCL 1/4 WAVE WHIP 482-512 | Corresponding kit number: AN000197A08 + AN000208A01 | GA00508 | 681 | $59.00
ADD: ANT MTCL LO PRO UNITY 450-512 | Corresponding kit number: AN000197A09 + AN000208A03 | GA00509 | 681 | $59.00

#### Dual Radio Operation Options

The APX Dual Radio Feature offers the capability to control TWO (2) APX8500, APX7500, APX6500, or APX6500Li mobile radios from ONE (1) O7 or E5 control head. APX Dual Radio allows for mixing and matching of radios across tiers (i.e. APX 8500 with APX 6500) and power levels (High Power with Mid Power).

Each radio in an APX Dual Radio system must be ordered independently.

The mobiles in a dual radio solution can be single or dual band. Both radios can be on the same or different frequency bands.

One radio must be ordered with the Primary Radio option (GA01113) and the other with the Secondary Radio option (GA01117). This will include both the SW and HW required for dual radio operation.

Although each radio must be ordered as either a Primary or Secondary radio, each radio can be configured to work as a Primary, Secondary, or a Standalone radio.

Only one speaker can be connected to the control head and it will play audio from the primary radio. A 30 ft. speaker extension cable is included on the secondary radio to connect the second speaker directly to the secondary radio. If a longer cable is needed, a 131 ft. version can be purchased from AAD (part # HKN6251)

The Dual Radio feature is incompatible with the multi-control head options.

Description | Full Description | Nomenclature | APC | Price
ENH: DUAL RADIO OPERATION (PRIMARY RADIO) | The Primary radio must be ordered with an O7 CH, or E5 CH. APX Dual Radio is not compatible with any other control head. The primary radio includes a short dual radio CAN cable (HKN6245) to connect both radios together. If the stack mount trunnion is ordered, a right-angle version of this cable (HKN6249) will ship instead to facilitate stack-mounted installations. If a different length is desired, the standard remote mount control head cables can also be used to connect both together. | GA01113 | 656 | $715.00
ENH: DUAL RADIO OPERATION (SECONDARY RADIO) | The secondary radio must be ordered with no control head (G88). | GA01117 | 656 | $715.00

#### Dual Radio Options

The Dual Radio trunnion is new to accommodate the smaller form factor of the Enhanced APX 6500. HLN7045A, offered on APX 6500 AN models, is not compatible with the Enhanced APX 6500. HLN7045B is compatible will all Enhanced APX 6500 and APX 8500 models.

Description | Full Description | Nomenclature | APC | Price
ADD: DUAL RADIO STACKABLE MP TRUNNION KIT | Corresponding kit: HLN7045B | GA01115 | 527 | $350.00

#### System Enhancement Options (Optional)

The APX 8500 comes standard with G170 Radio Trace and G683 Trunked One Touch

The following options are optional and will provide additional capabilities, if required.

Description | Full Description | Nomenclature | APC | Price
ADD: DVRS MSU ACTIVATION | Allows mobile to host A DVR, Requires Remote mount G67. Additional hardware may be needed to operate properly with a DVR Requires depot to change a mobile from a MSU to PSU. Compatible with GA09011 Data Modem Tethering. Require GA01779 (aftermarket cable KT000247A04) when both GA09011 and GA00631 are ordered. | GA00631 | 656 | $294.00
ADD: APX MOBILE RADIO AUTHENTICAT | Requires P25 9600 Trunking (G361). | GA01767 | 527 | $110.00
ADD: WI-FI CAPABILITY | Compatible with Enhanced (BN) models only. Requires a Wi-Fi antenna. Supports codeplug updates, firmware refreshes, and FLASHport upgrades over pre-provisioned wireless networks. Requires Radio Management SW (ordered separately). Must order Out of the Box Wi-Fi Provisioning option (GA09007) if provisioning the radios out of the box using Wi-Fi is desired. | GA09001 | 681 | $353.00
ADD: OUT OF THE BOX WI-FI PROVISIONING | Requires GA09001 (Wi-Fi) | GA09007 | 681 | $0.00

#### 6. Feature Antennas

When WiFi GA09001 is selected you must order either a Multi-function (GPS/WIFI/ BT) or individual single function GPS , Wi-Fi/BT antennas.

(Bluetooth requires a WiFi antenna to function).

Multifunction Antennas (Must Select One if Multifunction is Selected)

Requires Wi-Fi (GA09001)

Description | Full Description | Nomenclature | APC | Price
ADD: WIFI/GNSS FLEXIBLE CABLE LMR195 | Corresponding kit: AN000163A01. AN000163A05 has flexible BT/WiFi cable (PFP-195) but has 1-1.5 dB lower gain compared to AN000163A01 that has stiffer PFP-240 cable. | GA00250 | 681 | $110.00
ADD: WIFI/GNSS FLEXIBLE CABLE LMR195 | Corresponding kit: AN000163A02 Requires Motorcycle (G138) | GA00250 | 681 | $118.00
ADD: GNSS/BT-WIFI THRU MNT ANT, 17FT FLEXIBLE PFP-100A/195, QMA | Corresponding kit: AN000163A05. AN000163A01 has stiffer BT/Wi-Fi cable (PFP-240) but it has 1-1.5 dB better gain compared to AN000163A05 that has flexible PFP-195 cable. | GA00250AC | 681 | $130.00

GPS Antennas (Must select one if single function GPS is required)

Description | Full Description | Nomenclature | APC | Price
ADD: COVERT GNSS GLASSMOUNT LMR100 | Corresponding kit: PMAN4109 | GA01580AA | 681 | $82.00
ADD: GPS/GNSS MAG MOUNT ANTENNA | Corresponding kits: CB000091A04, & PMAN4010 | GA01305 | 656 | $71.00
ADD: GPS ANTENNA | Requires GA01576. Corresponding kit: HAG4000 | GA00226 | 656 | $89.00
ADD: GPS ANTENNA MTCL | Corresponding kit: HAG4001. Requires Motorcycle (G138). | GA00269 | 656 | $89.00

GPS Antenna Adaptor

Description | Full Description | Nomenclature | APC | Price
ADD: SMA TO QMA ADAPTER | Requires GA01305, or GA00226. Corresponding kit: CB000091A04. Corresponding kit: CB000091A04 | GA01576 | 986 | $22.00

Wi-Fi/BT Antennas (Must select one if single function Wi-Fi/BT is requested)

Description | Full Description | Nomenclature | APC | Price
ADD: COVERT WIFI GLASSMOUNT 2.4/5 GHZ | Corresponding kit: PMAN5101 Requires Wi-Fi (GA09001). | GA01579AB | 681 | $77.00

#### 7. Encryption Algorithms (Must Select One)

All APX Radios require an encryption selection. QA05751 ADD: “Clear Radio No ADP” is now a $0 choice. ADD: “ADP Only” G193/Q667 is still a $0 option. (AES 256 is the only approved encryption algorithm by P25 CAP and SAFECOM)

Description | Full Description | Nomenclature | APC | Price
ADD: AES ENCRYPTION APX AND ADP | Requires digital operation. P25 CAP Compliant option. Includes ADP. | G843 | 656 | $560.00
ADD: ADP ONLY (NON-P25 CAP COMPLIANT) (US ONLY) | Provides for ADP ONLY, a Non-P25 CAP Compliant, non-FIPS compliant option. If another encryption is required, please order that option which will internally generate ADP. | G193 | 430 | $0.00

#### Multikey (Optional)

All multikey options require an encryption algorithm selection.

Description | Full Description | Nomenclature | APC | Price
ADD: MULTIPLE KEY ENCRYPTION OPERATION | Required when using more than one encryption algorithm or encryption key. | W969 | 656 | $363.00
ENH: ASTRO 25 OTAR W/ MULTIKEY | Not compatible with ADP-Only. Includes multikey, trunking OTAR, and Tactical OTAR. Tactical OTAR can only be utilized when IV&D is purchased. Requires AES. | G298 | 656 | $814.00
ADD: MULTI SYSTEM OTAR | Requires ASTRO 25 OTAR W/ MULTIKEY (G298) | GA01620 | 656 | $177.00

#### 8. Remote Mount Cables (17 FT STD)

Description | Full Description | Nomenclature | APC | Price
ADD:CBL REMOTE MOUNT 10 FEET | Corresponding kit: HKN6170 | G618 | 656 | $12.00
ADD: REMOTE MOUNT CBL 17 FEET | Included at no charge with Single Control Head Remote Mount installations and High Power. Corresponding kit: HKN6169 | G628 | 656 | $18.00
ADD: REMOTE MOUNT CBL 30 FEET | Corresponding kit: HKN6168 | G610 | 656 | $30.00
ADD: REMOTE MOUNT CBL 50 FEET | Corresponding kit: HKN6167 | G609 | 656 | $42.00
ADD:CBL REMOTE MOUNT 75 FEET | Corresponding kit: HKN6166A | G607 | 656 | $54.00
ADD:REMOTE MOUNT CBL 115 FEET | Corresponding kit: HKN6165 | G879 | 656 | $65.00
ADD: REMOTE MOUNT CABLE 128 FT | ***For Dual/Tri/Quad configurations, the total cable length may not be greater that 131 ft (40 meters). Therefore, this cable should not be used with a dual, tri, or quad control radio*** Corresponding kit: HKN6164 | G582 | 656 | $77.00

#### Data/Programming Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: USB DATA INTFC CABLE-DASH | 6 FT USB W/IGNITION SENSE Corresponding kit: HKN6163B. Can be used to program APX Mobile Radios. | G308 | 656 | $59.00
ADD:USB DATA INTFC CABLE-TRK | 16.5 FT USB W/IGNITION SENSE Corresponding kit: HKN6172B. Can be used to program APX Mobile Radios. | G309 | 656 | $59.00

#### J600 Adapter (Optional)

The APX 8500's new one-sided design removed the J600 port used for DVR and Motorola Siren (SLIM does not require this). Required for remote mount and DVRS support.

Description | Full Description | Nomenclature | APC | Price
ADD: J600 ADAPTER CABLE | Accessory Kit: KT000247A01 | GA01515 | 681 | $112.00
DEL: NO J600 ADAPTER CABLE NEEDED | - | GA01517 | 681 | $0.00

#### Cable Accessories (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: EXTERNAL ALARM RELAY AND CABLE | For either HORN or LIGHTS. NOT both | W116 | 656 | $89.00
ADD: CABLE URC TO TRANSCEIVER | Connects Universal Relay Controller to APX Transciver via a RJ45 and CGAI connection. | GA00260 | 656 | $18.00
ADD:REMOTE MOUNT VIP CBL APX | Park/Kill, Gunlock, 'Horn Ring/Horn Transfer' or Horn/Lights Park/Kill and Horn 'Ring/Horn Transfer' only available with Motorola Siren. Gunlock supported on O9 Control Head Only. CORRESPONDING KIT: (HKN6196B) | G322 | 656 | $42.00
ADD: UNIVERSAL RELAY CONTROLLER | Required to Control Vehicle Lights with the O3, 07 and O9 Control Heads.Requires URC Cable GA00260. | GA00259 | 656 | $294.00
ADD: GCAI EXTENSION CABLE 2 FT | For use with 07, O9 Control Heads and GCAI style Mic. KIT #PMKN4093A. | GA00589 | 656 | $35.00
ADD: KEY LOCK MOUNT APX | Remote Mount Mid Power Only. | W81 | 471 | $39.00

#### 8: Microphones (optional – standard includes keypad mic)

Description | Full Description | Nomenclature | APC | Price
REMOVE STD KEYPAD MIC PRICING IN BASE RADIO | IF SELECTING FROM BELOW |  |  | $(212.00)
ENH: HAND MIC,GCAI WATER RESISTANT | Not compatible with control station operation. Corresponding kit HMN1089A | G892 | 656 | $85.00
ADD: MODEL III GCAI KEYPAD HANDSET | Not compatible with Control Station. Corresponding kit: HMN4097A | GA00221 | 656 | $348.00
ADD:GATEWAY RSM AND WIRELESS RSM WITH VEHICLE CHARGER | Includes 12V Vehicle Charger Corresponding kit: RLN6551 | GA01354AA | 656 | $589.00
ADD:GATEWAY RSM AND WIRELESS RSM | Corresponding kit: RLN6552 | GA01439 | 656 | $461.00
ADD: CONTROL STATION DESK GCAI MIC | Not compatible with Remote Mount. Requires Control Station, DEK, and Dash Mount. Corresponding Kit: RMN5070 | W382 | 656 | $199.00
ADD:GATEWAY RSM | Corresponding kit: PMMN4097 | GA01438 | 656 | $148.00
ADD: HANDSET/HANGUP MIC ARMORED CABLE | Armored Cable, No Toggle Switch Accessory Kit: HKN1018 | W874 | 656 | $300.00
ADD: STD PALM MICROPHONE APX | Corresponding kit: HMN1090 | W22 | 471 | $85.00
ADD:HANDSET/HANGUP MIC | Not compatible with Control Station. Coiled Cable with Toggle Switch Accessory Kit: HLN1457A | G874 | 656 | $285.00
ADD: VISOR MIC REMOTE MOUNT | Requires PTT Option. Incompatible with Control Station. Corresponding Kit Number: RMN5054 | W872 | 656 | $35.00
ADD: GOOSENECK PTT | Requires Visor Mic. Kit Number: HMN1087A | G233 | 656 | $66.00
ADD: PTT FOOTSWITCH | Requires Visor Mic. Kit Number: GLN7278 | G235 | 656 | $60.00
ADD: PUSHBUTTON PTT | - | GA00304 | 656 | $66.00
ADD: NO MICROPHONE NEEDED | - | G90 | 656 | $0.00

#### Emergency (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: EMERGENCY ID EXT. FOOTSWITCH | Corresponding kit: HLN5113. | W470 | 656 | $66.00
ADD: EXTERNAL EMERGENCY PUSHBUTTON | Corresponding kit: HLN5131 | W688 | 656 | $66.00

#### Direct Mode Entry & Status/Message

Require Remote Mount configuration.

Description | Full Description | Nomenclature | APC | Price
ADD: 8 MODE DIRECT ENTRY | Corresponding kit: H1835 | W599 | 656 | $212.00
ADD: 16 MODE DIRECT ENTRY | Corresponding kit: H1836 | W614 | 656 | $424.00
ADD: 24 MODE DIRECT ENTRY | Corresponding kit: H1837 | W615 | 656 | $636.00
ADD: STATUS/MESSAGE 8 | Corresponding kit: H1838 | W355 | 656 | $560.00
ADD: STATUS/MESSAGE 16 | Corresponding kit: H1839A | W374 | 656 | $765.00
ADD: DEK FOR WHELEN SIREN | Corresponding kit: H1883A | GA00814 | 656 | $124.00

#### 9: Speakers (Must Select One)

Speakers are not compatible with Control Station Operation.

Description | Full Description | Nomenclature | APC | Price
ADD: SPKR 15W WATER RESISTANT | Corresponding kit: HSN4040 | G831 | 656 | $71.00
ADD: SPKR 7.5W WATER RESISANT | Corresponding kit: HSN4038 | G832 | 656 | $72.00
ADD: AUXILIARY SPKR 7.5 WATT | Corresponding kit: HSN4031 | B18 | 656 | $71.00
ADD: AUXILARY COVERT SPKR 10W APX | Corresponding kit: HSN4042 | GA01203 | 656 | $71.00
ADD: AUXILARY SPKR 13W (3.2OHM) | Corresponding kit: HSN4032 | W432 | 656 | $85.00
ADD: NO SPEAKER NEEDED | Required for Control Station | G142 | 656 | $0.00

#### Auxiliary Wildcard

Description | Full Description | Nomenclature | APC | Price
ADD: AUXILIARY SWITCH PANEL | Remote Mount Required. Corresponding kit: HLN1196. | W591 | 656 | $195.00

#### Documentation (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: PRINTED TEST RESULTS APEX | - | G799 | 656 | $12.00
ADD: APX MOBILE USER GUIDE | User Guide CD. PDFs of User Guides can be found on the page. | G657 | 656 | $30.00
ADD: DATA LINK MANAGER APP CD- MOBILES | Option provides the NVN5424 Data CD. Please order this option if you would like the Data CD, and are unable to obtain it through other sources such as MOL. | QA00205 | 655 | $0.00

#### RFID (Optional)

Description | Full Description | Nomenclature | APC | Price
ADD: RFID LABEL | - | GA00268 | 656 | $30.00

#### 11. Service Option (Must Select One)

Description | Full Description | Nomenclature | APC | Price
ADD: 3Y ESSENTIAL SERVICE | - | G78 | 185 | $288.00
ADD: 3Y ESSENTIAL ACCIDENTAL DAMAGE | - | GA00249AE | 185 | $402.00
ADD: 5Y ESSENTIAL SERVICE | - | GA00318 | 185 | $480.00
ADD: 5Y ESSENTIAL ACCIDENTAL DAMAGE | - | GA00255AF | 185 | $670.00
ADD: 7Y ESSENTIAL SERVICE | - | HA00694 | 185 | $670.00
ADD: 7Y ESSENTIAL ACCIDENTAL DAMAGE | - | HA00695 | 185 | $844.00

#### Programming Solutions

CPS single unit programming is included with all APX N-Series device purchases. For advanced programming solutions including features like batch programming, programming over WiFi or LTE, Motorola hosted or Cloud solutions, you will need to order one of the below tools. You may select between 1-5 years of access. RadioCentral and RadioManagement (MSI Hosted) are ordered on a per device, per year basis. The pricing in the table below is per device, per year.

Description | Full Description | Nomenclature | APC | Price
RadioManagement (On-Prem) | See “How to Order” section in the Ordering Guide below. | N/A | N/A | N/A

Customer Programming Software

Description | Full Description | Nomenclature | APC | Price
CABLE CH, PROGRAMMING,USB | HKN6184C - Used to program the radio with Customer Programming Software and Tuner Software. Compatible with APX mobile radios. | HKN6184C | 261 | $243.00

Programming and Data Cables
(Please see CPS PART NUMBER GUIDE for cable descriptions)

Description | Full Description | Nomenclature | APC | Price
CABLE KIT 20' DATA | RS232 Data Interface Cable - REMOTE | HKN6161 | 500 | $50.00
CABLE CH, PROGRAMMING,USB | HKN6184C - Used to program the radio with Customer Programming Software and Tuner Software. Compatible with APX mobile radios. | HKN6184C | 261 | $243.00

####