Back

##### KVL 4000 FLASHport

###### Product Catalog

##### Jump to ...

- Model
- Ordering Information
- Configuration
- Ship Card

Back

##### KVL 4000 FLASHport

### Model

KVL
Key Variable Loader
FLASHport® Aftermarket Upgrades

### Ordering Information

#### General Information

FLASHport® Aftermarket Software is used to upgrade the existing System Software Package or to add Enhancement Options to existing KVL (Key Variable Loaders.) The FLASHport® Upgrade Kit contains:

- Relevant software on a CD-Rom
- Upgrade Instructions

The KVL Software Upgrade DOES require the use of a personal computer and programming cable. The software is delivered via the CD-Rom.

#### Ordering Requirements

1. Each Upgrade Kit (T7586) consists of a CD-Rom that can upgrade one individual KVL.
2. Tech Edit will request for KVL Serial Number and Current Operation Mode Programmed in KVL - ASN Mode or ASTRO 25 Mode. Please have this information ready when ordering KVL Flashport.
3. REQUIRED to select REFRESH option of existing operation mode when upgrading KVL - CA01635AA, CA01636AA, CA02010AA.
4. REQUIRED to use USB communication charging cable for any operation mode upgrades or refresh - 25-108022-04R.
5. Modem (DSUSR5637MODEM) is required with ASTRO 25 Mode when using KVL-KMF communication remotely.
6. USB/ethernet adapter (DSPSA1U1EE) is REQUIRED for -

- ASTRO 25 MODE when using KVL-KMF communication remotely via IP connectivity
- USB/ethernet adapter (DSPSA1U1EE) is REQUIRED for Radio Authentication.

REMINDER: When selecting an upgrade (e.g. CA01633AA or CA01798AA) you must also select Software Refresh options for any existing modes on your KVL4000 (e.g. CA01635AA, CA01636AA, CA02010AA)

REMINDER: You will be required to enter the Serial Number of the KVL you will be upgrading. KVL serial numbers begin with 201. Failure to enter the correct KVL serial number may result in a non-functional Upgrade CD.

REMINDER: The algorithm, DES, is only available on APX 6000 and above.

*ENCRYPTION--All encryption products, kits, software, and technology require an approved export license prior to shipment. Review the following link http://exportcontrols.mot.com/ for any possible licensing restriction. The international use of encryption algorithms (except for DES, DES-XL, & DES-OFB) are highly restricted by the U. S. Federal Government. License approvals are considered for export to a limited selection of countries and end users. Review the above link, for a list of contacts, for the Global Trade Compliance Organization, for licensing information before submitting bids, proposals, or accepting orders for algorithm based encryption products.

### Configuration

#### Models

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
KVL 4000 FLASHPORT UPGRADE | - | T7586 | 462 | $100.00

#### Options

Operation Mode

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ASTRO 25 MODE | Please select ASTRO 25 Mode if you would like to enable this feature and already have ASN Mode enabled. Incompatible with CA01635AA. | CA01633AA | 462 | $250.00
ADD: ASN MODE | Please select ASN Mode if you would like to enable this feature and already have ASTRO 25 Mode enabled. Incompatible with CA01636AA | CA01798AA | 462 | $500.00

Systems Enhancement Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: KVL RADIO AUTHEN FLASHPORT | Please select Radio Authentication Mode if you would like to enable this feature. ASTRO 25 Mode is required. Incompatible with CA02010AA | QA01767AP | 462 | $500.00

Software Refresh

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SW UPGRADE TO CURRENT ASTRO 25 | This refresh is REQUIRED if you already have ASTRO 25 Mode enabled in KVL. Not compatible with CA01633AA | CA01635AA | 462 | $50.00
ENH: KVL RADIO AUTHENTICATION UPGRADE | This refresh is REQUIRED if you already have Radio Authentication Mode enabled in KVL. Not compatible with QA01767AP | CA02010AA | 201 | $50.00
ENH: SW UPGRADE TO CURRENT ASN MODE | This refresh is REQUIRED if you already have ASN Mode enabled in KVL. Not compatible with CA01798AA | CA01636AA | 462 | $50.00

Algorithm Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DVP-XL ENCRYPTION | - | CA01632AA | 462 | $750.00
ADD: DVI-XL ENCRYPTION | - | CA01640AA | 462 | $750.00
ADD: DES/DES-XL/DES-OFB ENCRYPTION | - | CA01638AA | 462 | $1,550.00
ADD: ADP PRIVACY | - | CA01641AA | 462 | $300.00
ADD: AES ENCRYPTION | - | CA01639AA | 462 | $750.00

UNDEFINED

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: LOCALIZED ENABLED ENCRYPTION (BR) | - | CA02611 | 462 | $750.00

####

### Ship Card

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
FIXEDSTN | SCB | T7586 | KVL 4000 FLASHPORT UPGRADE | 462 | 53