Back

##### MOTOMESH Extension

###### Product Catalog

##### Jump to ...

- Model
- General Information
- Features and Components
- Ordering Requirements
- Service and Training
- Ship Card

Back

##### MOTOMESH Extension

### Model

MOTOMESH Extension Kit - 2.4/4.9 GHz Broadband Data Solution

### General Information

The MOTOMESH Extension Kit is a prepackaged system for municipalities and public safety agencies looking to provide dedicated licensed network connectivity to first responders, license-free mobile broadband to public works employees, and WiFi access to public users - all over a single network. The MOTOMESH Extension kit enables cost-effective scalability and simplified municipal wireless broadband deployments. It is the first and only integrated private and public combined solution available on the market.

The MOTOMESH solution is a dual-band wireless broadband data system that operates at the 2.4 GHz ISM band (unlicensed) and 4.9 GHz (licensed) public safety band using mesh networking technology. This system provides both wide-area broadband data coverage and peer-to-peer ad-hoc networking. This system also provides users with sustained high data rate performance at vehicular speeds and with location capabilities, which are unique attributes that are not found in competing solutions and are considered critical to many public safety applications. The system is designed primarily to satisfy the needs of public safety on the 4.9 GHz band. This system is also designed to simultaneously serve other municipal constituencies, such as public works agencies and general public access, over the unlicensed 2.4 GHz band. The multiple use cases provide a strong value proposition for municipalities by spreading the Total Cost of Ownership (TCO) rationalization over a wider base of users.

In addition to a MOTOMESH equipment package (detailed below) the MOTOMESH Extension kit includes various options: AirMobile™, Wireless Network Extension, and Multi-Net Mobility™. AirMobile allows you to easily manage large file transfers and software updates. Wireless Network Extension allows you to extend your mobile coverage with access to public networks. Multi-Net Mobility adds security and session persistence while you seamlessly roam across coverage areas and between your private network and the public network.

### Features and Components

The complete MOTOMESH Extension Kit offers the optimal combination of features to leverage the integrated technology.

MOTOMESH

- Infrastructure meshing to create a wide-area broadband wireless backhaul

- High data rate mobile communication at vehicular speeds, achieving 6 Mbps burst data rates to a single user

- Support high speed motion and seamless hand-off between infrastructure nodes

- Self-forming and self-healing wide-area wireless mesh routing, providing increased network availability and robustness

- Client meshing allows for ad hoc and unique vehicle extensions

- Geo-location services

- Quality of Service for mission critical communications and differentiated services

- Symmetric data rates to and from users

- Wireless element management system, including configuration managements, statistics reporting, alarms and remote firmware upgrade

- Hardware and User authentication of wireless networking devices

- Differentiated services using IP Quality of Service

- IP networking and transport services with a single mobile internet switching center kit

The MOTOMESH Extension Kit includes the following MOTOMESH Level 2 Starter Kit components:

2 Internet Access Points with VLAN (IAP7300-01)

4 Mesh Wireless Routers (MWR7300) without Ethernet ports

5 Vehicular Mounted Modems (VMM7300)

15 Wireless Modem Cards (WMC7300)

1 Linux MiSC with 200 Device Licenses

2 Mesh Cameras

For more information, see the MOTOMESH E-CAT Pages and Mesh Camera E-CAT Pages

In addition to the standard MOTOMESH equipment described above, the full MOTOMESH Extension Kit solution includes:

AirMobile

- Secure, 256 bit, AES-compliant data encryption with compression

- Centralized, automated, scheduled, prioritized content delivery

- Robust error and session recovery

- Individual and group update capability

- Transfer progress indicators and per-client upload tracking

The AirMobile option includes the following components:

1 AirMobile server, server software, and OS

20 AirMobile client licenses

For more information, see the AirMobile Page

Wireless Network Extension

- First and only integrated private and public solution on the market

- Single point of contact for customer's wireless data network design and customer care

- Expanded broadband coverage to wide area

- Application roaming when combined with Multi-Net Mobility

The Wireless Network Extension option includes the following components:

5 Wireless PCMCIA data cards with installation software and user guide

2 Year unlimited* data plan for 5 users

* Subject to restrictions per carrier

Multi-Net Mobility

- End-to-End Security with "always on" AES 256 bit encryption between end device and fixed equipment

- Session Persistence to automatically suspend/reconnect open application sessions across network holes

- Intelligent Routing selects the best available network, blocks applications from unintended networks and prioritizes application traffic

The Multi-Net Mobility option includes the following components:

1 HP ProLiant DL360 server, with Linux, keyboard, and mouse

1 19 inch monitor

1 Multi-Net Mobility server software package

20 Multi-Net Mobility client licenses - for 15 WMC cards and 5 VMMs (additional can be ordered as required)

For more information, see the Multi-Net Mobility Page

Installation and optimization is included as part of the MOTOMESH Extension solution. Reference the Technical Support SOW for more details.

This and other customer communication templates can be found at the TAG Contracts and Compliance Site

### Ordering Requirements

A detailed site survey and system design should be done prior to ordering, to determine the proper network configuration required. This should be done in conjunction with the Broadband Specialist in your region or through your Business Development Manager.

All orders must be entered into the Customer Order Fulfillment (COF) system.

A complete MOTOMESH Extension system configuration consists of the following, but can be ordered a la carte. (Note: the AirMobile pricing below is only available when ordered with the Starter Kit):

1. 1 MOTOMESH Level 2 Starter Kit with design and implementation services -

2. 1 AirMobile Server with 20 client licenses, installed -

3. 5 Wireless Network Extension data cards with 2 year data plans -

4. 1 Multi-Net Mobility server, software, and 20 client licenses, and installation -

Please consult the MOTOMESH System Home Page to gain access to the System Planner document, system configuration tool(s), FAQ list, and other support documentation that is relevant to the MOTOMESH solution prior to ordering.

The following process outline should be followed when ordering a MOTOMESH Extension Network:

Step 1 - Order a MOTOMESH Starter Kit

Step 2 - To add AirMobile, order:

1 SCA4304 AirMobile server software package

20 Option SCA4300 AirMobile client licenses

1 Option ZA00107AA CD-ROM media

1 DSPE860KMMWIN03 Dell PowerEdge 860 Server

Step 3 - To add Wireless Network Extension, order:

120 Kit TT1971A

5 Option TT05030AA

Step 4 - To add Multi-Net Mobility, order:

1 Model T7258A MNM Server Software

20 Option ZA00484AA MNM Client Licenses

1 DDN9003B Server with O/S

1 DS019BLK 19 inch monitor

1 Installation required, please contact your Business Development Manager for details.

Step 5 - Service and Technical Support:

Engineering, design, installation, optimization, test, and project management are all included

Step 6 - Training: Professional training classes are offered and conducted by Motorola's Worldwide Learning Services group. Contact Worldwide Learning Services at 847-538-7999 to obtain information about the training session offerings.

Step 7 - Field Upgrades, Spares, and Replacements: Hardware and software field upgrades, spares, and replacements are available as accessories as required.

Our certified and recommended backhaul products supplied by Motorola Canopy are provided and orderable as accessories for this system. These should be ordered based on the outcome of a detailed site survey and system design. Some common Canopy items are listed on these pages. For more complete information regarding Canopy models and options go to http://il02cms01.comm.mot.com/prodsys/pagelist.asp?catid=183

### Service and Training

Service

1 Year Standard Warranty and Maintenance is included with the product and includes Monday through Friday 9-4 CST technical support, software updates to address defect repair issues, and depot unit repair.

Post warranty services are offered as a bundle and include the following:

- Monday through Friday 9-4 CST technical support (7x24 support option is available)
- Software defects repair
- Depot Unit repair
- 8x5 on-site Dispatch of customer bucket truck to IAP/MWR sites
- 8x5 on-site dispatch of Motorola personnel for the MiSC (7x24 option is available)

Services can be ordered directly through the Customer Support Manager. Contact your regional business service BDM to arrange for a quotation.

Training

Both on-site and off-site training class options will be available. Class size will be limited, and on-site classes are to be held in Schaumburg. The pricing below is on a per student basis and only applies to on-site classes held in Schaumburg. Off-site classes will need to be quoted separately.

Contact Worldwide Learning Services at 847-538-7999 to obtain information about the training session offerings.

### Ship Card

Data Not Available

####