Back

##### PDR8000

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Software & Services
- Update History
- Ship Card

Back

##### PDR8000

### Model

PDR8000- PORTABLE DIGITAL REPEATER

Special ops and security detail teams requiring enhanced, Conventional, two-way radio network coverage can look to the PDR8000 Portable Digital Repeater as their solution of choice when on the move.

The lightweight suitcase is suited for discreet travel whereas the Rackmount form factor is designed to fit in a standard 19” rack. Set up the PDR8000 suitcase at a special event or incident to swiftly provide local P25 or analog FM, on-scene portable radio coverage. Connect to your dispatch console wherever it may be via a V.24 (for P25) or Ethernet IP (Analog or P25) connection.

### Updates

December 2024-

PRICING: As of Jan 1, 2025, there is a price increase on all PDR8000 base models. The pricing in the Model Selection section below reflects the new pricing.

FUTURECOM WEBSITE: The Futurecom website will no longer be accessible as of Jan 6th, 2025. All information has been relocated to MSI locations. Below are the Support Documentation & Software categories of information previously available on the Futurecom website with the new locations.

- PDR8000 Datasheets: Suitcase and Rackmount
- Firmware (available through Customer Hub): Firmware, Release Notes, Firmware Upgrade Instructions
- FRC Programming Software (available through Customer Hub): FRC Software, Release Notes
- Ordering Guide: PDR8000 Ordering Guide
- RF Safety Booklet: PDR8000, Booster Pack
- User Documentation:
  - Product Planner
  - PDR8000 and Booster Pack Deployment Guide
  - Programming Guide
  - Connectivity Deployment Application Note
  - Battery Pack and Charger User Guide

Miscellaneous: How to Video and Case Studies

September 2024- Please see Ordering Information section below for details on where the PDR8000 product can be shipped to. There are changes to the list of countries that this product meets regulatory and compliance requirements for. If there is an opportunity in a country not on the list, here is the process to submit a request for regulatory approval:

- contact regulatorycomplianceteamkrk@motorolasolutions.com to determine what is needed for regulatory approval
- work with Ernesto Gonzalez, International GTM, to create a business case
- submit business case to Mobile Devices Product Manager, Jennifer Price, for prioritization

August 2024- Please note that all prices are in USD. Unable to automatically convert to CAD for Canadian PCAT page at this time.

### Ordering Information

#### PDR8000 Regulatory and Compliance Valid Countries List

In addition to Canada and the United States, the PDR8000 can be sold to the following countries:

Algeria | Eritrea | Rwanda
Angola | Ethiopia | Saint Helena
Australia (UHF 380-430MHz only) | Gabon | Sao Tome and Principe
Azerbaijan | Gambia | Senegal
Benin | Georgia | Seychelles
Burkina Faso | Guinea | Sierra Leone
Burundi | Guinea-Bissau | Somalia
Cameroon | Kenya | South Sudan
Cape Verde | Liberia | Sudan
Central African Republic | Madagascar | Tajikistan
Chad | Malawi | Tanzania United Republic of
Comoros | Mali | Togo
Congo | Mauritania | Turkmenistan
Congo the Democratic Republic of the | Morocco | Uganda
Cote D'Ivoire | Mozambique | Uzbekistan
Djibouti | Niger | Zambia
Equatorial Guinea | Philippines | Zimbabwe

#### Standard Features

 Lightweight construction - less than 28 lbs. (including duplexer)

 Rapid deployment with AC or DC power source capability

 Closed case operation at 50% Transmit duty cycle

 Easy to swap internal duplexer

 Able to use external duplexer

 End-to-end Encryption supported

 Voting and Comparator operation

 Wireline V.24 serial connection to Motorola Solutions P25 system infrastructure

 Wireline Ethernet IP connection to consoles supporting Digital Fixed Station Interface Protocol Version 1 (analog and digital

 Standalone repeater for P25, analog FM, and mixed-mode operation

 LCD screen & keypad allow easy access to Channel Change and other features

Ordering Guide

### Configuration

To ensure accuracy of PDR8000 configuration, please create Quotes and Request Orders in CPQ- accessible through Salesforce.

Below are the steps for configurating a PDR8000. Please refer to the following video for a demonstration on how to configure in CPQ.

#### 1. Model Selection

Select the Frequency Band, Approximate Quantity of Order and Operation Mode.

#### Frequency Band

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
700MHz | PDR8000 700MHz | T93USS9PW1AN | 0482 | $11,076
800MHz | PDR8000 800MHz | T93VSS9PW1AN | 0482 | $11,076
VHF | PDR8000 VHF | T93KSS9AW1AN | 0482 | $11,076
UHF- 380-430MHz | PDR8000 UHF 380-430MHz | T93PSS9PW1AN | 0482 | $11,076
UHF- 450-470MHz | PDR8000 UHF 450-470MHz | T93RSS9PW1AN | 0482 | $11,076
UHF- 470-512MHz | PDR8000 UHF 470-512MHz | T93SSS9PW1AN | 0482 | $11,076

#### Approximate Quantity of Order

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
Less than 20 | For production reference | n/a | n/a | n/a
20 or more | For production reference | n/a | n/a | n/a

#### Configuration Type

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
Suitcase | ADD: PDR8000 PARTS COLLECTION VHF/UHF | QA09643AA | 0482 | $6,050
| ADD: PDR8000 PARTS COLLECTION 700/800 | QA09644AA | 0482 | $6,050
Rackmount | ADD: PDR RACKMOUNT - BASE NO DUPLEXER | QA09670AA | 0482 | $4,376
| ADD: PDR RACKMOUNT - BASE+PA NO DUPLEXER | QA09671AA | 0482 | $4,376
| ADD: PDR RACKMOUNT - BASE+ALARM NO DUP | QA09672AA | 0482 | $4,376
| ADD: PDR RACKMOUNT- BASE+PA+ALARM NO DUP | QA09673AA | 0482 | $4,376
| ADD: PDR RACKMOUNT - BASE+DUPLEXER | QA09645AA | 0482 | $4,376
| ADD: PDR RACKMOUNT - BASE+PA+DUPLEXER | QA09667AA | 0482 | $4,376
| ADD: PDR RACKMOUNT - BASE+ALARM+DUPLEXER | QA09668AA | 0482 | $4,376
| ADD: PDR RACKMOUNT - BASE+PA+ALARM+DUP | QA09669AA | 0482 | $4,376

#### Select Suitcase Color (suitcase configuration only)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
Black | ADD: CASE PDR8000 BLACK | QA09646AA | 0482 | $0
Yellow | ADD: CASE PDR8000 YELLOW | QA09647AA | 0482 | $385

#### 2. System Enhancements

Select the Duplexer and Feature types.

#### Duplexer

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
None | DEL: DELETE DUPLEXER | QA09674AA | 0482 | $0
700MHz | ADD: DUPLEXER 700MHz 764-775 & 794-805 | QA09655AA/QA09656AA | 0482 | $1,075
800MHz | ADD: DUPLEXER 800MHz 806-816 & 851-861 | QA09660AA/QA09661AA | 0482 | $1,075
VHF | ADD: 3D DUPLEXER | QA09650AA | 0482 | $1,075
| ADD: DUPLEXER ASM PDR8000 RACKMOUNT VHF (additional assembly for Rackmount only) | QA09770AA | 0482 | $225
UHF- 380-430MHz (9.5-10.5Mhz Tx to Rx Separation) | ADD: 3D DUPLEXER | QA09650AA | 0482 | $1,075
| ADD: DUPLEXER ASM PDR8000 RACKMOUNT UHF (additional assembly for Rackmount only) | QA09771AA | 0482 | $225
UHF- 380-430MHz (4.5-5.5Mhz Tx to Rx Separation) | ADD: 3D DUPLEXER | QA09650AA | 0482 | $1,075
| ADD: DUPLEXER ASM PDR8000 RACKMOUNT UHF (additional assembly for Rackmount only) | QA09771AA | 0482 | $225
UHF- 450-470MHz | ADD: DUPLEXER UHF 450-470 | QA09651AA/QA09652AA | 0482 | $1,075
| ADD: DUPLEXER ASM PDR8000 RACKMOUNT UHF (additional assembly for Rackmount only) | QA09771AA | 0482 | $225
Custom | ADD: CUSTOM FREQUENCY PLAN | QA09537AA | 0482 | $3,138

#### Feature Type

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
V.24 Wireline | ENH: PDR8000 V.24 WIRELINE OPERATION | QA09657AA | 0482 | $6,250
Deployment Profiles Capability | ENH: PDR8000 DEPLOYMENT PROFILES | QA09637AA | 0482 | $770
DFSI Operation | ENH: PDR8000 DFSI OPERATION | QA09638AA | 0482 | $6,250
Motorola IP Operation | ENH: PDR8000 MOTOROLA IP OPERATION | QA09664AA | 0482 | $6,250
50W Amplifier | ADD: RACKMOUNT PDR PA ASSEMBLY VHF | QA09640AA | 0482 | $7,945
| ADD: RACKMOUNT PDR PA ASM UHF 380-430MHz (not available in Canada) | QA09641AA | 0482 | $7,945
| ADD: RACKMOUNT PDR PA ASM UHF 450-470MHz (not available in Canada) | QA09642AA | 0482 | $7,945
Alarm Capability | ADD: RACKMOUNT ALARM CAPABILITY | QA09608AA | 0482 | $441

NOTE: Alarm capability and Power Amplifier enhancements are only available for the Rackmount configuration.

#### 3. Frequency Information

When frequency information is known, enter the PDR8000 frequencies. If frequency information is not known, select slider to save for quoting purposes.

#### 4. PDR8000 Frequencies

Enter customer frequencies that meet the selected duplexer frequency plan requirements. For simplex applications, the same Tx/Rx frequency can be used.

#### 5. Services

Select the required warranty type, duration and billing.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
Standard | 1 year | QA05100AA | 0185 | $0
Essential | 3 Years | LSV01S04107A | 0185 | $576
| 5 Years | LSV01S04107A | 0185 | $960
| 7 Years | LSV01S04107A | 0185 | $1,344
Essential with Accidental Damage | 3 Years | LSV01S04110A | 0185 | $1,692
| 5 Years | LSV01S04110A | 0185 | $2,820
| 7 Years | LSV01S04110A | 0185 | $3,948

NOTE: Essential with Accidental Damage is not available for the Rackmount configuration.

#### 6. Required Order Information

Enter the contact information for any technical questions that may come up related to the frequencies and equipment selected.

### Software & Services

Info coming soon.

### Update History

### Ship Card

Current delivery lead time is 16-18 weeks ARO with valid frequency information.