Back

##### APX 6500 Mobile Radio

###### Product Catalog

##### Jump to ...

- Model
- Updates
- Ordering Information
- Configuration
- Ship Card

Back

##### APX 6500 Mobile Radio

### Model

ASTRO® Digital Enhanced APX 6500 Mobile Subscriber

700/800 MHz
764-776 MHz (3-30 W); 851-870 MHz (3-35 W)

Secure and Trunked Radio Systems

### Updates

- CLICK HERE to see the Latest Lead Time Estimates

Effective June 19th, 2020: The price of the O5 control head (option G442 and kit H1904) will be increased to $572. Please consider the new E5 control head as an option.

Effective March 11th, 2020: The APX 6500 7/800, UHF R1, and VHF Models have evolved to support newer technologies like WiFi and SmartConnect. This model also has a smaller form factor and will support motorcycle configuration. Direct cloning with Legacy models will not be available. In order to receive an Enhanced APX 6500 7/800 Model, order M25URS9PW1BN, M25QSS9PW1BN, M25KSS9PW1BN.

The 7/800 models are available now.

Orders for the UHF R1 & VHF Models will go on hold until Ship Acceptance in June, 2020.

Effective March 5th, 2020: All U.S. orders will book as P25 CAP Compliant by internally generating the P25 “clear” non-encryption option QA05751 (Disable Encryption) if no other encryption is selected. ADP will no longer ship standard. It will now be an orderable option (G193 for mobiles, Q667 for portables). Units shipped with QA05751 are not field-upgradable for encryption and any changes will require units to be sent to a depot. Further ordering changes are captured in the Encryption Algorithm and Multikey sections below.

### Ordering Information

#### Please Read All Option Descriptions Before Making Your Selection

Required Selections:

1) Main Model (M25URS9PW1BN)

2) Mounting

3) Control Head Selection

4) RF Antenna

5) Operation Mode

6) Feature Antenna(s)

7) Remote Mount Cables (if remote mount is selected)

8) Microphone

9) Speaker

10) Service

### Configuration

#### 1. Main Model (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
APX6500 ENHANCED 7/800 MHZ | Enhanced Model | M25URS9PW1BN | 527 | $3,518.00

#### 2. Mounting (Must Select One)

If a remote mount cable other than 5 meters (17ft) is desired for Remote Mount, please reference the "Remote Mount Cables" section.

The O3 dash and remote mount configurations are the same except that the dash mount configurations does not come with the 17ft extension cable, PMLN4958.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DASH MOUNT | Required for Control Station Operation. | G66 | 656 | $138.00

#### Motorcycle Mounting (Optional)

HMN1079 (Motorcycle Mic) and HSN4031 (Speaker) are mandatory selections with this option. Motorcycle mount requires the O2, O5 or O7 Control Head and G67 Remote Mounting. Only available with 5 meter (17 ft) cable). Incompatible with DVRS MSU operation (GA00631).

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX MOTORCYCLE CH SFWR | Requires M25URS9PW1BN model and G67 (Remote Mount) | G138 | 656 | $0.00
ADD:REMOTE MOUNT MOTORCYCLE | Requires G138 (Motorcycle) | G67BA | 656 | $440.00

#### Trunnion Screws

The APX 6500 Enhanced model will ship with HLN6861 to accommodate the smaller form factor. If it is required to use the previous APX 6500 model trunnion, HLN7002, order GA01693 which provides KT000053A01, screws that will fit the previous trunnion.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD : LEGACY TRUNNION SCREW KIT | Corresponding kit: KT000053A01 Requires remote mount | GA01693 | 471 | $11.00

#### Control Station Operation (Optional)

O2, O5, & O7 Control Heads Only. Must select one.

Requires Dash Mount (G66)

Some microphones are not compatible with Control Station Operation. Please read descriptions carefully.

Although the Power Supply is optional, it is needed for a full Control Station solution.

Power Supply HPN4007 (used in Control Station configuration for AN Models) is not approved for use on M25URS9PW1BN. Please use KT000254A01 (G91).

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: CONTROL STATION POWER SUPPLY | Although the Power Supply is optional, it is needed for a full Control Station solution. Corresponding kit: KT000254A01 | G91 | 656 | $296.00
ADD: CONTROL STATION OPERATION | Requires a O2, O5, or O7 Control Head. Requires Dash Mount (G66) Some microphones are not compatible with Control Station Operation. Please read descriptions carefully. | W665 | 656 | $77.00

#### 3A Control Head Software (Required)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX CONTROL HEAD SOFTWARE | Required for all mobile radio configurations. | G444 | 656 | $0.00

#### 3B Control Head Options (Must select one)
O2 Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX O2 CONTROL HEAD | Default Gray. Order G201 if green is required. | GA00804 | 656 | $541.00
ADD:IMPACT GREEN COLOR HOUSING (O2) | When ordered in conjunction with GA00804 you will get a green housing. | G201 | 656 | $28.00
ADD: SCHOOL SERCURITY ENHANCEMENT PACKAGE | Education O2 Emergency Push Button | GA01056 | 514 | $55.00

#### O3 Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD:CH SIREN & LIGHTS KEYPAD | Available on O3 (G72) and O7 (GA00805) Control Heads. | GA00806 | 656 | $55.00
ADD: APX O3 HANDHELD CH | Requires No Microphone (G90). If Lights & Siren Keypad and Software is required, order GA00806. | G72 | 656 | $1,041.00

#### O5 Control Head Option

Effective June 19th, 2020: The price of the O5 control head (option G442 and kit H1904) will be increased to $572. Please consider the new E5 control head as an option.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: O5 CONTROL HEAD | Effective June 19th, 2020: The price of the O5 control head (option G442 and kit H1904) will be increased to $572. Please consider the new E5 control head as an option. | G442 | 656 | $629.00

#### E5 Control Head Option

#### O7 Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX O7 CONTROL HEAD. | If Lights & Siren Keypad and Software is required, order GA00806. | GA00805 | 656 | $695.00
ADD:CH SIREN & LIGHTS KEYPAD | Available on O3 (G72) and O7 (GA00805) Control Heads. | GA00806 | 656 | $55.00

#### No Control Head Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX MOBILE NO CONTROL HEAD | If you already have a control head and don't require it, select G88. Requires remote mount option (G67). | G88 | 681 | $0.00

#### Dual Control Head (Optional)

The APX 6500 mobile can support up to two control heads on a single transceiver. This allows control of a single APX 6500 transceiver from two different control head locations.

Dual Control Head requires Remote Mount.

When ordering the dual control head option, only one type of control head can be selected.

Only available with O2, O5, O7 Control Heads.

The Dual Control Head Option requires an equal number of microphones, speakers, and CAN cables.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: APX DUAL-CONTRL HD HARDWARE | Requires either O2/O5/O7 Control Head. Requires a remote mount configuration. Requires a selection of 2 for microphones, speakers and CAN cables. | GA00092 | 656 | $627.00

#### 4. RF Antenna (Required)
No Antenna Requested

#### 7/800 Antennas

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANT 3DB LOW-PROFILE 762-870 | Corresponding kit: HAF4013 Incompatible with motorcycle operation. | G174 | 656 | $47.00
ADD: ANT 3DB ELEVATED FEED 762-870 | Corresponding kit: HAF4014. Incompatible with motorcycle operation. | G175 | 656 | $83.00
ADD: ANT 1/4 WAVE 762-870 MHZ | Corresponding kit: HAF4016 Incompatible with motorcycle operation. | G335 | 656 | $15.00
ALT: ANT 3DB GAIN 762-870MHZ | Corresponding kit: HAF4017 Incompatible with motorcycle operation. | W484 | 656 | $42.00
ADD: ANT 3DB LOWPRO MCYC 762-870 | Corresponding kit number: HAF4018 Requires motorcycle operation (G138) | G174 | 656 | $47.00
ADD: ANT 3DB MCYCLE 762-870MHZ | Corresponding kit number: HAF4015. Requires motorcycle operation (G138) | G335 | 656 | $15.00

#### Dual Radio Operation Options

The APX Dual Radio Feature offers the capability to control TWO (2) APX8500, APX7500, APX6500, or APX6500Li mobile radios from ONE (1) O7 control head. APX Dual Radio allows for mixing and matching of radios across tiers (i.e. APX 8500 with APX 6500) and power levels (High Power with Mid Power).

Each radio in an APX Dual Radio system must be ordered independently.

The mobiles in a dual radio solution can be single or dual band. Both radios can be on the same or different frequency bands.

One radio must be ordered with the Primary Radio option (GA01113) and the other with the Secondary Radio option (GA01117). This will include both the SW and HW required for dual radio operation.

Although each radio must be ordered as either a Primary or Secondary radio, each radio can be configured to work as a Primary, Secondary, or a Standalone radio.

Only one speaker can be connected to the control head and it will play audio from the primary radio. A 30 ft. speaker extension cable is included on the secondary radio to connect the second speaker directly to the secondary radio. If a longer cable is needed, a 131 ft. version can be purchased from AAD (part # HKN6251)

The Dual Radio feature is incompatible with the multi-control head options.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: DUAL RADIO OPERATION (PRIMARY RADIO) | The Primary radio must be ordered with an O7 CH. APX Dual Radio is not compatible with any other control head. The primary radio includes a short dual radio CAN cable (HKN6245) to connect both radios together. If the stack mount trunnion is ordered, a right-angle version of this cable (HKN6249) will ship instead to facilitate stack-mounted installations. If a different length is desired, the standard remote mount control head cables can also be used to connect both together. | GA01113 | 656 | $715.00
ENH: DUAL RADIO OPERATION (SECONDARY RADIO) | The secondary radio must be ordered with no control head (G88). | GA01117 | 656 | $715.00

#### Dual Radio Options

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DUAL RADIO STACKABLE MP TRUNNION | Corresponding kit: HLN7045B | GA01115 | 656 | $327.00

#### 5: Operation Mode (Must Select One)
5A: Digital Trunking (SN/SZ P25 Phase I Interop)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: P25 TRUNKING SOFTWARE APX | Required when ordering Smartzone Operation (G51) & Digital Operation (G806). Smartzone Omnilink (G173) is included with this option. | G361 | 656 | $330.00
ENH: SMARTZONE OPERATION APX6500 | Incompatible with G48. | G51 | 527 | $1,320.00

#### 5B: Digital Trunking (SN/SZ)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SMARTZONE OPERATION APX6500 | Incompatible with G48. | G51 | 527 | $1,320.00

#### 5C: Digital Conventional (P25)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: CONVENTIONAL OPERATION APX6500 | Not compatible with G51. | G48 | 527 | $550.00

#### 5D: Analog Trunking

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SW ASTRO READY (ANALOG) | Not compatible with G806 or with Encryption Algorithm W969, W793, W797, G625, G298, G851, or G843 when combined with a Trunking Software Option. | G241 | 656 | $0.00
ENH: SMARTZONE OPERATION APX6500 | Incompatible with G48. | G51 | 527 | $1,320.00

#### 5E: Analog Conventional

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SW ASTRO READY (ANALOG) | Not compatible with G806 or with Encryption Algorithm W969, W793, W797, G625, G298, G851, or G843 when combined with a Trunking Software Option. | G241 | 656 | $0.00
ENH: CONVENTIONAL OPERATION APX6500 | Not compatible with G51. | G48 | 527 | $550.00

#### System Enhancement Options (Optional)

The following options are optional and will provide additional capabilities, if required.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: MOBILE PERSONAL ACCOUNTABILITY SW | Requires Digital Operation. | G445 | 571 | $150.00
ADD: APX MOBILE RADIO AUTHENTICAT | Requires P25 9600 Trunking (G361). | GA01767 | 527 | $110.00
ADD: DVRS MSU ACTIVATION | Incompatible with Data Modem Tethering. Requires Remote Mount (G67). | GA00631 | 656 | $275.00
ENH: OVER THE AIR PROVISIONING | Requires P25 9600 Trunking (G361). There is no Analog Functionality for this feature. To do in field POP25 programming must use Advanced System Key (DVN4046A). | G996 | 656 | $110.00
ENH: ENHANCEMENT LEVEL 2 | Please reference the Enhancement Level Reference Guide for more details. | GA01771 | 527 | $220.00
ADD: DVRS PSU ACTIVATION | Enables DVRS Enhanced PSU functionality on APX Mobile Radios. Requires Digital Operation. QA00631 is to be ordered for radios that are not connected directly to a DVR. If you are connecting your radio directly to a DVR then order GA00631. | QA00631 | 655 | $110.00
ADD: MISSION CRITICAL GEOFENCING | Requires Digital Operation (G806), IV&D (W947), and GPS (GA00229). | GA09012 | 471 | $165.00
ADD: DIGITAL TONE SIGNALING | Requires Digital Operation (G806). | GA09000 | 656 | $165.00
ADD: GROUP SERVICES | Offers Conventional Alias updates, Trunking Alias updates and Trunking Group Messaging. This option requires Digital Operation (G806) for Conventional only capabilities and G361 for any Trunking only capabilities. You can now also do Over the Air Firmware Updates with this feature. | GA09008 | 656 | $165.00
ADD: MULITCAST VOTING SCAN | Requires Digital Operation (G806). This feature allows for voting of the Conventional Channels only. | G387 | 656 | $220.00
ADD: SITE SELECTABLE ALERT FOR P25 TRUNKING | Requires P25 9600 Trunking (G361). | GA00982 | 656 | $165.00
ADD: TDMA OPERATION APX | Requires P25 9600 Trunking (G361) | GA00580 | 656 | $495.00
ADD: DATA MODEM TETHERING | Requires Remote Mount (G67). Includes GA01545. Incompatible with DVRS MSU (GA00631). Provides for aftermarket cable: KT000247A01. | GA09011 | 681 | $110.00
ENH: TACTICAL RADIO STW-STUN/KILL | Requires Digital Operation (G806), IV&D (W947), and Hardware Encryption. | H02 | 481 | $83.00
ADD: WI-FI CAPABILITY | Compatible with M25URS9PW1BN model only. Requires a WiFi antenna. Supports codeplug updates, firmware refreshes, and FLASHport upgrades over pre-provisioned wireless networks. Requires Radio Management SW (ordered separately). Must order Out of the Box WiFi Provisioning option (GA09007) if provisioning the radios out of the box using WiFi is desired. | GA09001 | 681 | $330.00
ADD: OUT OF THE BOX WI-FI PROVISIONING | Requires GA09001 (WiFi) | GA09007 | 681 | $0.00
ADD: SMARTCONNECT | Requires with WiFi (GA09001) or Data Modem Tethering (GA09011). Also requires KT000259A01, USB Ethernet Satellite Cable when using the Sierra Wireless MG90 or the Cobalt Satellite Modem. | GA01630 | 681 | $0.00

#### 6. Feature Antennas (Must select one)

Must select from either Multi-function section or Singe function GPS section and Single Functoin WI-FI section (if GA09001 is ordered).

Even though GPS comes standard, a GPS antenna, Digital and IV&D are required to implement the full solution.

Step Component

Multifunction Antennas (Must Select One in Multifunction is Selected)

Requires WiFi (GA09001)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: WIFI/GNSS FLEXIBLE CABLE LMR195 | Corresponding kit: AN000163A01 Requires M25URS9PW1BN model | GA00250 | 681 | $110.00
ADD: WIFI/GNSS FLEXIBLE CABLE LMR195 | Corresponding kit: AN000163A02 Requires M25URS9PW1BN and Motorcycle (G138) | GA00250 | 681 | $110.00
ADD: NO GPS/WI-FI ANTENNA NEEDED | Requires M25URS9PW1BN | GA01606AA | 681 | $0.00

#### GPS Antennas (Must select one if single function GPS is required)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: COVERT GNSS GLASSMOUNT LMR100 | Corresponding kit: PMAN4109 Requires M25URS9PW1BN | GA01580AA | 681 | $77.00

#### Wifi Antennas (Must select one if single function WiFi is requested)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: COVERT WIFI GLASSMOUNT 2.4/5 GHZ | Corresponding kit: PMAN5101 Requires M25URS9PW1BN model and WiFi (GA09001). | GA01579AB | 681 | $77.00

#### Advanced System Key (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: HW KEY SUPPLEMENTAL DATA | The software key is the default Advance System Key option that ships standard on all APX products. You cannot order software key QA01749. The HARDWARE KEY QA01648 can be ordered instead. Be sure to enter the correct system owner ID in the supplemental data. If an incorrect ID is entered, a FLASHport order is required to fix the error. Order HARDWARE KEY (QA01648) if required to operate/program on a trunking system. Not compatible with conventional. | QA01648AA | 0655 | $6.00

#### Encryption Algorithms (Optional)

All APX 6500 Mobile Radios ship standard with Single Key Advanced Digital Privacy (ADP).

ADP Privacy is not FIPS compliant - ADP Privacy not supported by OTAR - ADP is digital P25 conventional / P25 trunking only

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: DES/DES-XL/DES-OFB ENCRYPTION AND ADP | Requires Multikey | G625 | 656 | $659.00
ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | Option will go on hold. Any changes to encryption will require sending the unit to the depot. Customers who require compliance with DHS Project 25 CAP Encryption Requirements and who requires a clear radio with no encryption enabled will need to select this option. | QA05751AA | 0655 | $0.00
ADD: AES/DES-XL/DES-OFB ENCRYPTION AND ADP | Not compatible with G843 and G625. Requires Multikey. | G851 | 656 | $879.00
ADD: AES ENCRYPTION APX AND ADP | Requires P25 operation. When ordered with DVP-XL (W797), requires Multikey. | G843 | 656 | $523.00
ADD: DVP-XL ENCRYPTION AND ADP | When ordered with AES Encryption, requires Multikey. | W797 | 656 | $536.00

#### Multikey (Optional. Can only select one)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: MULTIPLE KEY ENCRYPTION OPERATION | Required when using more than one encryption algorithm or encryption key. Required when DES Encryptions, or when AES and DVP are ordered together. | W969 | 656 | $363.00
ENH: ASTRO 25 OTAR W/ MULTIKEY | Includes Multikey (W969), Trunking OTAR, and Tactical OTAR. Tactical OTAR requires IV&D. | G298 | 656 | $814.00
ADD:TACTICAL OTAR APX | Requires digital (G806) and IV&D (W947). | H04 | 656 | $385.00
ADD: MULTI SYSTEM OTAR | Requires OTAR with Multikey (G298) | GA01620 | 656 | $165.00

#### 7. Remote Mount Cables (17 FT STD)

Multi-control head options delete the 17 FT standard cable and customers are required to order a cable per control head. Multi-control head options delete the 17 FT standard cable and customers are required to order a cable per control head. Only for O5 & O7 Control Heads.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD:REMOTE MOUNT CBL 115 FEET | Corresponding kit: HKN6165 | G879 | 656 | $61.00
ADD:CBL REMOTE MOUNT 10 FEET | Corresponding kit: HKN6170 | G618 | 656 | $11.00
ADD: REMOTE MOUNT CBL 30 FEET | Corresponding kit: HKN6168 | G610 | 656 | $28.00
ADD:CBL REMOTE MOUNT 75 FEET | Corresponding kit: HKN6166A | G607 | 656 | $50.00
ADD: REMOTE MOUNT CBL 50 FEET | Corresponding kit: HKN6167 | G609 | 656 | $39.00
ADD: REMOTE MOUNT CABLE 128 FT | For dual control head configurations, the total cable length may not be greater that 131 ft (40 meters). Therefore, this cable should not be used with a dual control head configuration. Corresponding kit: HKN6164 (actual cable length is 128 ft) | G582 | 656 | $72.00
ADD: REMOTE MOUNT CBL 17 FEET | Included at no charge with Single Control Head Remote Mount installations. Corresponding kit: HKN6169 | G628 | 656 | $17.00

#### Data/Programming Cable (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: RS232 DATA INTFC CBL DASH | 6 FT RS232 DATA CABLE Corresponding kit: HKN6160A. | G303 | 656 | $55.00
ADD: RS232 DATA INTFC CBL TRK | 20 FT RS232 Data Cable. Corresponding kit: HKN6161A. | G304 | 656 | $55.00
ADD:USB DATA INTFC CABLE-TRK | 16.5 ft USB with ignition sense. Corresponding kit: HKN6172B. Can be used to program APX Mobile Radios. | G309 | 656 | $55.00
ADD: USB DATA INTFC CABLE-DASH | 6 ft USB with ignition sense. Corresponding kit: HKN6163B. Can be used to program APX Mobile Radios. | G308 | 656 | $55.00

#### 3c: Optional Data Link Manager CD. Available for download from MOL.

#### Cable Accessories (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: UNIVERSAL RELAY CONTROLLER | Required to Control Vehicle Lights with the O3, O7 and O9 Control Heads. Requires URC Cable GA00260. | GA00259 | 656 | $275.00
ADD:REMOTE MOUNT VIP CBL APX | Park/Kill, Gunlock, 'Horn Ring/Horn Transfer' or Horn/Lights Park/Kill and Horn 'Ring/Horn Transfer' only available with Motorola Siren. Gunlock supported on O9 Control Head Only. Corresponding Kit: (HKN6196B) | G322 | 656 | $39.00
ADD: EXTERNAL ALARM RELAY AND CABLE | For either horn or lights, not both. | W116 | 656 | $83.00
ADD: GCAI EXTENSION CABLE 2 FT | For use with O7, O9 Control Heads and GCAI style Mic. Corresponding kit: PMKN4093 | GA00589 | 656 | $33.00
ADD: CABLE URC TO TRANSCEIVER | Connects Universal Relay Controller to APX Transciver via a RJ45 and CGAI connection. | GA00260 | 656 | $17.00
ADD: KEY LOCK MOUNT APX | Remote Mount Mid Power Only. | W81 | 471 | $36.00
ADD:BUZZER 110MA APX | Corresponding Kit: HLN6953 | B116 | 656 | $55.00

#### 8: Microphones (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD:HANDSET/HANGUP MIC | Coiled Cable with Toggle Switch Accessory Kit: HLN1457A | G874 | 656 | $285.00
ADD: MODEL III GCAI KEYPAD HANDSET | Corresponding kit: HMN4097 | GA00221 | 656 | $325.00
ADD: HANDSET/HANGUP MIC ARMORED CABLE | Armored Cable, No Toggle Switch Accessory Kit: HKN1018 | W874 | 656 | $300.00
ADD: VISOR MIC REMOTE MOUNT | Requires G90 No Microphone Needed & G235 Foot switch PTT. Kit Number: RMN5054 | W872 | 656 | $33.00
ADD:GATEWAY RSM AND WIRELESS RSM WITH VEHICLE CHARGER | Includes 12V Vehicle Charger Corresponding kit: RLN6551 | GA01354AA | 656 | $550.00
ADD: GOOSENECK PTT | Requires W872 Visor Mic. Kit Number: HMN1087A | G233 | 656 | $62.00
ADD: PTT FOOTSWITCH | Requires W872 Visor Mic. Kit Number: GLN7278 | G235 | 656 | $56.00
ADD: NO MICROPHONE NEEDED | Select this option when ordering O3 Handheld Control Head (G72). If ordering with Motorcycle G138 the DB 25 connector on harness needs to be sealed to prevent corrosion. | G90 | 656 | $0.00
ADD: KEYPAD MIC GCAI | Corresponding kit: HMN4079 | W20 | 471 | $198.00
ADD: STD PALM MICROPHONE APX | Corresponding kit: HMN1090 | W22 | 471 | $79.00
ADD: CONTROL STATION DESK GCAI MIC | Dash Mount Required Corresponding Kit: RMN5070 | W382 | 656 | $186.00
ADD:GATEWAY RSM AND WIRELESS RSM | Corresponding kit: RLN6552 | GA01439 | 656 | $431.00
ADD:GATEWAY RSM | Corresponding kit: PMMN4097 | GA01438 | 656 | $138.00
ADD: KEY LOCK MOUNT APX | Remote Mount Mid Power Only. | W81 | 471 | $36.00
ADD: HANDSET/HANGUP COILED CABLE | Not compatible with O3 CH or Control Station Operation. Corresponding Kit: HKN1018 | G876 | 656 | $415.00

#### Emergency

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: EXTERNAL EMERGENCY PUSHBUTTON | Corresponding kit: HLN5131 | W688 | 656 | $62.00
ADD: EMERGENCY ID EXT. FOOTSWITCH | Corresponding kit: HLN5113. | W470 | 656 | $62.00

#### Direct Mode Entry & Status/Message (Optional)

DEKs are incompatible with the O3 Control Head (except for DEK for Whelen Siren - GA00814). They require Remote Mount Configuration.

Please note, 24 modes are the maximum number of modes available. Although a combination of Direct Mode Entry boxes and Status/Message boxes can be used, the maximum available entries is 24.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 16 MODE DIRECT ENTRY | Corresponding Kit: H1836 | W614 | 656 | $396.00
ADD: 24 MODE DIRECT ENTRY | Corresponding Kit: H1837 | W615 | 656 | $594.00
ADD: DEK FOR WHELEN SIREN W/ O3 CH ONLY | Requires O3 CH. Corresponding kit: H1882 | GA00812 | 656 | $116.00
ADD: DEK FOR WHELEN SIREN | Corresponding kit: H1883 | GA00814 | 656 | $116.00
ADD: 8 MODE DIRECT ENTRY | Corresponding Kit: H1835 | W599 | 656 | $198.00
ADD: STATUS/MESSAGE 16 | Corresponding Kit: H1839A | W374 | 656 | $715.00
ADD: STATUS/MESSAGE 8 | Corresponding Kit: H1838A | W355 | 656 | $523.00

#### 9: Speakers (Must Select One)

Not compatible with Control Station Operation. Control Station Operation requires No Speaker Needed (G142).

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: NO SPEAKER NEEDED | Required for Control Station Operation (W665) | G142 | 656 | $0.00
ADD: SPKR 15W WATER RESISTANT | Corresponding kit: HSN4040 | G831 | 656 | $66.00
ADD: AUXILARY SPKR 13W (3.2OHM) | Corresponding kit: HSN4032 | W432 | 656 | $79.00
ADD: AUXILIARY SPKR 7.5 WATT | Corresponding kit: HSN4031 | B18 | 656 | $66.00
ADD: AUXILARY COVERT SPKR 10W APX | Corresponding Kit: HSN4042 | GA01203 | 656 | $66.00
ADD: SPKR 7.5W WATER RESISANT | Corresponding Kit: HSN4038 | G832 | 656 | $67.00

#### Auxiliary WILDCARD (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: AUXILIARY SWITCH PANEL | Corresponding kit: HLN1196. Remote Mount Required. Incompatible with O3 control head or motorcycle. | W591 | 656 | $182.00

#### Documentation (Optional)

#### RFID (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: RFID LABEL | Corresponding kit: HLN7014 | GA00268 | 656 | $28.00

#### 10: Service Option (Must Select One)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: 3Y ESSENTIAL SERVICE | - | G78 | 185 | $288.00
ADD: 5Y ESSENTIAL SERVICE | - | GA00318 | 185 | $480.00

####

### Ship Card

- CLICK HERE to see the Latest Lead Time Estimates

####

Download as CSV

Product Type | FC | Nomenclature | Description | APC | Lead Time
--- | --- | --- | --- | --- | ---
FIXEDSTN | FSA | CB000091A04 | CABLE, COAXIAL,QMA PLUG TO SMA JACK CONNETOR | 362 | 5
DATATERM | FSA | H1835 | 8 MODE DIRECT ENTRY DEK | 656 | 115
DATATERM | FSA | H1836 | 16 MODE DIRECT ENTRY DEK KIT | 656 | 14
DATATERM | FSA | H1837 | 24 MODE DIRECT ENTRY DEK KIT | 656 | 10
DATATERM | FSA | H1838 | 8 STATUS MESSAGE DEK KIT | 656 | 3
DATATERM | FSA | H1839 | 16 STATUS MESSAGE DEK KIT | 656 | 11
PARTS | CDP | HAF4013 | ANTENNA (762-870 MHZ) 3DB LOW-PROFILE | 554 | 3
PARTS | CDP | HAF4013 | ANTENNA (762-870 MHZ) 3DB LOW-PROFILE | 554 | 3
PARTS | CDP | HAF4013 | ANTENNA (762-870 MHZ) 3DB LOW-PROFILE | 554 | 3
PARTS | SCB | HAF4014 | ANTENNA (762-870 MHZ) 3DB ELEVATED FEED | 554 | 6
PARTS | SCB | HAF4014 | ANTENNA (762-870 MHZ) 3DB ELEVATED FEED | 554 | 6
PARTS | SCB | HAF4016 | ANTENNA (762-870 MHZ) 1/4 WAVE | 554 | 7
PARTS | SCB | HAF4016 | ANTENNA (762-870 MHZ) 1/4 WAVE | 554 | 7
PARTS | SCB | HAF4016 | ANTENNA (762-870 MHZ) 1/4 WAVE | 554 | 7
PARTS | CDP | HAF4017 | ANTENNA (762-870 MHZ) 3DB GAIN COLLINEAR | 554 | 3
PARTS | CDP | HAF4017 | ANTENNA (762-870 MHZ) 3DB GAIN COLLINEAR | 554 | 3
PARTS | CDP | HAF4017 | ANTENNA (762-870 MHZ) 3DB GAIN COLLINEAR | 554 | 3
PARTS | CDP | HAF4017 | ANTENNA (762-870 MHZ) 3DB GAIN COLLINEAR | 554 | 16
PARTS | CDP | HKN1018 | HSET/HANGUP NORMAL ARMOURED CABLE | 500 | 4
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
MOBILES | SCB | HKN4192 | POWER CABLE, 20 FOOT TO 12V BATTERY | 706 | 19
FIXEDSTN | PDC | HKN6161B | CABLE KIT 20' REMOTE MOUNT DATA | 362 | 128
PARTS | CDP | HKN6165 | CABLE, REMOTE MOUNT, 115 FT | 362 | 4
PARTS | CDP | HKN6165 | CABLE, REMOTE MOUNT, 115 FT | 362 | 4
PARTS | CDP | HKN6167B | CABLE, REMOTE MOUNT, 15M | 362 | 9
PARTS | CDP | HKN6167B | CABLE, REMOTE MOUNT, 15M | 362 | 3
PARTS | PGF | HKN6169B | CABLE, REMOTE MOUNT, 5M | 362 | 10
PARTS | PGF | HKN6169B | CABLE, REMOTE MOUNT, 5M | 362 | 10
PARTS | CDP | HKN6169B | CABLE, REMOTE MOUNT, 5M | 362 | 6
PARTS | PDC | HKN6169B | CABLE, REMOTE MOUNT, 5M | 362 | 4
MOBILES | FSA | HLN1196 | WILDCARD | 362 | 145
MOBILES | FSA | HLN1196 | WILDCARD | 362 | 145
PARTS | CDP | HLN1457 | HANDSET/HANGUP (HANGUP CUP) | 706 | 69
MOBILES | CDP | HMN1079C | MOD MOTORCYCLE WP MIC DB9 PIN CONN | 500 | 22
MOBILES | CDP | HMN1079C | MOD MOTORCYCLE WP MIC DB9 PIN CONN | 500 | 18
MOBILES | CDP | HMN1089C | ASSY:PRD OTH,HAND MIC,GCAI,WTR REST | 476 | 39
MOBILES | PDC | HMN1090D | ASSY,MIC,FRNT,GRY,STD PALM MIC (GCA | 476 | 3
MOBILES | PDC | HMN1090D | ASSY,MIC,FRNT,GRY,STD PALM MIC (GCA | 476 | 13
FIXEDSTN | CDP | HMN4079 | XTL5000 KEYPAD MICROPHONE | 706 | 24
PARTS | CDP | HMN4097A | MODEL III KEYPAD TELEPH HANDSET KIT | 706 | 3
PARTS | CDP | HMN4097A | MODEL III KEYPAD TELEPH HANDSET KIT | 706 | 3
PARTS | CDP | HMN4097A | MODEL III KEYPAD TELEPH HANDSET KIT | 706 | 6
FIXEDSTN | CDP | HSN4031B | EXT SPKR 7.5W | 706 | 10
FIXEDSTN | CDP | HSN4031B | EXT SPKR 7.5W | 706 | 3
PARTS | PDC | HSN4032B | MCS EXT SPKR 13W | 706 | 3
PARTS | PDC | HSN4032B | MCS EXT SPKR 13W | 706 | 3
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 9
PARTS | CDP | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 10
PARTS | PDC | HSN4038 | EXTERNAL 7.5 WATT WATER RESISTANT REMOTE MOUNT SPEAKER | 706 | 38
PORTABLES | VAN | HSN4040A | EXTERNAL WATER RESISTANT SPEAKER 15 WATTS | 706 | 3
COMPONENTS | CDP | HSN6003C | MCYCLE WP SPEAKER | 706 | 62
COMPONENTS | CDP | HSN6003C | MCYCLE WP SPEAKER | 706 | 62
COMPONENTS | CDP | HSN6003C | MCYCLE WP SPEAKER | 706 | 62
FIXEDSTN | CDP | KT000254A01 | POWER SUPPLY,EXT 280W, 100-240VAC WITH 6PN MOLEX TO SAE ADPTR CBL | 785 | 9
MOBILES | PGF | M25URS9PW1BN | APX6500 ENHANCED 7/800 MHZ | 527 | 28
PARTS | CDP | PMKN4033A | CABLE, MOBILE MIC EXTENSION, 10FT | 706 | 5
PARTS | CDP | PMKN4033A | CABLE, MOBILE MIC EXTENSION, 10FT | 706 | 5
PARTS | CDP | PMKN4033A | CABLE, MOBILE MIC EXTENSION, 10FT | 706 | 11
PARTS | PDC | PMLN4958B | O3 CAN 17' EXTENSION CABLE | 362 | 8
PARTS | PDC | PMLN4958B | O3 CAN 17' EXTENSION CABLE | 362 | 8
PARTS | CDP | PMLN4958B | O3 CAN 17' EXTENSION CABLE | 362 | 41
FIXEDSTN | CDP | PMMN4097C | MOBILE MICROPHONE WITH BLUETOOTH GATEWAY | 742 | 6
APX_PORTABLE | US1 | QA01648AA | ADD: HW KEY SUPPLEMENTAL DATA | 0655 |
APX_PORTABLE | US1 | QA05751AA | ADD: NO ENCRYPTION, CLEAR RADIO (NO ADP) (US ONLY) | 0655 |
PORTABLES | PGF | RLN5926A | PUSH BUTTON PTT | 706 | 20
PORTABLES | PGF | RLN5926A | PUSH BUTTON PTT | 706 | 20
PORTABLES | PGF | RLN5926A | PUSH BUTTON PTT | 706 | 20
FIXEDSTN | CDP | RLN6551B | LONG RANGE WIRELESS MOBILE RADIO SOLUTION W/VC | 189 | 251
DATATERM | PDC | RMN5054B | SMART VISOR MIC | 706 | 46
DATATERM | PDC | RMN5054B | SMART VISOR MIC | 706 | 46
DATATERM | PDC | RMN5054B | SMART VISOR MIC | 706 | 46
PARTS | PGF | RMN5070A | AS. SPECTRA & XTL5000 DESKTOP MIC | 706 | 13
PARTS | PGF | RMN5070A | AS. SPECTRA & XTL5000 DESKTOP MIC | 706 | 13