Back

##### APX NEXT Opt Config

###### Product Catalog

##### Jump to ...

- Configuration

Back

##### APX NEXT Opt Config

### Configuration

####

#### 2. Operation Mode (Must Select One)

2A: Digital Trunking (SN/SZ P25 Phase I Interop)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SMARTZONE OPERATION | A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | H38DA | 0437 | $1,412.00
ADD: P25 9600 BAUD TRUNKING | MUST also order H38 & Q806. INCLUDED at 'NO Charge' Q173-OminLink. APX digital radios require Advanced System Keys (ASK- DVN4046A) to be configured to operate on a trunking system. | Q361CD | 0437 | $353.00
ADD: ASTRO DIGITAL CAI OPERATION | - | Q806CH | 0437 | $607.00

#### 2B: Digital Trunking (SN/SZ)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SMARTZONE OPERATION | A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | H38DA | 0437 | $1,412.00
ADD: ASTRO DIGITAL CAI OPERATION | - | Q806CH | 0437 | $607.00

#### 2C: Digital Conventional (P25)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ASTRO DIGITAL CAI OPERATION | - | Q806CH | 0437 | $607.00
ADD: CONVENTIONAL OPERATION | - | H35DD | 0437 | $589.00

#### 2D: Analog Trunking

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: SMARTZONE OPERATION | A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased. | H38DA | 0437 | $1,412.00
ADD: ANALOG OPERATION | - | Q241CB | 0437 | $0.00

#### 2E: Analog Conventional

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: ANALOG OPERATION | - | Q241CB | 0437 | $0.00
ADD: CONVENTIONAL OPERATION | - | H35DD | 0437 | $589.00

#### 3. WiFi Connectivity (Required)

WiFi Capability and Out of Box Provisioning must be selected with APX NEXT family of radios.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: WIFI CAPABILITY | The APX NEXT, APX NEXT XE, and APX NEXT XN radios are enabled with LTE service. However, if LTE coverage is not available, the radios can use a preset default Wi-Fi SSID, to wirelessly download radio configurations and updates. • Includes Out of Box Provisioning over WiFi (QA09007) | QA09001AM | 0437 | $353.00

#### Encryption Algorithm Types (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: DES,DES-XL,DES-OFB ENCRYPTION AND ADP | (Analog 25 khz) / DES-OFB (Digital 12.5 khz Only) | Q625BK | 0437 | $705.00
SOFTWARE LICENSE ENH: DVP-XL ENCRYPTION AND ADP | Compatible with Digital and Analog (25kHZ Only) operations. ADP Privacy ships standard with Single Key. Multikey is required for multiple algorithms, such as ADP/AES or ADP/DES | H797DW | 0437 | $574.00
ADD: AES/DES-XL/DES-OFB ENCRYPTION AND ADP | NOT compatible with Q629 or Q625. Must order multikey if you want to use both algorithms. | Q15AU | 0437 | $941.00
ADD: NO ADP FOR P25 CAP | Customers who require compliance with DHS Project 25 CAP Encryption Requirements and who requires a clear radio with no encryption enabled will need to select option QA05751. The radios will need to be sent to the Motorola Depot if Encryption is needed in the future. | QA05751AF | 0437 | $0.00
SOFTWARE LICENSE ENH: AES ENCRYPTION AND ADP | - | Q629BD | 0437 | $560.00
SOFTWARE LICENSE ENH: MULTIKEY | - | H869DB | 0437 | $388.00

#### Submersible Selection (Optional)

NOTE: Delta-T is an optional selection for standard APX NEXT models.

Delta-T is mandatory when APX NEXT XE rugged option QA02006 is selected.

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ENH: SUBMERSIBLE (DELTA T) | MIL-STD Delta-T, IP68 (2m, 4hr) | H499KC | 0437 | $177.00

#### System Enhancement Options (Optional)

Description | Full Description | Nomenclature | APC | Price
--- | --- | --- | --- | ---
ADD: TDMA OPERATION | Requires Q806, H38, Q361. A SOFTWARE or HARDWARE KEY or WACN KEY is REQUIRED to be purchased with any APX Radio operating in trunking. HARDWARE KEY or WACN KEY will still REQUIRE a DVN4046 to be purchased | QA00580BA | 0437 | $530.00
ADD: VIQI VC RADIO OPERATION | Use ViQi Voice Control to operate the radio with voice commands. Change Channels and Zones, adjust Volume level, activate Audio Profiles, start/stop Scan, get Battery Level information. | QA09028AA | 0437 | $0.00
ADD: ENHANCED DATA | Digital (Q806/G806), Smartzone (H38/G51), IV&D (Q947) and P25 Trunking (Q361/G361) are required when ordering QA03399 (Enhanced Data) | QA03399AK | 0437 | $177.00
ADD: MULTICAST VOTING SCAN | Requires Q806 (ASTRO DIGITAL CAI OPERATION) | Q387CB | 0437 | $235.00
ADD: FALL ALERT / MANDOWN OPERATION | If a user becomes incapacitated, and is lying down motionless, an automatic Man Down Emergency Alarm or Emergency Call will be sent out on the programmed talk group. | QA01843AR | 0437 | $177.00
ADD: DVRS PSU ACTIVATION | Extends Portable Subscriber Unit (PSU) coverage through a Digital Vehicular Repeater System (DVRS) connected to a High Power Mobile radio. | QA00631AL | 0437 | $118.00
ADD: APX PERSONNEL ACCOUNTABILITY | Using a Systems Definition, Inc. fireground accountability application, incident commanders can easily identify who has responded to the incident, conduct roll-calls, identify a responder’s Mayday alarm, issue an evacuation notification even monitor the battery levels of responder's radios or remotely change the radio to a different talkgroup. | Q445BC | 0437 | $177.00
ADD: DIGITAL TONE SIGNALING | Alert first responders to an incident by broadcasting a series of distinct, recognizable tones followed by a voice transmission from dispatch. Works on P25 conventional or trunked systems, providing digital Quik-Call II operation (identical in operation to the legacy analog version). | QA09000AG | 0437 | $177.00
ADD: MULTI SYSTEM OTAR | Requires Q498 ASTRO 25 OTAR W/ MULTIKEY | QA07680AA | 0655 | $177.00
ADD: FRONT PANEL PROGRAMMING & CLONING (FEDERAL) | The APX NEXT radio can do FPP on a Trunking equipped radio only on conventional channels. Does not require a pin # or a dongle. | Q52BF | 0437 | $177.00
ADD: FRONT PANEL PROGRAMMING & CLONING | The APX NEXT radio can do FPP on a Trunking equipped radio only on conventional channels. Requires a pin #, but not a dongle. | Q53BF | 0437 | $177.00
ADD: PSU CONV SCAN | Requires DVRS PSU Activation | HA00677AA | 0579 | $0.00
ADD: PROGRAMMING OVER P25 (OTAP) | Requires Digital and IV&D. Compatible with P25 Trunking and Conventional Operation. POP25 requires AES encryption for ASTRO Conventional operation. To do in field POP25 programming must use Advanced System Key (DVN4046A). | G996 | 655 | $118.00
ENH: MULTI-CODE PLUG PROGRAMMING | Allows the radio to be programmed with a maximum of of 1 primary and 9 secondary codeplugs. The user can select a new codeplug via radio menu / settings on the radio. | QA09772AA | 0437 | $177.00
ADD: P25 LINK LAYER AUTHENTICATION | - | QA01767BL | 0437 | $118.00
SOFTWARE LICENSE ENH: ASTRO 25 OTAR W/ MULTIKEY | - | Q498BN | 0437 | $871.00

### Click on the link below to return to the radio main price page:

- CLICK HERE to return to the APX NEXT All Band page
- CLICK HERE to return to the APX NEXT Single Band page
- CLICK HERE to return to the APX NEXT XE All Band page
- CLICK HERE to return to the APX NEXT XE Single Band page
- CLICK HERE to return to the APX NEXT XN All Band page
- CLICK HERE to return to the APX NEXT XN Single Band page